diff -Nur linux-4.1.13.orig/arch/sh/Kconfig linux-4.1.13/arch/sh/Kconfig
--- linux-4.1.13.orig/arch/sh/Kconfig	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/Kconfig	2015-12-05 00:16:48.000000000 +0100
@@ -66,7 +66,7 @@
 	select HAVE_MIXED_BREAKPOINTS_REGS
 	select PERF_EVENTS
 	select ARCH_HIBERNATION_POSSIBLE if MMU
-	select SPARSE_IRQ
+	select SPARSE_IRQ if !CPU_SUBTYPE_0PF
 	select HAVE_CC_STACKPROTECTOR
 
 config SUPERH64
@@ -108,6 +108,9 @@
 config ARCH_HIBERNATION_POSSIBLE
 	def_bool n
 
+config ARCH_USES_GETTIMEOFFSET
+	def_bool n
+
 config SYS_SUPPORTS_APM_EMULATION
 	bool
 	select ARCH_SUSPEND_POSSIBLE
@@ -184,6 +187,11 @@
 	select CPU_SH2
 	select UNCACHED_MAPPING
 
+config CPU_SH2J
+	bool
+	select CPU_SH2
+	select ARCH_USES_GETTIMEOFFSET
+
 config CPU_SH3
 	bool
 	select CPU_HAS_INTEVT
@@ -303,6 +311,12 @@
 	help
 	  Select MX-G if running on an R8A03022BG part.
 
+# SH-2J Processor Support
+
+config CPU_SUBTYPE_0PF
+	bool "Support 0PF J2 SoftCore"
+	select CPU_SH2J
+
 # SH-3 Processor Support
 
 config CPU_SUBTYPE_SH7705
@@ -753,6 +767,7 @@
 				SH_7751_SOLUTION_ENGINE
 	default "0x00004000" if PAGE_SIZE_16KB || SH_SH03
 	default "0x00002000" if PAGE_SIZE_8KB
+	default "0x0003F000" if CPU_SUBTYPE_0PF
 	default "0x00001000"
 	help
 	  This sets the default offset of zero page.
diff -Nur linux-4.1.13.orig/arch/sh/Makefile linux-4.1.13/arch/sh/Makefile
--- linux-4.1.13.orig/arch/sh/Makefile	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/Makefile	2015-12-05 00:16:48.000000000 +0100
@@ -4,6 +4,7 @@
 # Copyright (C) 1999  Kaz Kojima
 # Copyright (C) 2002 - 2008  Paul Mundt
 # Copyright (C) 2002  M. R. Brown
+# Copyright (C) 2012  SEI, Inc. (sh2j)
 #
 # This file is subject to the terms and conditions of the GNU General Public
 # License.  See the file "COPYING" in the main directory of this archive
@@ -19,6 +20,7 @@
 isa-$(CONFIG_SH_DSP)			:= sh
 isa-$(CONFIG_CPU_SH2)			:= sh2
 isa-$(CONFIG_CPU_SH2A)			:= sh2a
+isa-$(CONFIG_CPU_SH2J)			:= sh2j
 isa-$(CONFIG_CPU_SH3)			:= sh3
 isa-$(CONFIG_CPU_SH4)			:= sh4
 isa-$(CONFIG_CPU_SH4A)			:= sh4a
@@ -31,6 +33,8 @@
 endif
 
 cflags-$(CONFIG_CPU_SH2)		:= $(call cc-option,-m2,)
+cflags-$(CONFIG_CPU_SH2J)		:= $(call cc-option,-m2,) \
+					   $(call cc-option,-melf,)
 cflags-$(CONFIG_CPU_SH2A)		+= $(call cc-option,-m2a,) \
 					   $(call cc-option,-m2a-nofpu,) \
 					   $(call cc-option,-m4-nofpu,)
@@ -91,6 +95,7 @@
 defaultimage-$(CONFIG_SH_7724_SOLUTION_ENGINE)	:= uImage
 defaultimage-$(CONFIG_SH_7206_SOLUTION_ENGINE)	:= vmlinux
 defaultimage-$(CONFIG_SH_7619_SOLUTION_ENGINE)	:= vmlinux
+defaultimage-$(CONFIG_SH_0PF)			:= vmlinux
 
 # Set some sensible Kbuild defaults
 KBUILD_IMAGE		:= $(defaultimage-y)
@@ -173,6 +178,7 @@
 # As an example, in order of preference, SH-2A > SH-2 > common definitions.
 #
 cpuincdir-$(CONFIG_CPU_SH2A)	+= cpu-sh2a
+cpuincdir-$(CONFIG_CPU_SH2J)	+= cpu-sh2j
 cpuincdir-$(CONFIG_CPU_SH2)	+= cpu-sh2
 cpuincdir-$(CONFIG_CPU_SH3)	+= cpu-sh3
 cpuincdir-$(CONFIG_CPU_SH4A)	+= cpu-sh4a
diff -Nur linux-4.1.13.orig/arch/sh/boards/Kconfig linux-4.1.13/arch/sh/boards/Kconfig
--- linux-4.1.13.orig/arch/sh/boards/Kconfig	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/boards/Kconfig	2015-12-05 00:16:48.000000000 +0100
@@ -90,6 +90,13 @@
 	  Select 7343 SolutionEngine if configuring for a Hitachi
 	  SH7343 (SH-Mobile 3AS) evaluation board.
 
+config 0PF_FPGA
+	bool "0PF FPGA"
+	depends on CPU_SUBTYPE_0PF
+	help
+	  Select 0PF_FPGA if you are configuring for an FPGA with
+	  the SH2j-workalike SoftCore from http://0pf.org
+
 config SH_HP6XX
 	bool "HP6XX"
 	select SYS_SUPPORTS_APM_EMULATION
diff -Nur linux-4.1.13.orig/arch/sh/boards/Makefile linux-4.1.13/arch/sh/boards/Makefile
--- linux-4.1.13.orig/arch/sh/boards/Makefile	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/boards/Makefile	2015-12-05 00:16:48.000000000 +0100
@@ -15,3 +15,4 @@
 obj-$(CONFIG_SH_SH7757LCR)	+= board-sh7757lcr.o
 obj-$(CONFIG_SH_APSH4A3A)	+= board-apsh4a3a.o
 obj-$(CONFIG_SH_APSH4AD0A)	+= board-apsh4ad0a.o
+obj-$(CONFIG_0PF_FPGA)		+= board-0pf.o
diff -Nur linux-4.1.13.orig/arch/sh/boards/board-0pf.c linux-4.1.13/arch/sh/boards/board-0pf.c
--- linux-4.1.13.orig/arch/sh/boards/board-0pf.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-4.1.13/arch/sh/boards/board-0pf.c	2015-12-05 00:16:48.000000000 +0100
@@ -0,0 +1,270 @@
+/*
+ * board-0pf.c
+ *
+ * Copyright (C) 2006 Yoshinori Sato
+ * Copyright (C) 2009 D. Jeff Dionne
+ *
+ * 0PF j-series CPU on FPGA
+ */
+#include <linux/platform_device.h>
+#include <linux/sched.h>
+#include <linux/kernel.h>
+#include <linux/param.h>
+#include <linux/interrupt.h>
+#include <linux/profile.h>
+#include <linux/init.h>
+#include <linux/irq.h>
+#include <linux/device.h>
+#include <linux/module.h>
+#include <asm/io.h>
+#include <asm/irq.h>
+#include <asm/rtc.h>
+#include <asm/machvec.h>
+#include <asm/board-0pf.h>
+
+int shj_irq_demux(int irq)
+{
+	return irq;		/* punt.. */
+}
+
+static void shj_ack_noop(struct irq_data *data)
+{
+	asm("nop;nop");
+	/* Dummy function.  */
+}
+
+static inline void shj_enable_irq(struct irq_data *data)
+{
+	unsigned int irq = data->irq;
+	volatile unsigned int vui;
+
+//	printk("%s: IRQ %d (0x%x)\n", __func__, irq, irq);
+
+	switch (irq) {
+	case PIT_IRQ:
+		//AQ_PIO = 0x0BB;
+		/* enable, lvl 2, vector 64 */
+		AQ_SYS = (1 << 26) |	/* enable PIT */
+		    (0x02 << 20) |	/* interrupt level 2 */
+		    (PIT_IRQ << 12) |	/* vector 64 */
+		    1;		/* turn off interval timer */
+		break;
+
+	case Irq_UART0:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_UART0, 0xf);	/* clear old setting */
+		vui |= ID2Pri(EIrqID_UART0, 0x7);	/* set interrupt level */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_UART1:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_UART1, 0xf);	/* clear old setting */
+		vui |= ID2Pri(EIrqID_UART1, 0x7);	/* set interrupt level */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_GPS:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_GPS, 0xf);	/* clear old setting */
+		vui |= ID2Pri(EIrqID_GPS, 0x7);	/* set interrupt level */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_I2C:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_I2C, 0xf);	/* clear old setting */
+		vui |= ID2Pri(EIrqID_I2C, 0x7);	/* set interrupt level */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_EMAC:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_EMAC, 0xf);	/* clear old setting */
+		vui |= ID2Pri(EIrqID_EMAC, 0x8);	/* set interrupt level */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		printk("EMAC prio is: %x\n", vui);
+		break;
+
+        case Irq_GPIO:
+                vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+                vui &= ~ID2Pri(EIrqID_GPIO, 0xf);       /* clear old setting */
+                vui |= ID2Pri(EIrqID_GPIO, 0x7);        /* set interrupt level */
+                *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+                break;
+
+        case Irq_1PPS: // prio is higher for 1PPS porposes
+                vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+                vui &= ~ID2Pri(EIrqID_1PPS, 0xf);       /* clear old setting */
+                vui |= ID2Pri(EIrqID_1PPS, 0x9);        /* set interrupt level */
+                *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+                printk("1PPS prio is: %x\n", vui);
+                break;
+
+	default:
+		break;
+
+	}
+}
+
+static inline void shj_disable_irq(struct irq_data *data)
+{
+	volatile unsigned int vui;
+	unsigned int irq = data->irq;
+
+	printk("%s: IRQ %d\n", __func__, irq);
+
+	switch (irq) {
+	case PIT_IRQ:
+		/* enable, lvl 2, vector 64 */
+		AQ_SYS = (0 << 26) |	/* disable PIT */
+		    (0x02 << 20) |	/* interrupt level 2 */
+		    (PIT_IRQ << 12) |	/* vector 64 */
+		    1;		/* turn off interval timer */
+		break;
+
+	case Irq_UART0:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_UART0, 0xf);	/* clear setting */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_UART1:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_UART1, 0xf);	/* clear setting */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_GPS:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_GPS, 0xf);	/* clear setting */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_I2C:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_I2C, 0xf);	/* clear setting */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+	case Irq_EMAC:
+		vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+		vui &= ~ID2Pri(EIrqID_EMAC, 0xf);	/* clear setting */
+		*(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+		break;
+
+        case Irq_GPIO:
+                vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+                vui &= ~ID2Pri(EIrqID_GPIO, 0xf);       /* clear setting */
+                *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+                break;
+
+        case Irq_1PPS:
+                vui = *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri);
+                vui &= ~ID2Pri(EIrqID_1PPS, 0xf);       /* clear setting */
+                *(volatile unsigned int *)(sys_SYS_BASE + Sys_IntPri) = vui;
+                break;
+
+	default:
+		break;
+	}
+}
+
+static struct irq_chip shj_irq_chip = {
+	.name = "0PF_INTC",
+	.irq_enable = shj_enable_irq,
+	.irq_disable = shj_disable_irq,
+	.irq_ack = shj_ack_noop,
+};
+
+static void __init shj_irq_init(void)
+{
+	int c;
+
+	printk(KERN_INFO "0PF FPGA interrupt controller...\n");
+
+	for (c = 0; c < NR_IRQS; c++) {
+		//irq_desc[c].action = NULL;
+		//irq_desc[c].depth = 1;
+		irq_set_chip_and_handler_name(c, &shj_irq_chip,
+					      handle_simple_irq, "simple");
+	}
+}
+
+#ifdef CONFIG_ARCH_USES_GETTIMEOFFSET
+// Commit 7b1f62076 switched this to a pointer
+/*
+ * Should return nanoseconds since last timer tick
+ */
+u32 shj_gettimeoffset(void)
+{
+	u32 clocks_counter = readl(SHJ_PIT_PCNTR);
+
+	return clocks_counter * readl(SHJ_NSEC_PER_CLOCK);
+}
+
+static void __init shj_board_setup(char **cmdline)
+{
+	arch_gettimeoffset = shj_gettimeoffset;
+}
+#else
+#define shj_gettimeoffset 0
+#endif
+
+static struct sh_machine_vector mv_se __initmv = {
+	.mv_name = "0PF_FPGA",
+	//.mv_nr_irqs = 256,
+	.mv_irq_demux = shj_irq_demux,
+	.mv_init_irq = shj_irq_init,
+	.mv_setup = shj_board_setup,
+};
+
+static irqreturn_t timer_interrupt(int irq, void *dev_id)
+{
+	// AQ_PIO = 0x011; // GREEN
+
+	if (current->pid)
+		profile_tick(CPU_PROFILING);
+
+	xtime_update(1);
+	update_process_times(user_mode(get_irq_regs()));
+
+	return IRQ_HANDLED;
+}
+
+static void __init start_pit(void)
+{
+	if (request_irq
+	    (PIT_IRQ, timer_interrupt, IRQF_TIMER, "pit", NULL))
+		printk("irq_desc[%p] : fail to register\n", &irq_desc[PIT_IRQ]);
+
+	irq_set_chip_and_handler_name(PIT_IRQ, &shj_irq_chip, handle_edge_irq,
+				      "pit");
+}
+
+static int __init shj_initialise(void)
+{
+	struct irq_data *data;
+
+	pr_info("0PF Machine setup...\n");
+
+	start_pit();
+
+	data = irq_get_irq_data(Irq_UART0);
+	shj_enable_irq(data);
+
+	data = irq_get_irq_data(Irq_UART1);
+	shj_enable_irq(data);
+
+	data = irq_get_irq_data(Irq_EMAC);
+	shj_enable_irq(data);
+
+	data = irq_get_irq_data(PIT_IRQ);
+	shj_enable_irq(data);
+
+	pr_info("0PF Machine setup done.\n");
+
+	return 0;
+}
+
+arch_initcall(shj_initialise);
diff -Nur linux-4.1.13.orig/arch/sh/configs/0pf_defconfig linux-4.1.13/arch/sh/configs/0pf_defconfig
--- linux-4.1.13.orig/arch/sh/configs/0pf_defconfig	1970-01-01 01:00:00.000000000 +0100
+++ linux-4.1.13/arch/sh/configs/0pf_defconfig	2015-12-05 00:16:48.000000000 +0100
@@ -0,0 +1,945 @@
+#
+# Automatically generated file; DO NOT EDIT.
+# Linux/sh 4.1.0-rc6 Kernel Configuration
+#
+CONFIG_SUPERH=y
+CONFIG_SUPERH32=y
+# CONFIG_SUPERH64 is not set
+CONFIG_ARCH_DEFCONFIG="arch/sh/configs/shx3_defconfig"
+CONFIG_RWSEM_GENERIC_SPINLOCK=y
+CONFIG_GENERIC_BUG=y
+CONFIG_GENERIC_HWEIGHT=y
+# CONFIG_ARCH_SUSPEND_POSSIBLE is not set
+# CONFIG_ARCH_HIBERNATION_POSSIBLE is not set
+CONFIG_ARCH_USES_GETTIMEOFFSET=y
+CONFIG_STACKTRACE_SUPPORT=y
+CONFIG_LOCKDEP_SUPPORT=y
+CONFIG_HAVE_LATENCYTOP_SUPPORT=y
+# CONFIG_ARCH_HAS_ILOG2_U32 is not set
+# CONFIG_ARCH_HAS_ILOG2_U64 is not set
+CONFIG_NO_IOPORT_MAP=y
+CONFIG_DMA_NONCOHERENT=y
+CONFIG_NEED_DMA_MAP_STATE=y
+CONFIG_NEED_SG_DMA_LENGTH=y
+CONFIG_PGTABLE_LEVELS=2
+CONFIG_DEFCONFIG_LIST="/lib/modules/$UNAME_RELEASE/.config"
+CONFIG_IRQ_WORK=y
+
+#
+# General setup
+#
+CONFIG_BROKEN_ON_SMP=y
+CONFIG_INIT_ENV_ARG_LIMIT=32
+CONFIG_CROSS_COMPILE=""
+# CONFIG_COMPILE_TEST is not set
+CONFIG_LOCALVERSION=""
+# CONFIG_LOCALVERSION_AUTO is not set
+CONFIG_HAVE_KERNEL_GZIP=y
+CONFIG_HAVE_KERNEL_BZIP2=y
+CONFIG_HAVE_KERNEL_LZMA=y
+CONFIG_HAVE_KERNEL_XZ=y
+CONFIG_HAVE_KERNEL_LZO=y
+CONFIG_KERNEL_GZIP=y
+# CONFIG_KERNEL_BZIP2 is not set
+# CONFIG_KERNEL_LZMA is not set
+# CONFIG_KERNEL_XZ is not set
+# CONFIG_KERNEL_LZO is not set
+CONFIG_DEFAULT_HOSTNAME="(none)"
+# CONFIG_SYSVIPC is not set
+# CONFIG_FHANDLE is not set
+# CONFIG_USELIB is not set
+CONFIG_HAVE_ARCH_AUDITSYSCALL=y
+
+#
+# IRQ subsystem
+#
+CONFIG_MAY_HAVE_SPARSE_IRQ=y
+CONFIG_GENERIC_IRQ_SHOW=y
+CONFIG_IRQ_DOMAIN=y
+CONFIG_IRQ_FORCED_THREADING=y
+# CONFIG_SPARSE_IRQ is not set
+CONFIG_GENERIC_CLOCKEVENTS=y
+
+#
+# Timers subsystem
+#
+CONFIG_HZ_PERIODIC=y
+
+#
+# CPU/Task time and stats accounting
+#
+CONFIG_TICK_CPU_ACCOUNTING=y
+# CONFIG_BSD_PROCESS_ACCT is not set
+
+#
+# RCU Subsystem
+#
+CONFIG_TINY_RCU=y
+CONFIG_SRCU=y
+# CONFIG_TASKS_RCU is not set
+# CONFIG_RCU_STALL_COMMON is not set
+# CONFIG_TREE_RCU_TRACE is not set
+CONFIG_RCU_KTHREAD_PRIO=0
+# CONFIG_RCU_EXPEDITE_BOOT is not set
+# CONFIG_BUILD_BIN2C is not set
+# CONFIG_IKCONFIG is not set
+CONFIG_LOG_BUF_SHIFT=17
+# CONFIG_CGROUPS is not set
+# CONFIG_CHECKPOINT_RESTORE is not set
+CONFIG_NAMESPACES=y
+# CONFIG_UTS_NS is not set
+# CONFIG_USER_NS is not set
+# CONFIG_PID_NS is not set
+# CONFIG_SCHED_AUTOGROUP is not set
+# CONFIG_SYSFS_DEPRECATED is not set
+# CONFIG_RELAY is not set
+CONFIG_BLK_DEV_INITRD=y
+CONFIG_INITRAMFS_SOURCE="initrd/root-dev initrd/root-files"
+CONFIG_INITRAMFS_ROOT_UID=0
+CONFIG_INITRAMFS_ROOT_GID=0
+# CONFIG_RD_GZIP is not set
+# CONFIG_RD_BZIP2 is not set
+# CONFIG_RD_LZMA is not set
+# CONFIG_RD_XZ is not set
+# CONFIG_RD_LZO is not set
+# CONFIG_RD_LZ4 is not set
+# CONFIG_CC_OPTIMIZE_FOR_SIZE is not set
+CONFIG_SYSCTL=y
+CONFIG_ANON_INODES=y
+CONFIG_HAVE_UID16=y
+# CONFIG_EXPERT is not set
+CONFIG_UID16=y
+CONFIG_MULTIUSER=y
+CONFIG_SGETMASK_SYSCALL=y
+CONFIG_SYSFS_SYSCALL=y
+# CONFIG_SYSCTL_SYSCALL is not set
+CONFIG_KALLSYMS=y
+CONFIG_PRINTK=y
+CONFIG_BUG=y
+CONFIG_ELF_CORE=y
+CONFIG_BASE_FULL=y
+CONFIG_FUTEX=y
+CONFIG_EPOLL=y
+CONFIG_SIGNALFD=y
+CONFIG_TIMERFD=y
+CONFIG_EVENTFD=y
+# CONFIG_BPF_SYSCALL is not set
+CONFIG_AIO=y
+CONFIG_ADVISE_SYSCALLS=y
+# CONFIG_EMBEDDED is not set
+CONFIG_HAVE_PERF_EVENTS=y
+CONFIG_PERF_USE_VMALLOC=y
+
+#
+# Kernel Performance Events And Counters
+#
+CONFIG_PERF_EVENTS=y
+CONFIG_VM_EVENT_COUNTERS=y
+CONFIG_SLUB_DEBUG=y
+# CONFIG_COMPAT_BRK is not set
+# CONFIG_SLAB is not set
+CONFIG_SLUB=y
+# CONFIG_PROFILING is not set
+CONFIG_HAVE_OPROFILE=y
+# CONFIG_UPROBES is not set
+# CONFIG_HAVE_64BIT_ALIGNED_ACCESS is not set
+CONFIG_HAVE_KPROBES=y
+CONFIG_HAVE_KRETPROBES=y
+CONFIG_HAVE_ARCH_TRACEHOOK=y
+CONFIG_HAVE_DMA_ATTRS=y
+CONFIG_GENERIC_SMP_IDLE_THREAD=y
+CONFIG_GENERIC_IDLE_POLL_SETUP=y
+CONFIG_HAVE_REGS_AND_STACK_ACCESS_API=y
+CONFIG_HAVE_CLK=y
+CONFIG_HAVE_DMA_API_DEBUG=y
+CONFIG_HAVE_HW_BREAKPOINT=y
+CONFIG_HAVE_MIXED_BREAKPOINTS_REGS=y
+CONFIG_ARCH_WANT_IPC_PARSE_VERSION=y
+CONFIG_HAVE_CC_STACKPROTECTOR=y
+# CONFIG_CC_STACKPROTECTOR is not set
+CONFIG_CC_STACKPROTECTOR_NONE=y
+# CONFIG_CC_STACKPROTECTOR_REGULAR is not set
+# CONFIG_CC_STACKPROTECTOR_STRONG is not set
+CONFIG_MODULES_USE_ELF_RELA=y
+CONFIG_OLD_SIGSUSPEND=y
+CONFIG_OLD_SIGACTION=y
+
+#
+# GCOV-based kernel profiling
+#
+CONFIG_ARCH_HAS_GCOV_PROFILE_ALL=y
+CONFIG_HAVE_GENERIC_DMA_COHERENT=y
+CONFIG_SLABINFO=y
+CONFIG_RT_MUTEXES=y
+CONFIG_BASE_SMALL=0
+# CONFIG_MODULES is not set
+CONFIG_BLOCK=y
+# CONFIG_LBDAF is not set
+# CONFIG_BLK_DEV_BSG is not set
+# CONFIG_BLK_DEV_BSGLIB is not set
+# CONFIG_BLK_DEV_INTEGRITY is not set
+# CONFIG_BLK_CMDLINE_PARSER is not set
+
+#
+# Partition Types
+#
+# CONFIG_PARTITION_ADVANCED is not set
+CONFIG_MSDOS_PARTITION=y
+CONFIG_EFI_PARTITION=y
+
+#
+# IO Schedulers
+#
+CONFIG_IOSCHED_NOOP=y
+# CONFIG_IOSCHED_DEADLINE is not set
+# CONFIG_IOSCHED_CFQ is not set
+CONFIG_DEFAULT_NOOP=y
+CONFIG_DEFAULT_IOSCHED="noop"
+CONFIG_INLINE_SPIN_UNLOCK_IRQ=y
+CONFIG_INLINE_READ_UNLOCK=y
+CONFIG_INLINE_READ_UNLOCK_IRQ=y
+CONFIG_INLINE_WRITE_UNLOCK=y
+CONFIG_INLINE_WRITE_UNLOCK_IRQ=y
+# CONFIG_FREEZER is not set
+
+#
+# System type
+#
+CONFIG_CPU_SH2=y
+CONFIG_CPU_SH2J=y
+# CONFIG_CPU_SUBTYPE_SH7619 is not set
+# CONFIG_CPU_SUBTYPE_SH7201 is not set
+# CONFIG_CPU_SUBTYPE_SH7203 is not set
+# CONFIG_CPU_SUBTYPE_SH7206 is not set
+# CONFIG_CPU_SUBTYPE_SH7263 is not set
+# CONFIG_CPU_SUBTYPE_SH7264 is not set
+# CONFIG_CPU_SUBTYPE_SH7269 is not set
+# CONFIG_CPU_SUBTYPE_MXG is not set
+CONFIG_CPU_SUBTYPE_0PF=y
+# CONFIG_CPU_SUBTYPE_SH7705 is not set
+# CONFIG_CPU_SUBTYPE_SH7706 is not set
+# CONFIG_CPU_SUBTYPE_SH7707 is not set
+# CONFIG_CPU_SUBTYPE_SH7708 is not set
+# CONFIG_CPU_SUBTYPE_SH7709 is not set
+# CONFIG_CPU_SUBTYPE_SH7710 is not set
+# CONFIG_CPU_SUBTYPE_SH7712 is not set
+# CONFIG_CPU_SUBTYPE_SH7720 is not set
+# CONFIG_CPU_SUBTYPE_SH7721 is not set
+# CONFIG_CPU_SUBTYPE_SH7750 is not set
+# CONFIG_CPU_SUBTYPE_SH7091 is not set
+# CONFIG_CPU_SUBTYPE_SH7750R is not set
+# CONFIG_CPU_SUBTYPE_SH7750S is not set
+# CONFIG_CPU_SUBTYPE_SH7751 is not set
+# CONFIG_CPU_SUBTYPE_SH7751R is not set
+# CONFIG_CPU_SUBTYPE_SH7760 is not set
+# CONFIG_CPU_SUBTYPE_SH4_202 is not set
+# CONFIG_CPU_SUBTYPE_SH7723 is not set
+# CONFIG_CPU_SUBTYPE_SH7724 is not set
+# CONFIG_CPU_SUBTYPE_SH7734 is not set
+# CONFIG_CPU_SUBTYPE_SH7757 is not set
+# CONFIG_CPU_SUBTYPE_SH7763 is not set
+# CONFIG_CPU_SUBTYPE_SH7770 is not set
+# CONFIG_CPU_SUBTYPE_SH7780 is not set
+# CONFIG_CPU_SUBTYPE_SH7785 is not set
+# CONFIG_CPU_SUBTYPE_SH7786 is not set
+# CONFIG_CPU_SUBTYPE_SHX3 is not set
+# CONFIG_CPU_SUBTYPE_SH7343 is not set
+# CONFIG_CPU_SUBTYPE_SH7722 is not set
+# CONFIG_CPU_SUBTYPE_SH7366 is not set
+
+#
+# Memory management options
+#
+CONFIG_QUICKLIST=y
+CONFIG_PAGE_OFFSET=0x00000000
+CONFIG_FORCE_MAX_ZONEORDER=14
+CONFIG_MEMORY_START=0x10000000
+CONFIG_MEMORY_SIZE=0x8000000
+# CONFIG_29BIT is not set
+CONFIG_32BIT=y
+CONFIG_ARCH_FLATMEM_ENABLE=y
+CONFIG_ARCH_SPARSEMEM_ENABLE=y
+CONFIG_ARCH_SPARSEMEM_DEFAULT=y
+CONFIG_ARCH_SELECT_MEMORY_MODEL=y
+CONFIG_PAGE_SIZE_4KB=y
+# CONFIG_PAGE_SIZE_8KB is not set
+# CONFIG_PAGE_SIZE_16KB is not set
+# CONFIG_PAGE_SIZE_64KB is not set
+CONFIG_SELECT_MEMORY_MODEL=y
+CONFIG_FLATMEM_MANUAL=y
+# CONFIG_SPARSEMEM_MANUAL is not set
+CONFIG_FLATMEM=y
+CONFIG_FLAT_NODE_MEM_MAP=y
+CONFIG_SPARSEMEM_STATIC=y
+CONFIG_HAVE_MEMBLOCK=y
+CONFIG_HAVE_MEMBLOCK_NODE_MAP=y
+CONFIG_ARCH_DISCARD_MEMBLOCK=y
+# CONFIG_HAVE_BOOTMEM_INFO_NODE is not set
+CONFIG_PAGEFLAGS_EXTENDED=y
+CONFIG_SPLIT_PTLOCK_CPUS=999999
+# CONFIG_PHYS_ADDR_T_64BIT is not set
+CONFIG_ZONE_DMA_FLAG=0
+CONFIG_NR_QUICK=1
+CONFIG_NOMMU_INITIAL_TRIM_EXCESS=1
+CONFIG_NEED_PER_CPU_KM=y
+# CONFIG_CLEANCACHE is not set
+# CONFIG_ZPOOL is not set
+# CONFIG_ZBUD is not set
+
+#
+# Cache configuration
+#
+# CONFIG_CACHE_WRITEBACK is not set
+# CONFIG_CACHE_WRITETHROUGH is not set
+CONFIG_CACHE_OFF=y
+
+#
+# Processor features
+#
+# CONFIG_CPU_LITTLE_ENDIAN is not set
+CONFIG_CPU_BIG_ENDIAN=y
+# CONFIG_SH_FPU_EMU is not set
+
+#
+# Board support
+#
+CONFIG_0PF_FPGA=y
+
+#
+# Timer and clock configuration
+#
+CONFIG_SH_PCLK_FREQ=32000000
+CONFIG_SH_CLK_CPG=y
+CONFIG_SH_CLK_CPG_LEGACY=y
+
+#
+# CPU Frequency scaling
+#
+
+#
+# CPU Frequency scaling
+#
+# CONFIG_CPU_FREQ is not set
+
+#
+# DMA support
+#
+
+#
+# Companion Chips
+#
+
+#
+# Additional SuperH Device Drivers
+#
+# CONFIG_HEARTBEAT is not set
+# CONFIG_PUSH_SWITCH is not set
+
+#
+# Kernel features
+#
+CONFIG_HZ_100=y
+# CONFIG_HZ_250 is not set
+# CONFIG_HZ_300 is not set
+# CONFIG_HZ_1000 is not set
+CONFIG_HZ=100
+# CONFIG_SCHED_HRTICK is not set
+# CONFIG_CRASH_DUMP is not set
+CONFIG_PHYSICAL_START=0x10000000
+# CONFIG_SECCOMP is not set
+CONFIG_PREEMPT_NONE=y
+# CONFIG_PREEMPT_VOLUNTARY is not set
+# CONFIG_PREEMPT is not set
+CONFIG_GUSA=y
+
+#
+# SuperH / SH-Mobile Driver Options
+#
+CONFIG_SH_INTC=y
+
+#
+# Interrupt controller options
+#
+
+#
+# Boot options
+#
+CONFIG_ZERO_PAGE_OFFSET=0x0003F000
+CONFIG_BOOT_LINK_OFFSET=0x00800000
+CONFIG_ENTRY_OFFSET=0x00001000
+# CONFIG_CMDLINE_OVERWRITE is not set
+CONFIG_CMDLINE_EXTEND=y
+CONFIG_CMDLINE="console=ttyUL0"
+
+#
+# Bus options
+#
+# CONFIG_PCCARD is not set
+
+#
+# Executable file formats
+#
+CONFIG_BINFMT_ELF_FDPIC=y
+CONFIG_BINFMT_SCRIPT=y
+CONFIG_BINFMT_FLAT=y
+# CONFIG_BINFMT_ZFLAT is not set
+# CONFIG_BINFMT_SHARED_FLAT is not set
+# CONFIG_HAVE_AOUT is not set
+# CONFIG_BINFMT_MISC is not set
+CONFIG_COREDUMP=y
+
+#
+# Power management options (EXPERIMENTAL)
+#
+# CONFIG_PM is not set
+
+#
+# CPU Idle
+#
+# CONFIG_CPU_IDLE is not set
+# CONFIG_ARCH_NEEDS_CPU_IDLE_COUPLED is not set
+# CONFIG_NET is not set
+
+#
+# Device Drivers
+#
+
+#
+# Generic Driver Options
+#
+# CONFIG_UEVENT_HELPER is not set
+CONFIG_DEVTMPFS=y
+CONFIG_DEVTMPFS_MOUNT=y
+# CONFIG_STANDALONE is not set
+# CONFIG_PREVENT_FIRMWARE_BUILD is not set
+CONFIG_FW_LOADER=y
+# CONFIG_FIRMWARE_IN_KERNEL is not set
+CONFIG_EXTRA_FIRMWARE=""
+# CONFIG_FW_LOADER_USER_HELPER_FALLBACK is not set
+CONFIG_ALLOW_DEV_COREDUMP=y
+# CONFIG_SYS_HYPERVISOR is not set
+# CONFIG_GENERIC_CPU_DEVICES is not set
+# CONFIG_DMA_SHARED_BUFFER is not set
+
+#
+# Bus devices
+#
+# CONFIG_MTD is not set
+CONFIG_ARCH_MIGHT_HAVE_PC_PARPORT=y
+# CONFIG_PARPORT is not set
+# CONFIG_BLK_DEV is not set
+
+#
+# Misc devices
+#
+# CONFIG_SENSORS_LIS3LV02D is not set
+# CONFIG_DUMMY_IRQ is not set
+# CONFIG_ENCLOSURE_SERVICES is not set
+# CONFIG_SRAM is not set
+# CONFIG_C2PORT is not set
+
+#
+# EEPROM support
+#
+# CONFIG_EEPROM_93CX6 is not set
+
+#
+# Texas Instruments shared transport line discipline
+#
+
+#
+# Altera FPGA firmware download module
+#
+
+#
+# Intel MIC Bus Driver
+#
+
+#
+# Intel MIC Host Driver
+#
+
+#
+# Intel MIC Card Driver
+#
+# CONFIG_ECHO is not set
+# CONFIG_CXL_BASE is not set
+
+#
+# SCSI device support
+#
+CONFIG_SCSI_MOD=y
+# CONFIG_RAID_ATTRS is not set
+# CONFIG_SCSI is not set
+# CONFIG_SCSI_DMA is not set
+CONFIG_HAVE_PATA_PLATFORM=y
+# CONFIG_ATA is not set
+# CONFIG_MD is not set
+
+#
+# Input device support
+#
+CONFIG_INPUT=y
+# CONFIG_INPUT_FF_MEMLESS is not set
+# CONFIG_INPUT_POLLDEV is not set
+# CONFIG_INPUT_SPARSEKMAP is not set
+# CONFIG_INPUT_MATRIXKMAP is not set
+
+#
+# Userland interfaces
+#
+# CONFIG_INPUT_MOUSEDEV is not set
+# CONFIG_INPUT_JOYDEV is not set
+# CONFIG_INPUT_EVDEV is not set
+# CONFIG_INPUT_EVBUG is not set
+
+#
+# Input Device Drivers
+#
+# CONFIG_INPUT_KEYBOARD is not set
+# CONFIG_INPUT_MOUSE is not set
+# CONFIG_INPUT_JOYSTICK is not set
+# CONFIG_INPUT_TABLET is not set
+# CONFIG_INPUT_TOUCHSCREEN is not set
+# CONFIG_INPUT_MISC is not set
+
+#
+# Hardware I/O ports
+#
+# CONFIG_SERIO is not set
+# CONFIG_GAMEPORT is not set
+
+#
+# Character devices
+#
+CONFIG_TTY=y
+CONFIG_VT=y
+CONFIG_CONSOLE_TRANSLATIONS=y
+CONFIG_VT_CONSOLE=y
+CONFIG_HW_CONSOLE=y
+# CONFIG_VT_HW_CONSOLE_BINDING is not set
+CONFIG_UNIX98_PTYS=y
+# CONFIG_DEVPTS_MULTIPLE_INSTANCES is not set
+# CONFIG_LEGACY_PTYS is not set
+# CONFIG_SERIAL_NONSTANDARD is not set
+# CONFIG_TRACE_SINK is not set
+CONFIG_DEVMEM=y
+# CONFIG_DEVKMEM is not set
+
+#
+# Serial drivers
+#
+# CONFIG_SERIAL_8250 is not set
+
+#
+# Non-8250 serial port support
+#
+CONFIG_SERIAL_UARTLITE=y
+CONFIG_SERIAL_UARTLITE_CONSOLE=y
+CONFIG_SERIAL_UARTLITE_0PF=y
+# CONFIG_SERIAL_SH_SCI is not set
+CONFIG_SERIAL_CORE=y
+CONFIG_SERIAL_CORE_CONSOLE=y
+# CONFIG_SERIAL_SCCNXP is not set
+# CONFIG_SERIAL_ALTERA_JTAGUART is not set
+# CONFIG_SERIAL_ALTERA_UART is not set
+# CONFIG_SERIAL_ARC is not set
+# CONFIG_SERIAL_FSL_LPUART is not set
+# CONFIG_IPMI_HANDLER is not set
+# CONFIG_HW_RANDOM is not set
+# CONFIG_R3964 is not set
+# CONFIG_RAW_DRIVER is not set
+# CONFIG_TCG_TPM is not set
+
+#
+# I2C support
+#
+# CONFIG_I2C is not set
+# CONFIG_SPI is not set
+# CONFIG_SPMI is not set
+# CONFIG_HSI is not set
+
+#
+# PPS support
+#
+# CONFIG_PPS is not set
+
+#
+# PPS generators support
+#
+
+#
+# PTP clock support
+#
+
+#
+# Enable PHYLIB and NETWORK_PHY_TIMESTAMPING to see the additional clocks.
+#
+CONFIG_ARCH_HAVE_CUSTOM_GPIO_H=y
+# CONFIG_W1 is not set
+# CONFIG_POWER_SUPPLY is not set
+# CONFIG_POWER_AVS is not set
+# CONFIG_HWMON is not set
+# CONFIG_THERMAL is not set
+# CONFIG_WATCHDOG is not set
+CONFIG_SSB_POSSIBLE=y
+
+#
+# Sonics Silicon Backplane
+#
+# CONFIG_SSB is not set
+CONFIG_BCMA_POSSIBLE=y
+
+#
+# Broadcom specific AMBA
+#
+# CONFIG_BCMA is not set
+
+#
+# Multifunction device drivers
+#
+# CONFIG_MFD_CORE is not set
+# CONFIG_MFD_CROS_EC is not set
+# CONFIG_HTC_PASIC3 is not set
+# CONFIG_MFD_KEMPLD is not set
+# CONFIG_MFD_MT6397 is not set
+# CONFIG_MFD_SM501 is not set
+# CONFIG_ABX500_CORE is not set
+# CONFIG_MFD_SYSCON is not set
+# CONFIG_MFD_TI_AM335X_TSCADC is not set
+# CONFIG_MFD_TMIO is not set
+# CONFIG_REGULATOR is not set
+# CONFIG_MEDIA_SUPPORT is not set
+
+#
+# Graphics support
+#
+
+#
+# Direct Rendering Manager
+#
+
+#
+# Frame buffer Devices
+#
+# CONFIG_FB is not set
+# CONFIG_FB_SH_MOBILE_MERAM is not set
+# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
+# CONFIG_VGASTATE is not set
+
+#
+# Console display driver support
+#
+CONFIG_DUMMY_CONSOLE=y
+CONFIG_DUMMY_CONSOLE_COLUMNS=80
+CONFIG_DUMMY_CONSOLE_ROWS=25
+# CONFIG_SOUND is not set
+
+#
+# HID support
+#
+# CONFIG_HID is not set
+CONFIG_USB_OHCI_LITTLE_ENDIAN=y
+# CONFIG_USB_SUPPORT is not set
+# CONFIG_UWB is not set
+# CONFIG_MMC is not set
+# CONFIG_MEMSTICK is not set
+# CONFIG_NEW_LEDS is not set
+# CONFIG_ACCESSIBILITY is not set
+CONFIG_RTC_LIB=y
+# CONFIG_RTC_CLASS is not set
+# CONFIG_DMADEVICES is not set
+# CONFIG_AUXDISPLAY is not set
+# CONFIG_VIRT_DRIVERS is not set
+
+#
+# Virtio drivers
+#
+# CONFIG_VIRTIO_MMIO is not set
+
+#
+# Microsoft Hyper-V guest support
+#
+# CONFIG_STAGING is not set
+CONFIG_CLKDEV_LOOKUP=y
+
+#
+# Hardware Spinlock drivers
+#
+
+#
+# Clock Source drivers
+#
+# CONFIG_ATMEL_PIT is not set
+# CONFIG_SH_TIMER_CMT is not set
+# CONFIG_SH_TIMER_MTU2 is not set
+# CONFIG_SH_TIMER_TMU is not set
+# CONFIG_EM_TIMER_STI is not set
+# CONFIG_MAILBOX is not set
+
+#
+# Remoteproc drivers
+#
+# CONFIG_STE_MODEM_RPROC is not set
+
+#
+# Rpmsg drivers
+#
+
+#
+# SOC (System On Chip) specific Drivers
+#
+# CONFIG_SOC_TI is not set
+# CONFIG_PM_DEVFREQ is not set
+# CONFIG_EXTCON is not set
+# CONFIG_MEMORY is not set
+# CONFIG_IIO is not set
+# CONFIG_PWM is not set
+# CONFIG_IPACK_BUS is not set
+# CONFIG_RESET_CONTROLLER is not set
+# CONFIG_FMC is not set
+
+#
+# PHY Subsystem
+#
+# CONFIG_GENERIC_PHY is not set
+# CONFIG_BCM_KONA_USB2_PHY is not set
+# CONFIG_POWERCAP is not set
+# CONFIG_MCB is not set
+
+#
+# Android
+#
+# CONFIG_ANDROID is not set
+
+#
+# File systems
+#
+# CONFIG_EXT2_FS is not set
+# CONFIG_EXT3_FS is not set
+# CONFIG_EXT4_FS is not set
+# CONFIG_REISERFS_FS is not set
+# CONFIG_JFS_FS is not set
+# CONFIG_BTRFS_FS is not set
+# CONFIG_NILFS2_FS is not set
+# CONFIG_F2FS_FS is not set
+# CONFIG_FS_POSIX_ACL is not set
+CONFIG_FILE_LOCKING=y
+# CONFIG_FSNOTIFY is not set
+# CONFIG_DNOTIFY is not set
+# CONFIG_INOTIFY_USER is not set
+# CONFIG_FANOTIFY is not set
+# CONFIG_QUOTA is not set
+# CONFIG_QUOTACTL is not set
+# CONFIG_AUTOFS4_FS is not set
+# CONFIG_FUSE_FS is not set
+# CONFIG_OVERLAY_FS is not set
+
+#
+# Caches
+#
+# CONFIG_FSCACHE is not set
+
+#
+# CD-ROM/DVD Filesystems
+#
+# CONFIG_ISO9660_FS is not set
+# CONFIG_UDF_FS is not set
+
+#
+# DOS/FAT/NT Filesystems
+#
+CONFIG_FAT_FS=y
+# CONFIG_MSDOS_FS is not set
+CONFIG_VFAT_FS=y
+CONFIG_FAT_DEFAULT_CODEPAGE=437
+CONFIG_FAT_DEFAULT_IOCHARSET="utf8"
+# CONFIG_NTFS_FS is not set
+
+#
+# Pseudo filesystems
+#
+CONFIG_PROC_FS=y
+CONFIG_PROC_SYSCTL=y
+CONFIG_KERNFS=y
+CONFIG_SYSFS=y
+# CONFIG_HUGETLB_PAGE is not set
+# CONFIG_CONFIGFS_FS is not set
+# CONFIG_MISC_FILESYSTEMS is not set
+CONFIG_NLS=y
+CONFIG_NLS_DEFAULT="utf8"
+# CONFIG_NLS_CODEPAGE_437 is not set
+# CONFIG_NLS_CODEPAGE_737 is not set
+# CONFIG_NLS_CODEPAGE_775 is not set
+# CONFIG_NLS_CODEPAGE_850 is not set
+# CONFIG_NLS_CODEPAGE_852 is not set
+# CONFIG_NLS_CODEPAGE_855 is not set
+# CONFIG_NLS_CODEPAGE_857 is not set
+# CONFIG_NLS_CODEPAGE_860 is not set
+# CONFIG_NLS_CODEPAGE_861 is not set
+# CONFIG_NLS_CODEPAGE_862 is not set
+# CONFIG_NLS_CODEPAGE_863 is not set
+# CONFIG_NLS_CODEPAGE_864 is not set
+# CONFIG_NLS_CODEPAGE_865 is not set
+# CONFIG_NLS_CODEPAGE_866 is not set
+# CONFIG_NLS_CODEPAGE_869 is not set
+# CONFIG_NLS_CODEPAGE_936 is not set
+# CONFIG_NLS_CODEPAGE_950 is not set
+# CONFIG_NLS_CODEPAGE_932 is not set
+# CONFIG_NLS_CODEPAGE_949 is not set
+# CONFIG_NLS_CODEPAGE_874 is not set
+# CONFIG_NLS_ISO8859_8 is not set
+# CONFIG_NLS_CODEPAGE_1250 is not set
+# CONFIG_NLS_CODEPAGE_1251 is not set
+# CONFIG_NLS_ASCII is not set
+# CONFIG_NLS_ISO8859_1 is not set
+# CONFIG_NLS_ISO8859_2 is not set
+# CONFIG_NLS_ISO8859_3 is not set
+# CONFIG_NLS_ISO8859_4 is not set
+# CONFIG_NLS_ISO8859_5 is not set
+# CONFIG_NLS_ISO8859_6 is not set
+# CONFIG_NLS_ISO8859_7 is not set
+# CONFIG_NLS_ISO8859_9 is not set
+# CONFIG_NLS_ISO8859_13 is not set
+# CONFIG_NLS_ISO8859_14 is not set
+# CONFIG_NLS_ISO8859_15 is not set
+# CONFIG_NLS_KOI8_R is not set
+# CONFIG_NLS_KOI8_U is not set
+# CONFIG_NLS_MAC_ROMAN is not set
+# CONFIG_NLS_MAC_CELTIC is not set
+# CONFIG_NLS_MAC_CENTEURO is not set
+# CONFIG_NLS_MAC_CROATIAN is not set
+# CONFIG_NLS_MAC_CYRILLIC is not set
+# CONFIG_NLS_MAC_GAELIC is not set
+# CONFIG_NLS_MAC_GREEK is not set
+# CONFIG_NLS_MAC_ICELAND is not set
+# CONFIG_NLS_MAC_INUIT is not set
+# CONFIG_NLS_MAC_ROMANIAN is not set
+# CONFIG_NLS_MAC_TURKISH is not set
+CONFIG_NLS_UTF8=y
+
+#
+# Kernel hacking
+#
+CONFIG_TRACE_IRQFLAGS_SUPPORT=y
+
+#
+# printk and dmesg options
+#
+# CONFIG_PRINTK_TIME is not set
+CONFIG_MESSAGE_LOGLEVEL_DEFAULT=4
+
+#
+# Compile-time checks and compiler options
+#
+# CONFIG_ENABLE_WARN_DEPRECATED is not set
+# CONFIG_ENABLE_MUST_CHECK is not set
+CONFIG_FRAME_WARN=1024
+# CONFIG_STRIP_ASM_SYMS is not set
+# CONFIG_UNUSED_SYMBOLS is not set
+# CONFIG_DEBUG_FS is not set
+# CONFIG_HEADERS_CHECK is not set
+# CONFIG_DEBUG_SECTION_MISMATCH is not set
+# CONFIG_MAGIC_SYSRQ is not set
+# CONFIG_DEBUG_KERNEL is not set
+
+#
+# Memory Debugging
+#
+# CONFIG_PAGE_EXTENSION is not set
+# CONFIG_SLUB_DEBUG_ON is not set
+# CONFIG_SLUB_STATS is not set
+CONFIG_HAVE_DEBUG_KMEMLEAK=y
+CONFIG_DEBUG_MEMORY_INIT=y
+
+#
+# Debug Lockups and Hangs
+#
+# CONFIG_PANIC_ON_OOPS is not set
+CONFIG_PANIC_ON_OOPS_VALUE=0
+CONFIG_PANIC_TIMEOUT=0
+# CONFIG_DEBUG_TIMEKEEPING is not set
+
+#
+# Lock Debugging (spinlocks, mutexes, etc...)
+#
+# CONFIG_STACKTRACE is not set
+CONFIG_HAVE_DEBUG_BUGVERBOSE=y
+CONFIG_DEBUG_BUGVERBOSE=y
+
+#
+# RCU Debugging
+#
+# CONFIG_PROVE_RCU is not set
+# CONFIG_SPARSE_RCU_POINTER is not set
+# CONFIG_TORTURE_TEST is not set
+CONFIG_HAVE_FUNCTION_TRACER=y
+CONFIG_HAVE_FUNCTION_GRAPH_TRACER=y
+CONFIG_HAVE_DYNAMIC_FTRACE=y
+CONFIG_HAVE_FTRACE_MCOUNT_RECORD=y
+CONFIG_HAVE_SYSCALL_TRACEPOINTS=y
+CONFIG_TRACING_SUPPORT=y
+# CONFIG_FTRACE is not set
+
+#
+# Runtime Testing
+#
+# CONFIG_ATOMIC64_SELFTEST is not set
+# CONFIG_TEST_HEXDUMP is not set
+# CONFIG_TEST_STRING_HELPERS is not set
+# CONFIG_TEST_KSTRTOX is not set
+# CONFIG_TEST_RHASHTABLE is not set
+# CONFIG_DMA_API_DEBUG is not set
+# CONFIG_TEST_FIRMWARE is not set
+# CONFIG_TEST_UDELAY is not set
+# CONFIG_MEMTEST is not set
+# CONFIG_SAMPLES is not set
+CONFIG_HAVE_ARCH_KGDB=y
+# CONFIG_SH_STANDARD_BIOS is not set
+# CONFIG_DWARF_UNWINDER is not set
+
+#
+# Security options
+#
+# CONFIG_KEYS is not set
+# CONFIG_SECURITY_DMESG_RESTRICT is not set
+# CONFIG_SECURITY is not set
+# CONFIG_SECURITYFS is not set
+CONFIG_DEFAULT_SECURITY_DAC=y
+CONFIG_DEFAULT_SECURITY=""
+# CONFIG_CRYPTO is not set
+# CONFIG_BINARY_PRINTF is not set
+
+#
+# Library routines
+#
+CONFIG_BITREVERSE=y
+# CONFIG_HAVE_ARCH_BITREVERSE is not set
+CONFIG_GENERIC_STRNCPY_FROM_USER=y
+CONFIG_GENERIC_STRNLEN_USER=y
+CONFIG_GENERIC_IO=y
+# CONFIG_CRC_CCITT is not set
+# CONFIG_CRC16 is not set
+# CONFIG_CRC_T10DIF is not set
+# CONFIG_CRC_ITU_T is not set
+CONFIG_CRC32=y
+# CONFIG_CRC32_SELFTEST is not set
+CONFIG_CRC32_SLICEBY8=y
+# CONFIG_CRC32_SLICEBY4 is not set
+# CONFIG_CRC32_SARWATE is not set
+# CONFIG_CRC32_BIT is not set
+# CONFIG_CRC7 is not set
+# CONFIG_LIBCRC32C is not set
+# CONFIG_CRC8 is not set
+# CONFIG_AUDIT_ARCH_COMPAT_GENERIC is not set
+# CONFIG_RANDOM32_SELFTEST is not set
+# CONFIG_XZ_DEC is not set
+# CONFIG_XZ_DEC_BCJ is not set
+CONFIG_HAS_IOMEM=y
+CONFIG_HAS_DMA=y
+CONFIG_GENERIC_ATOMIC64=y
+CONFIG_ARCH_HAS_ATOMIC64_DEC_IF_POSITIVE=y
+# CONFIG_AVERAGE is not set
+# CONFIG_CORDIC is not set
+# CONFIG_DDR is not set
+# CONFIG_ARCH_HAS_SG_CHAIN is not set
diff -Nur linux-4.1.13.orig/arch/sh/include/asm/board-0pf.h linux-4.1.13/arch/sh/include/asm/board-0pf.h
--- linux-4.1.13.orig/arch/sh/include/asm/board-0pf.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-4.1.13/arch/sh/include/asm/board-0pf.h	2015-12-05 00:16:48.000000000 +0100
@@ -0,0 +1,247 @@
+#ifndef SGM_BOARD_H
+#define SGM_BOARD_H
+
+#define sys_IntTable (*(unsigned*)0x0)
+#define sys_IntVectors 256
+
+/* Some of interrupt is fixed vector */
+#define Irq_MRES	0x02	/* Manual reset */
+#define Irq_CPUERR	0x09
+#define Irq_DMAERR	0x0a
+#define Irq_NMI		0x0b
+#define Irq_PIT		0x10	/* 100 Hz PIT */
+#define Irq_EMAC	0x11	/* irqs(0) */
+#define Irq_UART0	0x12	/* irqs(1) */
+#define Irq_GPS		0x13	/* irqs(2) */
+#define Irq_Ext		0x14	/* irqs(3)  use by CS42518*/
+#define Irq_1PPS	0x16	/* irqs(5) */
+#define Irq_UART1	0x17	/* irqs(6) */
+#define Irq_I2C		0x18	/* irqs(7) */
+#define Irq_TMR		0x19	/* a 12 bit countdown counter */
+#define Irq_GPIO	0x15
+
+/* External interrupt IDs */
+#define EIrqID_EMAC	0
+#define EIrqID_UART0	1
+#define EIrqID_GPS	2
+#define EIrqID_Ext	3
+#define EIrqID_GPIO	4
+#define EIrqID_1PPS	5
+#define EIrqID_UART1	6
+#define EIrqID_I2C	7
+
+/* External Interrupt ID convert to interrupt vector */
+#define ID2Vect(x)	(0x11 + (x))
+
+/* Convert external interupt ID to priority value */
+#define ID2Pri(id, pri)	((pri) << ((id) <<2))
+
+/* Convert vector to interrupt entry address */
+#define Vect2Irq(x)	((x) << 2)
+
+#define PIT_IRQ		Vect2Irq(Irq_PIT)
+#define EMAC_IRQ	Vect2Irq(Irq_EMAC)
+#define UART0_IRQ	Vect2Irq(Irq_UART0)
+#define GPS_IRQ		Vect2Irq(Irq_GPS)
+#define EXT_IRQ		Vect2Irq(Irq_Ext)
+#define UART1_IRQ	Vect2Irq(Irq_UART1)
+#define I2C_IRQ		Vect2Irq(Irq_I2C)
+#define TMR_IRQ		Vect2Irq(Irq_TMR)
+
+
+/* End of interrupt definations */
+#define sys_RAM_BASE 0x10000000
+#define sys_PIO_BASE 0xabcd0000
+#define sys_SPI_BASE 0xabcd0040
+#define sys_I2C_BASE 0xabcd0080 // 0xabcd0020
+#define sys_UART0_BASE 0xabcd0100
+#define sys_SYS_BASE 0xabcd0200
+#define sys_UART1_BASE 0xabcd0300
+#define sys_GPS_BASE 0xabcd0400
+#define sys_D2A_BASE 0xabcd0500
+#define sys_EMAC_BASE 0xabce0000
+
+#define AQ_PIO		(*(volatile unsigned int *)sys_PIO_BASE)
+#define AQ_I2C		(*(volatile unsigned int *)sys_I2C_BASE)
+#define AQ_SPI		(*(volatile unsigned int *)sys_SPI_BASE)
+#define AQ_UART0	(*(volatile unsigned int *)sys_UART0_BASE)
+#define AQ_SYS		(*(volatile unsigned int *)sys_SYS_BASE)
+#define AQ_UART1	(*(volatile unsigned int *)sys_UART1_BASE)
+#define AQ_GPS		(*(volatile unsigned int *)sys_GPS_BASE)
+#define AQ_D2A		(*(volatile unsigned int *)sys_D2A_BASE)
+#define AQ_EMAC		(*(volatile unsigned int *)sys_EMAC_BASE)
+
+
+struct st_uart16550
+{
+       	unsigned int RTX;
+       	unsigned int IER;
+       	unsigned int IIR;
+       	unsigned int LCR;
+       	unsigned int MCR;
+       	unsigned int LSR;
+       	unsigned int MSR;
+       	unsigned int SCR;
+};
+#define uLSRDR		0x01
+#define uLSROE		0x02
+#define uLSRPE		0x04
+#define uLSRFE		0x08
+#define uLSRBI		0x10
+#define uLSRTHRE	0x20
+#define uLSRTEMT	0x40
+#define uLSRRFE		0x80	/* Error in Revr FIFO */
+
+#if 0
+#define B115200 0x000a
+#define B38400	0x001e
+#define B19200	0x003c
+#define B9600	0x0078
+#define B4800	0x00f0
+#endif
+
+/* the following is belong to sys_SYS_BASE */
+#define Sys_IntCon	0x0
+/* When SIC_BRKON is set, BreadAddress will compare with Bus address to generate NMI interrupt */
+#define Sys_BRKADR	0x04
+/* Interrupt priority is 4 bits width, irqs(0) is [3,0], irqs(1) is [7,4] ... */
+#define Sys_IntPri	0x08
+/* End of offset define of sys_SYS_BASE */
+/* Refer to Aquarius datasheet Page 12, NMI is lvl16, and lvl0 will not be accept */
+/* Refer to define.v, IBit in SR [7:4] */
+#define SIC_ENMI	((unsigned int) 0x1<<31)	/* Emulate NMI */
+#define SIC EIRQ	((unsigned int) 0x1<<30)	/* Emulate IRQ */
+#define SIC_ECER	((unsigned int) 0x1<<29)	/* Emulate CPU Address Error */
+#define SIC_EDER	((unsigned int) 0x1<<28)	/* Emulate DMA Address Error */
+#define SIC_EMRS	((unsigned int) 0x1<<27)	/* Emulate Manual Reset */
+#define SIC_EPIT	((unsigned int) 0x1<<26)	/* Enable Periodical interval timer(PIT) */
+#define SIC_TMRON	((unsigned int) 0x1<<25)	/* Enable timer */
+#define SIC_BRKON	((unsigned int) 0x1<<24)	/* Break ON */
+#define SIC_ILVL	((unsigned int) 0xF<<20)	/* interrupt level for PIT */
+#define SIC_IVEC	((unsigned int) 0xFF<<12)	/* Interrupt Vector for PIT */
+#define SIC_TMR		((unsigned int)0xFFF)		/* Interval Timer when 0x0, it request IRQ*/
+
+/* PIO registers offset */
+#define Poffset_IO      0x00
+#define Poffset_imask   0x04
+#define Poffset_redge   0x08
+#define Poffset_changes 0x0c
+
+/* Keys are connected to Parallel Input, Active low */
+#define Pio_KeyEnter 	0x0001
+#define Pio_KeyESC	0x0002
+#define Pio_KeyNorth	0x0020
+#define Pio_KeyEast	0x0040
+#define Pio_KeySouth	0x0080
+#define Pio_KeyWest	0x0100
+
+/* SD_CD is active high of this bit */
+#define Pio_SD_CD	0x00200000
+
+#define Pio_1PPS	0x00800000
+
+/* IMPORTANT!!! Pio_LEDPwr is connected with with reset pins of USB, ETH-PHY
+ *              and GPS. DON'T CHANGE IT or use it for now!!!
+ * TODO: VHDL needs to fix Power LED to other location with set and reset feature
+ */
+#define Pio_LEDPwr	0x0010
+#define Pio_LEDErr	0x0020
+#define Pio_TP70	0x0040
+
+#if 0
+	#define I2c_busy	0x8000
+	#define I2c_next	0x4000
+	#define I2c_ack		0x2000
+	#define I2c_timeout	0x1000
+	#define I2c_timer	0x0800
+	#define I2c_mask 	0xf800
+#else
+        #define I2cO_ctrl       0x00
+        #define I2cO_slen       0x04
+        #define I2cO_word       0x0C
+
+        /* for I2cO_ctrl */
+        #define I2cC_busy       0x01
+        #define I2cC_timeout    0x02
+        #define I2cC_complete   0x04
+        #define I2cC_reset      0x08
+        #define I2cC_run        0x10
+        #define I2cC_irqen      0x20
+        #define I2cC_clk        0x40
+        #define I2cC_dat        0x80
+	#define I2cC_MaskDelay  0xff00
+	#define I2c_delay(x) ((x)<< 8)
+	#define I2cC_MaskAckTimeout     0xf0000
+	#define I2c_timeout(x)  ((x) << 16)
+        /* for I2cO_slen */
+        #define I2cS_MaskXlen   0x1f
+        #define I2cS_MaxLen     16
+        #define I2cS_MaskSpeed  0x30000
+        #define I2cS_100k       0x0
+        #define I2cS_400k       0x10000
+        #define I2cS_1m         0x20000
+        #define I2cS_3m4        0x30000
+        #define I2cS_Maskwordcount      0xf80000
+#endif
+
+/***********************************************************/
+/************************************   EMAC  **************/
+/***********************************************************/
+
+#define AQ_EMAC_BASE	0xABCE0000
+#define AQ_EMAC_CONTROL	0xABCE0000
+#define AQ_EMAC_STATUS	0xABCE0000
+
+/* Control bits */
+#define AQ_EMAC_ENABLE_RX	0x00000002
+#define AQ_EMAC_ENABLE_TX	0x00000004
+#define AQ_EMAC_READ		0x00000010
+#define AQ_EMAC_ENABLE_INT_RX	0x00000020
+#define AQ_EMAC_ENABLE_INT_TX	0x00000040
+
+/* Status bits */
+#define AQ_EMAC_TX_BUSY		0x00000004
+#define AQ_EMAC_COMPLETE	0x00000100
+#define AQ_EMAC_CRC		0x00000200
+
+#define AQ_EMAC_TX_LEN		0xABCE0004
+#define AQ_EMAC_MACL		0xABCE0008
+#define AQ_EMAC_MACH		0xABCE000C
+#define AQ_EMAC_RX_BUF		0xABCE1000
+#define AQ_EMAC_TX_BUF		0xABCE1800
+
+#define Emac_Rbuf	0x1000
+#define Emac_Xbuf	0x1800
+#define Emac_Ctrl	0x0000
+#define Emac_xlen	0x0004
+#define Emac_MACL	0x0008
+#define Emac_MACH	0x000c
+#define ECtrl_RecvEnable	0x2	/* Receive enable */
+#define ECtrl_Xmit		0x4	/* Read: Transmit busy(1); Write: Start transmit(1) */
+#define ECtrl_MACReset		0x8	/* Reset MAC address */
+#define ECtrl_Read		0x10	/* complete read from Receive FIFO */
+#define ECtrl_RIntEnable	0x20	/* Receive interrupt enable(1) */
+#define ECtrl_XIntEnable	0x40	/* Transmit interrupt enable(1) */
+#define ECtrl_PROM		0x80	/* Promiscuous Mode enable(1)/disable(0) */
+#define ECtrl_Complete		0x100	/* Receive packet waiting in FIFO */
+#define ECtrl_CRC		0x200	/* Receive packet has CRC error */
+#define ECtrl_getrxlen(x) ((x) >> 16)	/* Length of received package, when ECtrl_Complete is set */
+
+#define Spi_Ctrl	0x0
+#define Spi_Data	0x4
+#define SpiCtrl_ACS	0x01 	/* chipselect for applcation data */
+#define SpiCtrl_CCS	0x04	/* chipselect for FPGA configure */
+#define SpiCtrl_DCS	0x10	/* chipselect for D2A or extra SPI device */
+#define SpiCtrl_setDiv(x) ((x) << 27)	/* Div contrl SPI_CK = 12.5/(div + 1), Min: 400KHz for now*/
+#define SpiCtrl_Xmit	0x02
+#define SpiCtrl_Busy	0x02
+#define SpiCtrl_Loop	0x08	/* When it assert, mosi will connect to miso */
+/* by default SPI run at 12.5 MHz,maxium speed for Spartan 3E, for SPI Flash
+ * We need a DDS delay for different devices
+ */
+
+#define SHJ_PIT_PMR	0xABCD0210
+#define SHJ_PIT_PCNTR	0xABCD0214
+#define SHJ_NSEC_PER_CLOCK 0xABCD0218
+
+#endif
diff -Nur linux-4.1.13.orig/arch/sh/include/asm/processor.h linux-4.1.13/arch/sh/include/asm/processor.h
--- linux-4.1.13.orig/arch/sh/include/asm/processor.h	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/include/asm/processor.h	2015-12-05 00:16:49.000000000 +0100
@@ -15,7 +15,7 @@
  */
 enum cpu_type {
 	/* SH-2 types */
-	CPU_SH7619,
+	CPU_SH7619, CPU_0PF,
 
 	/* SH-2A types */
 	CPU_SH7201, CPU_SH7203, CPU_SH7206, CPU_SH7263, CPU_SH7264, CPU_SH7269,
diff -Nur linux-4.1.13.orig/arch/sh/include/cpu-sh2/cpu/cache.h linux-4.1.13/arch/sh/include/cpu-sh2/cpu/cache.h
--- linux-4.1.13.orig/arch/sh/include/cpu-sh2/cpu/cache.h	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/include/cpu-sh2/cpu/cache.h	2015-12-05 00:16:49.000000000 +0100
@@ -38,6 +38,10 @@
 #define CCR_CACHE_INVALIDATE	CCR_CACHE_CF
 #define CACHE_PHYSADDR_MASK	0x1ffffc00
 
+#elif defined(CONFIG_CPU_SUBTYPE_0PF)
+#define CCR			0xabcd00c0
+#define CCR_CACHE_ENABLE	0x80000000
+#define CCR_CACHE_RESET		0x101
 #endif
 
 #endif /* __ASM_CPU_SH2_CACHE_H */
diff -Nur linux-4.1.13.orig/arch/sh/kernel/cpu/init.c linux-4.1.13/arch/sh/kernel/cpu/init.c
--- linux-4.1.13.orig/arch/sh/kernel/cpu/init.c	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/cpu/init.c	2015-12-05 00:16:49.000000000 +0100
@@ -106,7 +106,7 @@
 /*
  * Generic first-level cache init
  */
-#ifdef CONFIG_SUPERH32
+#if defined(CONFIG_SUPERH32) && !defined(CONFIG_CPU_SUBTYPE_0PF)
 static void cache_init(void)
 {
 	unsigned long ccr, flags;
diff -Nur linux-4.1.13.orig/arch/sh/kernel/cpu/proc.c linux-4.1.13/arch/sh/kernel/cpu/proc.c
--- linux-4.1.13.orig/arch/sh/kernel/cpu/proc.c	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/cpu/proc.c	2015-12-05 00:16:49.000000000 +0100
@@ -26,6 +26,7 @@
 	[CPU_SH5_101]	= "SH5-101",	[CPU_SH5_103]	= "SH5-103",
 	[CPU_MXG]	= "MX-G",	[CPU_SH7723]	= "SH7723",
 	[CPU_SH7366]	= "SH7366",	[CPU_SH7724]	= "SH7724",
+	[CPU_0PF]	= "SH2J-0PF",
 	[CPU_SH7372]	= "SH7372",	[CPU_SH7734]	= "SH7734",
 	[CPU_SH_NONE]	= "Unknown"
 };
diff -Nur linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/Makefile linux-4.1.13/arch/sh/kernel/cpu/sh2/Makefile
--- linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/Makefile	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/cpu/sh2/Makefile	2015-12-05 00:16:49.000000000 +0100
@@ -5,3 +5,4 @@
 obj-y	:= ex.o probe.o entry.o
 
 obj-$(CONFIG_CPU_SUBTYPE_SH7619) += setup-sh7619.o clock-sh7619.o
+obj-$(CONFIG_CPU_SUBTYPE_0PF) += setup-0pf.o clock-0pf.o
diff -Nur linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/clock-0pf.c linux-4.1.13/arch/sh/kernel/cpu/sh2/clock-0pf.c
--- linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/clock-0pf.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/cpu/sh2/clock-0pf.c	2015-12-05 00:16:48.000000000 +0100
@@ -0,0 +1,80 @@
+/*
+ * arch/sh/kernel/cpu/sh2/clock-0pf.c
+ *
+ * 0PF FPGA support for the clock framework
+ *
+ *  Copyright (C) 2012  SEI, Inc.
+ *
+ * Based on clock-sh4.c
+ *  Copyright (C) 2005  Paul Mundt
+ *  Copyright (C) 2009  D. Jeff Dionne
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ */
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <asm/clock.h>
+#include <linux/timex.h>
+#include <linux/profile.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+
+#include <asm/freq.h>
+#include <asm/io.h>
+
+static void master_clk_init(struct clk *clk)
+{
+	clk->rate = CONFIG_SH_PCLK_FREQ; /* Fixed Rate */
+}
+
+static struct sh_clk_ops shj_master_clk_ops = {
+	.init		= master_clk_init,
+};
+
+static unsigned long module_clk_recalc(struct clk *clk)
+{
+	return clk->parent->rate;
+}
+
+static struct sh_clk_ops shj_module_clk_ops = {
+	.recalc		= module_clk_recalc,
+};
+
+static unsigned long bus_clk_recalc(struct clk *clk)
+{
+	return clk->parent->rate;
+}
+
+static struct sh_clk_ops shj_bus_clk_ops = {
+	.recalc		= bus_clk_recalc,
+};
+
+static struct sh_clk_ops shj_cpu_clk_ops = {
+	.recalc		= followparent_recalc,
+};
+
+static struct sh_clk_ops *shj_clk_ops[] = {
+	&shj_master_clk_ops,
+	&shj_module_clk_ops,
+	&shj_bus_clk_ops,
+	&shj_cpu_clk_ops,
+};
+
+void __init arch_init_clk_ops(struct sh_clk_ops **ops, int idx)
+{
+	if (idx < ARRAY_SIZE(shj_clk_ops))
+		*ops = shj_clk_ops[idx];
+}
+
+int __init arch_clk_init()
+{
+	int ret;
+
+	printk("%s(): 0PF Clock init...\n", __func__);
+
+	ret = cpg_clk_init(); /* appease Over-engineered "clock infrastructure" */
+
+	return ret;
+}
diff -Nur linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/entry.S linux-4.1.13/arch/sh/kernel/cpu/sh2/entry.S
--- linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/entry.S	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/cpu/sh2/entry.S	2015-12-05 00:16:49.000000000 +0100
@@ -3,6 +3,7 @@
  *
  * The SH-2 exception entry
  *
+ * Copyright (C) 2012  SEI,Inc.
  * Copyright (C) 2005-2008 Yoshinori Sato
  * Copyright (C) 2005  AXE,Inc.
  *
@@ -147,7 +148,11 @@
 	mov	#32,r8
 	cmp/hs	r8,r9
 	bt	trap_entry	! 64 > vec >= 32  is trap
-
+#if defined(CONFIG_CPU_SUBTYPE_0PF)
+	mov	#16,r8
+	cmp/hs	r8,r9
+	bt	interrupt_entry	! 32 > vec >= 16  is interrupt
+#endif
 	mov.l	4f,r8
 	mov	r9,r4
 	shll2	r9
@@ -245,6 +250,19 @@
 	.align	2
 1:	.long	do_address_error
 
+#if defined(CONFIG_CPU_SUBTYPE_0PF)
+ENTRY(pc_address_error_trap_handler)
+	mov	r15,r4				! regs
+	mov	#OFF_PC,r0
+	mov.l	@(r0,r15),r6			! pc
+	mov.l	1f,r0
+	jmp	@r0
+	 mov	#0,r5				! writeaccess is unknown
+
+	.align	2
+1:	.long	do_pc_address_error
+#endif // CONFIG_CPU_SUBTYPE_0PF
+
 restore_all:
 	stc	sr,r0
 	or	#0xf0,r0
diff -Nur linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/probe.c linux-4.1.13/arch/sh/kernel/cpu/sh2/probe.c
--- linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/probe.c	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/cpu/sh2/probe.c	2015-12-05 00:16:49.000000000 +0100
@@ -24,6 +24,12 @@
 	boot_cpu_data.dcache.linesz		= L1_CACHE_BYTES;
 	boot_cpu_data.dcache.flags		= 0;
 #endif
+
+#if defined(CONFIG_CPU_SUBTYPE_0PF)
+	boot_cpu_data.type                      = CPU_0PF;
+	boot_cpu_data.dcache.flags              = 0;
+#endif
+
 	/*
 	 * SH-2 doesn't have separate caches
 	 */
diff -Nur linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/setup-0pf.c linux-4.1.13/arch/sh/kernel/cpu/sh2/setup-0pf.c
--- linux-4.1.13.orig/arch/sh/kernel/cpu/sh2/setup-0pf.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/cpu/sh2/setup-0pf.c	2015-12-05 00:16:48.000000000 +0100
@@ -0,0 +1,82 @@
+/*
+ * 0PF-FPGA Setup
+ *
+ *  Copyright (C) 2006  Yoshinori Sato
+ *  Copyright (C) 2009  Paul Mundt
+ *  Copyright (C) 2009  D. Jeff Dionne
+ *  Copyright (C) 2012  SEI, Inc.
+ *                      by Oleksandr Zhadan
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ */
+#include <linux/platform_device.h>
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/io.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+#include <linux/serial_8250.h>
+#include <asm/board-0pf.h>
+
+#if defined(CONFIG_SERIAL_UARTLITE_0PF)
+static struct resource shj_uartlite_resources[] = {
+	[0] = DEFINE_RES_MEM(0xABCD0100, 16),
+	[1] = DEFINE_RES_IRQ(0x12),
+
+	[2] = DEFINE_RES_MEM(0xABCD0300, 16),
+	[3] = DEFINE_RES_IRQ(0x17),
+
+	[4] = DEFINE_RES_MEM(0xABCD0400, 16),
+	[5] = DEFINE_RES_IRQ(0x13),
+};
+
+static struct platform_device shj_uartlite_device[] = {
+	[0] = { .name = "uartlite", .id = 0 },
+	[1] = { .name = "uartlite", .id = 1 },
+	[2] = { .name = "uartlite", .id = 2 },
+};
+#endif
+
+/*****************************************************************************
+ *  0PF FPGA platform devices
+ ****************************************************************************/
+static struct platform_device *shj_devices[] __initdata = {
+#if defined(CONFIG_SERIAL_UARTLITE_0PF)
+	shj_uartlite_device,
+	shj_uartlite_device + 1,
+	shj_uartlite_device + 2,
+#endif
+};
+
+static int __init shj_devices_setup(void)
+{
+	int i;
+	pr_info("%s(): registering device resources\n", __func__);
+
+#if defined(CONFIG_SERIAL_UARTLITE_0PF)
+	for (i = 0; i < ARRAY_SIZE(shj_uartlite_device); i++) {
+		printk("Register UARTLITE resources %d\n", i);
+		if (platform_device_add_resources(
+				shj_uartlite_device + i,
+				shj_uartlite_resources + 2 * i,
+				2))
+			pr_err("Failed to set uartlite %d IRQ and MEM\n", i);
+
+	}
+#endif
+	platform_add_devices(shj_devices, ARRAY_SIZE(shj_devices));
+
+	return 0;
+}
+
+arch_initcall(shj_devices_setup);
+
+void __init native_machine_early_platform_add_devices(void)
+{
+}
+
+void __init plat_irq_setup(void)
+{
+}
diff -Nur linux-4.1.13.orig/arch/sh/kernel/irq.c linux-4.1.13/arch/sh/kernel/irq.c
--- linux-4.1.13.orig/arch/sh/kernel/irq.c	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/irq.c	2015-12-05 00:16:49.000000000 +0100
@@ -20,6 +20,8 @@
 #include <asm/thread_info.h>
 #include <cpu/mmu_context.h>
 
+#include <asm/board-0pf.h>
+
 atomic_t irq_err_count;
 
 /*
@@ -175,11 +177,24 @@
 	);
 }
 #else
+#define noinline __attribute__((noinline))
+static noinline void handle_irq_UART0(unsigned int irq) { generic_handle_irq(irq); }
+static noinline void handle_irq_UART1(unsigned int irq) { generic_handle_irq(irq); }
+static noinline void handle_irq_GPS(unsigned int irq) { generic_handle_irq(irq); }
+static noinline void handle_irq_EMAC(unsigned int irq) { generic_handle_irq(irq); }
 static inline void handle_one_irq(unsigned int irq)
 {
-	generic_handle_irq(irq);
+	switch(irq) {
+	case Irq_UART0: handle_irq_UART0(irq); break;
+	case Irq_UART1: handle_irq_UART1(irq); break;
+	case Irq_GPS:   handle_irq_GPS(irq); break;
+	case Irq_EMAC:  handle_irq_EMAC(irq); break;
+	default:
+		generic_handle_irq(irq);
+		break;
+	}
 }
-#endif
+#endif // CONFIG_IRQSTACKS
 
 asmlinkage __irq_entry int do_IRQ(unsigned int irq, struct pt_regs *regs)
 {
diff -Nur linux-4.1.13.orig/arch/sh/kernel/traps_32.c linux-4.1.13/arch/sh/kernel/traps_32.c
--- linux-4.1.13.orig/arch/sh/kernel/traps_32.c	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/kernel/traps_32.c	2015-12-05 00:16:49.000000000 +0100
@@ -34,6 +34,7 @@
 #ifdef CONFIG_CPU_SH2
 # define TRAP_RESERVED_INST	4
 # define TRAP_ILLEGAL_SLOT_INST	6
+# define TRAP_PC_ADDRESS_ERROR	8 // Aug 20, 2012 ulianov - SEI extension - PC governor
 # define TRAP_ADDRESS_ERROR	9
 # ifdef CONFIG_CPU_SH2A
 #  define TRAP_UBC		12
@@ -458,6 +459,14 @@
 	return ret;
 }
 
+#if defined(CONFIG_CPU_SUBTYPE_0PF)
+asmlinkage void do_pc_address_error(struct pt_regs *regs,
+				 unsigned long writeaccess,
+				 unsigned long address)
+{
+}
+#endif // CONFIG_CPU_SUBTYPE_0PF
+
 /*
  * Handle various address error exceptions:
  *  - instruction address error:
@@ -779,6 +788,9 @@
 #endif
 
 #ifdef CONFIG_CPU_SH2
+    #if defined(CONFIG_CPU_SUBTYPE_0PF)
+	set_exception_table_vec(TRAP_PC_ADDRESS_ERROR, address_error_trap_handler);
+    #endif
 	set_exception_table_vec(TRAP_ADDRESS_ERROR, address_error_trap_handler);
 #endif
 #ifdef CONFIG_CPU_SH2A
diff -Nur linux-4.1.13.orig/arch/sh/mm/cache-sh2.c linux-4.1.13/arch/sh/mm/cache-sh2.c
--- linux-4.1.13.orig/arch/sh/mm/cache-sh2.c	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/mm/cache-sh2.c	2015-12-05 00:16:49.000000000 +0100
@@ -3,6 +3,7 @@
  *
  * Copyright (C) 2002 Paul Mundt
  * Copyright (C) 2008 Yoshinori Sato
+ * Copyright (C) 2012 SEI, Inc.
  *
  * Released under the terms of the GNU GPL v2.0.
  */
@@ -16,6 +17,30 @@
 #include <asm/cacheflush.h>
 #include <asm/io.h>
 
+#if defined(CONFIG_CPU_SUBTYPE_0PF)
+
+// Just flush the whole thing each time
+static void j2_flush_icache_range(void *fwoosh)
+{
+	__raw_writel(CCR_CACHE_RESET, CCR);
+}
+
+// This should never happen, but...
+static void j2_flush_icache_page(void *fwoosh)
+{
+	__raw_writel(CCR_CACHE_RESET, CCR);
+}
+
+void __init sh2_cache_init(void)
+{
+	local_flush_icache_range = j2_flush_icache_range;
+	local_flush_icache_page = j2_flush_icache_page;
+	boot_cpu_data.dcache.n_aliases = 0;
+
+	__raw_writel(CCR_CACHE_RESET, CCR);
+}
+
+#else
 static void sh2__flush_wback_region(void *start, int size)
 {
 	unsigned long v;
@@ -89,3 +114,4 @@
 	__flush_purge_region		= sh2__flush_purge_region;
 	__flush_invalidate_region	= sh2__flush_invalidate_region;
 }
+#endif
diff -Nur linux-4.1.13.orig/arch/sh/mm/cache.c linux-4.1.13/arch/sh/mm/cache.c
--- linux-4.1.13.orig/arch/sh/mm/cache.c	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/arch/sh/mm/cache.c	2015-12-05 00:16:49.000000000 +0100
@@ -258,14 +258,16 @@
 		boot_cpu_data.icache.entry_mask,
 		boot_cpu_data.icache.alias_mask,
 		boot_cpu_data.icache.n_aliases);
-	printk(KERN_NOTICE "D-cache : n_ways=%d n_sets=%d way_incr=%d\n",
-		boot_cpu_data.dcache.ways,
-		boot_cpu_data.dcache.sets,
-		boot_cpu_data.dcache.way_incr);
-	printk(KERN_NOTICE "D-cache : entry_mask=0x%08x alias_mask=0x%08x n_aliases=%d\n",
-		boot_cpu_data.dcache.entry_mask,
-		boot_cpu_data.dcache.alias_mask,
-		boot_cpu_data.dcache.n_aliases);
+	if (boot_cpu_data.dcache.n_aliases) {
+		printk(KERN_NOTICE "D-cache : n_ways=%d n_sets=%d way_incr=%d\n",
+			boot_cpu_data.dcache.ways,
+			boot_cpu_data.dcache.sets,
+			boot_cpu_data.dcache.way_incr);
+		printk(KERN_NOTICE "D-cache : entry_mask=0x%08x alias_mask=0x%08x n_aliases=%d\n",
+			boot_cpu_data.dcache.entry_mask,
+			boot_cpu_data.dcache.alias_mask,
+			boot_cpu_data.dcache.n_aliases);
+	}
 
 	/*
 	 * Emit Secondary Cache parameters if the CPU has a probed L2.
diff -Nur linux-4.1.13.orig/drivers/tty/serial/Kconfig linux-4.1.13/drivers/tty/serial/Kconfig
--- linux-4.1.13.orig/drivers/tty/serial/Kconfig	2015-11-09 23:34:10.000000000 +0100
+++ linux-4.1.13/drivers/tty/serial/Kconfig	2015-12-05 00:16:49.000000000 +0100
@@ -594,7 +594,7 @@
 
 config SERIAL_UARTLITE
 	tristate "Xilinx uartlite serial port support"
-	depends on PPC32 || MICROBLAZE || MFD_TIMBERDALE || ARCH_ZYNQ
+	depends on PPC32 || MICROBLAZE || MFD_TIMBERDALE || ARCH_ZYNQ || CPU_SUBTYPE_0PF
 	select SERIAL_CORE
 	help
 	  Say Y here if you want to use the Xilinx uartlite serial controller.
@@ -611,6 +611,12 @@
 	  console (the system console is the device which receives all kernel
 	  messages and warnings and which allows logins in single user mode).
 
+config SERIAL_UARTLITE_0PF
+       tristate "Support 0PF UARTLITEs"
+       depends on SERIAL_UARTLITE = y && CPU_SUBTYPE_0PF
+       help
+         Say Y here to set up 0PF's UARTLITEs.
+
 config SERIAL_SUNCORE
 	bool
 	depends on SPARC
