config ADK_TARGET_SYSTEM_MIKROTIK_RB4XX
	bool "Mikrotik Routerboard 4xx"
	depends on ADK_TARGET_BIG_ENDIAN
	select ADK_TARGET_CPU_MIPS_MIPS32
	select ADK_TARGET_BOARD_ATH79
	select ADK_TARGET_WITH_MINIPCI
	select ADK_TARGET_WITH_SERIAL
	select ADK_TARGET_WITH_PCI
	select ADK_TARGET_WITH_SPI
	select ADK_TARGET_WITH_WATCHDOG
	select ADK_TARGET_WITH_NAND
	select ADK_TARGET_WITH_LEDS
	select ADK_TARGET_WITH_NET
	select ADK_TARGET_WITH_NETDEVICE
	select ADK_TARGET_WITH_BLOCK
	select ADK_TARGET_KERNEL_WITH_COMPRESSION
	help
	  Support for Mikrotik RB411/RB433/RB493g.

