diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/clock.c linux-2.6.30.5/arch/mips/ar7/clock.c
--- linux-2.6.30.5.orig/arch/mips/ar7/clock.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/clock.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,483 @@
+/*
+ * Copyright (C) 2007 Felix Fietkau <nbd@openwrt.org>
+ * Copyright (C) 2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#include <linux/init.h>
+#include <linux/types.h>
+#include <linux/module.h>
+#include <linux/delay.h>
+#include <asm/addrspace.h>
+#include <asm/io.h>
+#include <asm/ar7/ar7.h>
+
+#define BOOT_PLL_SOURCE_MASK	0x3
+#define CPU_PLL_SOURCE_SHIFT	16
+#define BUS_PLL_SOURCE_SHIFT	14
+#define USB_PLL_SOURCE_SHIFT	18
+#define DSP_PLL_SOURCE_SHIFT	22
+#define BOOT_PLL_SOURCE_AFE	0
+#define BOOT_PLL_SOURCE_BUS	0
+#define BOOT_PLL_SOURCE_REF	1
+#define BOOT_PLL_SOURCE_XTAL	2
+#define BOOT_PLL_SOURCE_CPU	3
+#define BOOT_PLL_BYPASS		0x00000020
+#define BOOT_PLL_ASYNC_MODE	0x02000000
+#define BOOT_PLL_2TO1_MODE	0x00008000
+
+#define TNETD7200_CLOCK_ID_CPU	0
+#define TNETD7200_CLOCK_ID_DSP	1
+#define TNETD7200_CLOCK_ID_USB	2
+
+#define TNETD7200_DEF_CPU_CLK	211000000
+#define TNETD7200_DEF_DSP_CLK	125000000
+#define TNETD7200_DEF_USB_CLK	48000000
+
+struct tnetd7300_clock {
+	u32 ctrl;
+#define PREDIV_MASK	0x001f0000
+#define PREDIV_SHIFT	16
+#define POSTDIV_MASK	0x0000001f
+	u32 unused1[3];
+	u32 pll;
+#define MUL_MASK	0x0000f000
+#define MUL_SHIFT	12
+#define PLL_MODE_MASK	0x00000001
+#define PLL_NDIV	0x00000800
+#define PLL_DIV		0x00000002
+#define PLL_STATUS	0x00000001
+	u32 unused2[3];
+};
+
+struct tnetd7300_clocks {
+	struct tnetd7300_clock bus;
+	struct tnetd7300_clock cpu;
+	struct tnetd7300_clock usb;
+	struct tnetd7300_clock dsp;
+};
+
+struct tnetd7200_clock {
+	u32 ctrl;
+	u32 unused1[3];
+#define DIVISOR_ENABLE_MASK 0x00008000
+	u32 mul;
+	u32 prediv;
+	u32 postdiv;
+	u32 postdiv2;
+	u32 unused2[6];
+	u32 cmd;
+	u32 status;
+	u32 cmden;
+	u32 padding[15];
+};
+
+struct tnetd7200_clocks {
+	struct tnetd7200_clock cpu;
+	struct tnetd7200_clock dsp;
+	struct tnetd7200_clock usb;
+};
+
+int ar7_cpu_clock = 150000000;
+EXPORT_SYMBOL(ar7_cpu_clock);
+int ar7_bus_clock = 125000000;
+EXPORT_SYMBOL(ar7_bus_clock);
+int ar7_dsp_clock;
+EXPORT_SYMBOL(ar7_dsp_clock);
+
+static int gcd(int a, int b)
+{
+	int c;
+
+	if (a < b) {
+		c = a;
+		a = b;
+		b = c;
+	}
+	while ((c = (a % b))) {
+		a = b;
+		b = c;
+	}
+	return b;
+}
+
+static void approximate(int base, int target, int *prediv,
+			int *postdiv, int *mul)
+{
+	int i, j, k, freq, res = target;
+	for (i = 1; i <= 16; i++)
+		for (j = 1; j <= 32; j++)
+			for (k = 1; k <= 32; k++) {
+				freq = abs(base / j * i / k - target);
+				if (freq < res) {
+					res = freq;
+					*mul = i;
+					*prediv = j;
+					*postdiv = k;
+				}
+			}
+}
+
+static void calculate(int base, int target, int *prediv, int *postdiv,
+	int *mul)
+{
+	int tmp_gcd, tmp_base, tmp_freq;
+
+	for (*prediv = 1; *prediv <= 32; (*prediv)++) {
+		tmp_base = base / *prediv;
+		tmp_gcd = gcd(target, tmp_base);
+		*mul = target / tmp_gcd;
+		*postdiv = tmp_base / tmp_gcd;
+		if ((*mul < 1) || (*mul >= 16))
+			continue;
+		if ((*postdiv > 0) & (*postdiv <= 32))
+			break;
+	}
+
+	if (base / (*prediv) * (*mul) / (*postdiv) != target) {
+		approximate(base, target, prediv, postdiv, mul);
+		tmp_freq = base / (*prediv) * (*mul) / (*postdiv);
+		printk(KERN_WARNING
+		       "Adjusted requested frequency %d to %d\n",
+		       target, tmp_freq);
+	}
+
+	printk(KERN_DEBUG "Clocks: prediv: %d, postdiv: %d, mul: %d\n",
+	       *prediv, *postdiv, *mul);
+}
+
+static int tnetd7300_dsp_clock(void)
+{
+	u32 didr1, didr2;
+	u8 rev = ar7_chip_rev();
+	didr1 = readl((void *)KSEG1ADDR(AR7_REGS_GPIO + 0x18));
+	didr2 = readl((void *)KSEG1ADDR(AR7_REGS_GPIO + 0x1c));
+	if (didr2 & (1 << 23))
+		return 0;
+	if ((rev >= 0x23) && (rev != 0x57))
+		return 250000000;
+	if ((((didr2 & 0x1fff) << 10) | ((didr1 & 0xffc00000) >> 22))
+	    > 4208000)
+		return 250000000;
+	return 0;
+}
+
+static int tnetd7300_get_clock(u32 shift, struct tnetd7300_clock *clock,
+	u32 *bootcr, u32 bus_clock)
+{
+	int product;
+	int base_clock = AR7_REF_CLOCK;
+	u32 ctrl = readl(&clock->ctrl);
+	u32 pll = readl(&clock->pll);
+	int prediv = ((ctrl & PREDIV_MASK) >> PREDIV_SHIFT) + 1;
+	int postdiv = (ctrl & POSTDIV_MASK) + 1;
+	int divisor = prediv * postdiv;
+	int mul = ((pll & MUL_MASK) >> MUL_SHIFT) + 1;
+
+	switch ((*bootcr & (BOOT_PLL_SOURCE_MASK << shift)) >> shift) {
+	case BOOT_PLL_SOURCE_BUS:
+		base_clock = bus_clock;
+		break;
+	case BOOT_PLL_SOURCE_REF:
+		base_clock = AR7_REF_CLOCK;
+		break;
+	case BOOT_PLL_SOURCE_XTAL:
+		base_clock = AR7_XTAL_CLOCK;
+		break;
+	case BOOT_PLL_SOURCE_CPU:
+		base_clock = ar7_cpu_clock;
+		break;
+	}
+
+	if (*bootcr & BOOT_PLL_BYPASS)
+		return base_clock / divisor;
+
+	if ((pll & PLL_MODE_MASK) == 0)
+		return (base_clock >> (mul / 16 + 1)) / divisor;
+
+	if ((pll & (PLL_NDIV | PLL_DIV)) == (PLL_NDIV | PLL_DIV)) {
+		product = (mul & 1) ?
+			(base_clock * mul) >> 1 :
+			(base_clock * (mul - 1)) >> 2;
+		return product / divisor;
+	}
+
+	if (mul == 16)
+		return base_clock / divisor;
+
+	return base_clock * mul / divisor;
+}
+
+static void tnetd7300_set_clock(u32 shift, struct tnetd7300_clock *clock,
+	u32 *bootcr, u32 frequency)
+{
+	int prediv, postdiv, mul;
+	int base_clock = ar7_bus_clock;
+
+	switch ((*bootcr & (BOOT_PLL_SOURCE_MASK << shift)) >> shift) {
+	case BOOT_PLL_SOURCE_BUS:
+		base_clock = ar7_bus_clock;
+		break;
+	case BOOT_PLL_SOURCE_REF:
+		base_clock = AR7_REF_CLOCK;
+		break;
+	case BOOT_PLL_SOURCE_XTAL:
+		base_clock = AR7_XTAL_CLOCK;
+		break;
+	case BOOT_PLL_SOURCE_CPU:
+		base_clock = ar7_cpu_clock;
+		break;
+	}
+
+	calculate(base_clock, frequency, &prediv, &postdiv, &mul);
+
+	writel(((prediv - 1) << PREDIV_SHIFT) | (postdiv - 1), &clock->ctrl);
+	mdelay(1);
+	writel(4, &clock->pll);
+	while (readl(&clock->pll) & PLL_STATUS);
+	writel(((mul - 1) << MUL_SHIFT) | (0xff << 3) | 0x0e, &clock->pll);
+	mdelay(75);
+}
+
+static void __init tnetd7300_init_clocks(void)
+{
+	u32 *bootcr = (u32 *)ioremap_nocache(AR7_REGS_DCL, 4);
+	struct tnetd7300_clocks *clocks =
+					(struct tnetd7300_clocks *)
+					ioremap_nocache(AR7_REGS_POWER + 0x20,
+					sizeof(struct tnetd7300_clocks));
+
+	ar7_bus_clock = tnetd7300_get_clock(BUS_PLL_SOURCE_SHIFT,
+		&clocks->bus, bootcr, AR7_AFE_CLOCK);
+
+	if (*bootcr & BOOT_PLL_ASYNC_MODE)
+		ar7_cpu_clock = tnetd7300_get_clock(CPU_PLL_SOURCE_SHIFT,
+			&clocks->cpu, bootcr, AR7_AFE_CLOCK);
+	else
+		ar7_cpu_clock = ar7_bus_clock;
+/*
+	tnetd7300_set_clock(USB_PLL_SOURCE_SHIFT, &clocks->usb,
+		bootcr, 48000000);
+*/
+	if (ar7_dsp_clock == 250000000)
+		tnetd7300_set_clock(DSP_PLL_SOURCE_SHIFT, &clocks->dsp,
+			bootcr, ar7_dsp_clock);
+
+	iounmap(clocks);
+	iounmap(bootcr);
+}
+
+static int tnetd7200_get_clock(int base, struct tnetd7200_clock *clock,
+	u32 *bootcr, u32 bus_clock)
+{
+	int divisor = ((readl(&clock->prediv) & 0x1f) + 1) *
+		((readl(&clock->postdiv) & 0x1f) + 1);
+
+	if (*bootcr & BOOT_PLL_BYPASS)
+		return base / divisor;
+
+	return base * ((readl(&clock->mul) & 0xf) + 1) / divisor;
+}
+
+
+static void tnetd7200_set_clock(int base, struct tnetd7200_clock *clock,
+	int prediv, int postdiv, int postdiv2, int mul, u32 frequency)
+{
+	printk(KERN_INFO
+		"Clocks: base = %d, frequency = %u, prediv = %d, "
+		"postdiv = %d, postdiv2 = %d, mul = %d\n",
+		base, frequency, prediv, postdiv, postdiv2, mul);
+
+	writel(0, &clock->ctrl);
+	writel(DIVISOR_ENABLE_MASK | ((prediv - 1) & 0x1F), &clock->prediv);
+	writel((mul - 1) & 0xF, &clock->mul);
+
+	for (mul = 0; mul < 2000; mul++) /* nop */;
+
+	while (readl(&clock->status) & 0x1) /* nop */;
+
+	writel(DIVISOR_ENABLE_MASK | ((postdiv - 1) & 0x1F), &clock->postdiv);
+
+	writel(readl(&clock->cmden) | 1, &clock->cmden);
+	writel(readl(&clock->cmd) | 1, &clock->cmd);
+
+	while (readl(&clock->status) & 0x1) /* nop */;
+
+	writel(DIVISOR_ENABLE_MASK | ((postdiv2 - 1) & 0x1F), &clock->postdiv2);
+
+	writel(readl(&clock->cmden) | 1, &clock->cmden);
+	writel(readl(&clock->cmd) | 1, &clock->cmd);
+
+	while (readl(&clock->status) & 0x1) /* nop */;
+
+	writel(readl(&clock->ctrl) | 1, &clock->ctrl);
+}
+
+static int tnetd7200_get_clock_base(int clock_id, u32 *bootcr)
+{
+	if (*bootcr & BOOT_PLL_ASYNC_MODE)
+		/* Async */
+		switch (clock_id) {
+		case TNETD7200_CLOCK_ID_DSP:
+			return AR7_REF_CLOCK;
+		default:
+			return AR7_AFE_CLOCK;
+		}
+	else
+		/* Sync */
+		if (*bootcr & BOOT_PLL_2TO1_MODE)
+			/* 2:1 */
+			switch (clock_id) {
+			case TNETD7200_CLOCK_ID_DSP:
+				return AR7_REF_CLOCK;
+			default:
+				return AR7_AFE_CLOCK;
+			}
+		else
+			/* 1:1 */
+			return AR7_REF_CLOCK;
+}
+
+
+static void __init tnetd7200_init_clocks(void)
+{
+	u32 *bootcr = (u32 *)ioremap_nocache(AR7_REGS_DCL, 4);
+	struct tnetd7200_clocks *clocks =
+					(struct tnetd7200_clocks *)
+					ioremap_nocache(AR7_REGS_POWER + 0x80,
+					sizeof(struct tnetd7200_clocks));
+	int cpu_base, cpu_mul, cpu_prediv, cpu_postdiv;
+	int dsp_base, dsp_mul, dsp_prediv, dsp_postdiv;
+	int usb_base, usb_mul, usb_prediv, usb_postdiv;
+
+/*
+	Log from Fritz!Box 7170 Annex B:
+
+	CPU revision is: 00018448
+	Clocks: Async mode
+	Clocks: Setting DSP clock
+	Clocks: prediv: 1, postdiv: 1, mul: 5
+	Clocks: base = 25000000, frequency = 125000000, prediv = 1,
+			postdiv = 2, postdiv2 = 1, mul = 10
+	Clocks: Setting CPU clock
+	Adjusted requested frequency 211000000 to 211968000
+	Clocks: prediv: 1, postdiv: 1, mul: 6
+	Clocks: base = 35328000, frequency = 211968000, prediv = 1,
+			postdiv = 1, postdiv2 = -1, mul = 6
+	Clocks: Setting USB clock
+	Adjusted requested frequency 48000000 to 48076920
+	Clocks: prediv: 13, postdiv: 1, mul: 5
+	Clocks: base = 125000000, frequency = 48000000, prediv = 13,
+			postdiv = 1, postdiv2 = -1, mul = 5
+
+	DSL didn't work if you didn't set the postdiv 2:1 postdiv2 combination,
+	driver hung on startup.
+	Haven't tested this on a synchronous board,
+	neither do i know what to do with ar7_dsp_clock
+*/
+
+	cpu_base = tnetd7200_get_clock_base(TNETD7200_CLOCK_ID_CPU, bootcr);
+	dsp_base = tnetd7200_get_clock_base(TNETD7200_CLOCK_ID_DSP, bootcr);
+
+	if (*bootcr & BOOT_PLL_ASYNC_MODE) {
+		printk(KERN_INFO "Clocks: Async mode\n");
+
+		printk(KERN_INFO "Clocks: Setting DSP clock\n");
+		calculate(dsp_base, TNETD7200_DEF_DSP_CLK,
+			&dsp_prediv, &dsp_postdiv, &dsp_mul);
+		ar7_bus_clock =
+			((dsp_base / dsp_prediv) * dsp_mul) / dsp_postdiv;
+		tnetd7200_set_clock(dsp_base, &clocks->dsp,
+			dsp_prediv, dsp_postdiv * 2, dsp_postdiv, dsp_mul * 2,
+			ar7_bus_clock);
+
+		printk(KERN_INFO "Clocks: Setting CPU clock\n");
+		calculate(cpu_base, TNETD7200_DEF_CPU_CLK, &cpu_prediv,
+			&cpu_postdiv, &cpu_mul);
+		ar7_cpu_clock =
+			((cpu_base / cpu_prediv) * cpu_mul) / cpu_postdiv;
+		tnetd7200_set_clock(cpu_base, &clocks->cpu,
+			cpu_prediv, cpu_postdiv, -1, cpu_mul,
+			ar7_cpu_clock);
+
+	} else
+		if (*bootcr & BOOT_PLL_2TO1_MODE) {
+			printk(KERN_INFO "Clocks: Sync 2:1 mode\n");
+
+			printk(KERN_INFO "Clocks: Setting CPU clock\n");
+			calculate(cpu_base, TNETD7200_DEF_CPU_CLK, &cpu_prediv,
+				&cpu_postdiv, &cpu_mul);
+			ar7_cpu_clock = ((cpu_base / cpu_prediv) * cpu_mul)
+								/ cpu_postdiv;
+			tnetd7200_set_clock(cpu_base, &clocks->cpu,
+				cpu_prediv, cpu_postdiv, -1, cpu_mul,
+				ar7_cpu_clock);
+
+			printk(KERN_INFO "Clocks: Setting DSP clock\n");
+			calculate(dsp_base, TNETD7200_DEF_DSP_CLK, &dsp_prediv,
+				&dsp_postdiv, &dsp_mul);
+			ar7_bus_clock = ar7_cpu_clock / 2;
+			tnetd7200_set_clock(dsp_base, &clocks->dsp,
+				dsp_prediv, dsp_postdiv * 2, dsp_postdiv,
+				dsp_mul * 2, ar7_bus_clock);
+		} else {
+			printk(KERN_INFO "Clocks: Sync 1:1 mode\n");
+
+			printk(KERN_INFO "Clocks: Setting DSP clock\n");
+			calculate(dsp_base, TNETD7200_DEF_DSP_CLK, &dsp_prediv,
+				&dsp_postdiv, &dsp_mul);
+			ar7_bus_clock = ((dsp_base / dsp_prediv) * dsp_mul)
+								/ dsp_postdiv;
+			tnetd7200_set_clock(dsp_base, &clocks->dsp,
+				dsp_prediv, dsp_postdiv * 2, dsp_postdiv,
+				dsp_mul * 2, ar7_bus_clock);
+
+			ar7_cpu_clock = ar7_bus_clock;
+		}
+
+	printk(KERN_INFO "Clocks: Setting USB clock\n");
+	usb_base = ar7_bus_clock;
+	calculate(usb_base, TNETD7200_DEF_USB_CLK, &usb_prediv,
+		&usb_postdiv, &usb_mul);
+	tnetd7200_set_clock(usb_base, &clocks->usb,
+		usb_prediv, usb_postdiv, -1, usb_mul,
+		TNETD7200_DEF_USB_CLK);
+
+	#warning FIXME
+	ar7_dsp_clock = ar7_cpu_clock;
+
+	iounmap(clocks);
+	iounmap(bootcr);
+}
+
+void __init ar7_init_clocks(void)
+{
+	switch (ar7_chip_id()) {
+	case AR7_CHIP_7100:
+#warning FIXME: Check if the new 7200 clock init works for 7100
+		tnetd7200_init_clocks();
+		break;
+	case AR7_CHIP_7200:
+		tnetd7200_init_clocks();
+		break;
+	case AR7_CHIP_7300:
+		ar7_dsp_clock = tnetd7300_dsp_clock();
+		tnetd7300_init_clocks();
+		break;
+	default:
+		break;
+	}
+}
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/gpio.c linux-2.6.30.5/arch/mips/ar7/gpio.c
--- linux-2.6.30.5.orig/arch/mips/ar7/gpio.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/gpio.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,49 @@
+/*
+ * Copyright (C) 2007 Felix Fietkau <nbd@openwrt.org>
+ * Copyright (C) 2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#include <linux/module.h>
+
+#include <asm/ar7/gpio.h>
+
+static const char *ar7_gpio_list[AR7_GPIO_MAX];
+
+int gpio_request(unsigned gpio, const char *label)
+{
+	if (gpio >= AR7_GPIO_MAX)
+		return -EINVAL;
+
+	if (ar7_gpio_list[gpio])
+		return -EBUSY;
+
+	if (label) {
+		ar7_gpio_list[gpio] = label;
+	} else {
+		ar7_gpio_list[gpio] = "busy";
+	}
+
+	return 0;
+}
+EXPORT_SYMBOL(gpio_request);
+
+void gpio_free(unsigned gpio)
+{
+	BUG_ON(!ar7_gpio_list[gpio]);
+	ar7_gpio_list[gpio] = NULL;
+}
+EXPORT_SYMBOL(gpio_free);
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/irq.c linux-2.6.30.5/arch/mips/ar7/irq.c
--- linux-2.6.30.5.orig/arch/mips/ar7/irq.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/irq.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,183 @@
+/*
+ * Copyright (C) 2006,2007 Felix Fietkau <nbd@openwrt.org>
+ * Copyright (C) 2006,2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#include <linux/interrupt.h>
+#include <linux/io.h>
+
+#include <asm/irq_cpu.h>
+#include <asm/mipsregs.h>
+#include <asm/ar7/ar7.h>
+
+#define EXCEPT_OFFSET	0x80
+#define PACE_OFFSET	0xA0
+#define CHNLS_OFFSET	0x200
+
+#define REG_OFFSET(irq, reg)	((irq) / 32 * 0x4 + reg * 0x10)
+#define SEC_REG_OFFSET(reg)	(EXCEPT_OFFSET + reg * 0x8)
+#define SEC_SR_OFFSET		(SEC_REG_OFFSET(0))	/* 0x80 */
+#define CR_OFFSET(irq)		(REG_OFFSET(irq, 1))	/* 0x10 */
+#define SEC_CR_OFFSET		(SEC_REG_OFFSET(1))	/* 0x88 */
+#define ESR_OFFSET(irq)		(REG_OFFSET(irq, 2))	/* 0x20 */
+#define SEC_ESR_OFFSET		(SEC_REG_OFFSET(2))	/* 0x90 */
+#define ECR_OFFSET(irq)		(REG_OFFSET(irq, 3))	/* 0x30 */
+#define SEC_ECR_OFFSET		(SEC_REG_OFFSET(3))	/* 0x98 */
+#define PIR_OFFSET		(0x40)
+#define MSR_OFFSET		(0x44)
+#define PM_OFFSET(irq)		(REG_OFFSET(irq, 5))	/* 0x50 */
+#define TM_OFFSET(irq)		(REG_OFFSET(irq, 6))	/* 0x60 */
+
+#define REG(addr) ((u32 *)(KSEG1ADDR(AR7_REGS_IRQ) + addr))
+
+#define CHNL_OFFSET(chnl) (CHNLS_OFFSET + (chnl * 4))
+
+static void ar7_unmask_irq(unsigned int irq_nr);
+static void ar7_mask_irq(unsigned int irq_nr);
+static void ar7_ack_irq(unsigned int irq_nr);
+static void ar7_unmask_sec_irq(unsigned int irq_nr);
+static void ar7_mask_sec_irq(unsigned int irq_nr);
+static void ar7_ack_sec_irq(unsigned int irq_nr);
+static void ar7_cascade(void);
+static void ar7_irq_init(int base);
+static int ar7_irq_base;
+
+static struct irq_chip ar7_irq_type = {
+	.name = "AR7",
+	.unmask = ar7_unmask_irq,
+	.mask = ar7_mask_irq,
+	.ack = ar7_ack_irq
+};
+
+static struct irq_chip ar7_sec_irq_type = {
+	.name = "AR7",
+	.unmask = ar7_unmask_sec_irq,
+	.mask = ar7_mask_sec_irq,
+	.ack = ar7_ack_sec_irq,
+};
+
+static struct irqaction ar7_cascade_action = {
+	.handler = no_action,
+	.name = "AR7 cascade interrupt"
+};
+
+static void ar7_unmask_irq(unsigned int irq)
+{
+	writel(1 << ((irq - ar7_irq_base) % 32),
+	       REG(ESR_OFFSET(irq - ar7_irq_base)));
+}
+
+static void ar7_mask_irq(unsigned int irq)
+{
+	writel(1 << ((irq - ar7_irq_base) % 32),
+	       REG(ECR_OFFSET(irq - ar7_irq_base)));
+}
+
+static void ar7_ack_irq(unsigned int irq)
+{
+	writel(1 << ((irq - ar7_irq_base) % 32),
+	       REG(CR_OFFSET(irq - ar7_irq_base)));
+}
+
+static void ar7_unmask_sec_irq(unsigned int irq)
+{
+	writel(1 << (irq - ar7_irq_base - 40), REG(SEC_ESR_OFFSET));
+}
+
+static void ar7_mask_sec_irq(unsigned int irq)
+{
+	writel(1 << (irq - ar7_irq_base - 40), REG(SEC_ECR_OFFSET));
+}
+
+static void ar7_ack_sec_irq(unsigned int irq)
+{
+	writel(1 << (irq - ar7_irq_base - 40), REG(SEC_CR_OFFSET));
+}
+
+void __init arch_init_irq(void) {
+	mips_cpu_irq_init();
+	ar7_irq_init(8);
+}
+
+static void __init ar7_irq_init(int base)
+{
+	int i;
+	/*
+	 * Disable interrupts and clear pending
+	 */
+	writel(0xffffffff, REG(ECR_OFFSET(0)));
+	writel(0xff, REG(ECR_OFFSET(32)));
+	writel(0xffffffff, REG(SEC_ECR_OFFSET));
+	writel(0xffffffff, REG(CR_OFFSET(0)));
+	writel(0xff, REG(CR_OFFSET(32)));
+	writel(0xffffffff, REG(SEC_CR_OFFSET));
+
+	ar7_irq_base = base;
+
+	for (i = 0; i < 40; i++) {
+		writel(i, REG(CHNL_OFFSET(i)));
+		/* Primary IRQ's */
+		set_irq_chip_and_handler(base + i, &ar7_irq_type,
+					 handle_level_irq);
+		/* Secondary IRQ's */
+		if (i < 32)
+			set_irq_chip_and_handler(base + i + 40,
+						 &ar7_sec_irq_type,
+						 handle_level_irq);
+	}
+
+	setup_irq(2, &ar7_cascade_action);
+	setup_irq(ar7_irq_base, &ar7_cascade_action);
+	set_c0_status(IE_IRQ0);
+}
+
+static void ar7_cascade(void)
+{
+	u32 status;
+	int i, irq;
+
+	/* Primary IRQ's */
+	irq = readl(REG(PIR_OFFSET)) & 0x3f;
+	if (irq) {
+		do_IRQ(ar7_irq_base + irq);
+		return;
+	}
+
+	/* Secondary IRQ's are cascaded through primary '0' */
+	writel(1, REG(CR_OFFSET(irq)));
+	status = readl(REG(SEC_SR_OFFSET));
+	for (i = 0; i < 32; i++) {
+		if (status & 1) {
+			do_IRQ(ar7_irq_base + i + 40);
+			return;
+		}
+		status >>= 1;
+	}
+
+	spurious_interrupt();
+}
+
+asmlinkage void plat_irq_dispatch(void)
+{
+	unsigned int pending = read_c0_status() & read_c0_cause() & ST0_IM;
+	if (pending & STATUSF_IP7)		/* cpu timer */
+		do_IRQ(7);
+	else if (pending & STATUSF_IP2)		/* int0 hardware line */
+		ar7_cascade();
+	else
+		spurious_interrupt();
+}
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/Makefile linux-2.6.30.5/arch/mips/ar7/Makefile
--- linux-2.6.30.5.orig/arch/mips/ar7/Makefile	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/Makefile	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,10 @@
+
+obj-y := \
+	prom.o \
+	setup.o \
+	memory.o \
+	irq.o \
+	time.o \
+	platform.o \
+	gpio.o \
+	clock.o
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/memory.c linux-2.6.30.5/arch/mips/ar7/memory.c
--- linux-2.6.30.5.orig/arch/mips/ar7/memory.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/memory.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,74 @@
+/*
+ * Based on arch/mips/mm/init.c
+ * Copyright (C) 1994 - 2000 Ralf Baechle
+ * Copyright (C) 1999, 2000 Silicon Graphics, Inc.
+ * Kevin D. Kissell, kevink@mips.com and Carsten Langgaard, carstenl@mips.com
+ * Copyright (C) 2000 MIPS Technologies, Inc.  All rights reserved.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+#include <linux/bootmem.h>
+#include <linux/init.h>
+#include <linux/mm.h>
+#include <linux/module.h>
+#include <linux/pfn.h>
+#include <linux/proc_fs.h>
+#include <linux/string.h>
+#include <linux/swap.h>
+
+#include <asm/bootinfo.h>
+#include <asm/page.h>
+#include <asm/sections.h>
+
+#include <asm/mips-boards/prom.h>
+
+static int __init memsize(void)
+{
+	u32 size = (64 << 20);
+	u32 *addr = (u32 *)KSEG1ADDR(0x14000000 + size - 4);
+	u32 *kernel_end = (u32 *)KSEG1ADDR(CPHYSADDR((u32)&_end));
+	u32 *tmpaddr = addr;
+
+	while (tmpaddr > kernel_end) {
+		*tmpaddr = (u32)tmpaddr;
+		size >>= 1;
+		tmpaddr -= size >> 2;
+	}
+
+	do {
+		tmpaddr += size >> 2;
+		if (*tmpaddr != (u32)tmpaddr)
+			break;
+		size <<= 1;
+	} while (size < (64 << 20));
+
+	writel(tmpaddr, &addr);
+
+	return size;
+}
+
+void __init prom_meminit(void)
+{
+	unsigned long pages;
+
+	pages = memsize() >> PAGE_SHIFT;
+	add_memory_region(PHYS_OFFSET, pages << PAGE_SHIFT,
+			  BOOT_MEM_RAM);
+}
+
+void __init prom_free_prom_memory(void)
+{
+	return;
+}
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/platform.c linux-2.6.30.5/arch/mips/ar7/platform.c
--- linux-2.6.30.5.orig/arch/mips/ar7/platform.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/platform.c	2009-08-26 20:06:50.000000000 +0200
@@ -0,0 +1,550 @@
+/*
+ * Copyright (C) 2006,2007 Felix Fietkau <nbd@openwrt.org>
+ * Copyright (C) 2006,2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#include <linux/autoconf.h>
+#include <linux/init.h>
+#include <linux/types.h>
+#include <linux/module.h>
+#include <linux/delay.h>
+#include <linux/dma-mapping.h>
+#include <linux/platform_device.h>
+#include <linux/mtd/physmap.h>
+#include <linux/serial.h>
+#include <linux/serial_8250.h>
+#include <linux/ioport.h>
+#include <linux/io.h>
+#include <linux/version.h>
+#include <linux/vlynq.h>
+#include <linux/leds.h>
+#include <linux/string.h>
+#include <linux/phy.h>
+#include <linux/phy_fixed.h>
+
+#include <asm/addrspace.h>
+#include <asm/ar7/ar7.h>
+#include <asm/ar7/gpio.h>
+#include <asm/ar7/prom.h>
+
+struct plat_vlynq_data {
+	struct plat_vlynq_ops ops;
+	int gpio_bit;
+	int reset_bit;
+};
+
+
+static int vlynq_on(struct vlynq_device *dev)
+{
+	int result;
+	struct plat_vlynq_data *pdata = dev->dev.platform_data;
+
+	if ((result = gpio_request(pdata->gpio_bit, "vlynq")))
+		goto out;
+
+	ar7_device_reset(pdata->reset_bit);
+
+	if ((result = ar7_gpio_disable(pdata->gpio_bit)))
+		goto out_enabled;
+
+	if ((result = ar7_gpio_enable(pdata->gpio_bit)))
+		goto out_enabled;
+
+	if ((result = gpio_direction_output(pdata->gpio_bit, 0)))
+		goto out_gpio_enabled;
+
+	mdelay(50);
+
+	gpio_set_value(pdata->gpio_bit, 1);
+	mdelay(50);
+
+	return 0;
+
+out_gpio_enabled:
+	ar7_gpio_disable(pdata->gpio_bit);
+out_enabled:
+	ar7_device_disable(pdata->reset_bit);
+	gpio_free(pdata->gpio_bit);
+out:
+	return result;
+}
+
+static void vlynq_off(struct vlynq_device *dev)
+{
+	struct plat_vlynq_data *pdata = dev->dev.platform_data;
+	ar7_gpio_disable(pdata->gpio_bit);
+	gpio_free(pdata->gpio_bit);
+	ar7_device_disable(pdata->reset_bit);
+}
+
+static struct resource physmap_flash_resource = {
+	.name = "mem",
+	.flags = IORESOURCE_MEM,
+	.start = 0x10000000,
+	.end = 0x107fffff,
+};
+
+static struct resource cpmac_low_res[] = {
+	{
+		.name = "regs",
+		.flags = IORESOURCE_MEM,
+		.start = AR7_REGS_MAC0,
+		.end = AR7_REGS_MAC0 + 0x7ff,
+	},
+	{
+		.name = "irq",
+		.flags = IORESOURCE_IRQ,
+		.start = 27,
+		.end = 27,
+	},
+};
+
+static struct resource cpmac_high_res[] = {
+	{
+		.name = "regs",
+		.flags = IORESOURCE_MEM,
+		.start = AR7_REGS_MAC1,
+		.end = AR7_REGS_MAC1 + 0x7ff,
+	},
+	{
+		.name = "irq",
+		.flags = IORESOURCE_IRQ,
+		.start = 41,
+		.end = 41,
+	},
+};
+
+static struct resource vlynq_low_res[] = {
+	{
+		.name = "regs",
+		.flags = IORESOURCE_MEM,
+		.start = AR7_REGS_VLYNQ0,
+		.end = AR7_REGS_VLYNQ0 + 0xff,
+	},
+	{
+		.name = "irq",
+		.flags = IORESOURCE_IRQ,
+		.start = 29,
+		.end = 29,
+	},
+	{
+		.name = "mem",
+		.flags = IORESOURCE_MEM,
+		.start = 0x04000000,
+		.end = 0x04ffffff,
+	},
+	{
+		.name = "devirq",
+		.flags = IORESOURCE_IRQ,
+		.start = 80,
+		.end = 111,
+	},
+};
+
+static struct resource vlynq_high_res[] = {
+	{
+		.name = "regs",
+		.flags = IORESOURCE_MEM,
+		.start = AR7_REGS_VLYNQ1,
+		.end = AR7_REGS_VLYNQ1 + 0xff,
+	},
+	{
+		.name = "irq",
+		.flags = IORESOURCE_IRQ,
+		.start = 33,
+		.end = 33,
+	},
+	{
+		.name = "mem",
+		.flags = IORESOURCE_MEM,
+		.start = 0x0c000000,
+		.end = 0x0cffffff,
+	},
+	{
+		.name = "devirq",
+		.flags = IORESOURCE_IRQ,
+		.start = 112,
+		.end = 143,
+	},
+};
+
+static struct resource usb_res[] = {
+	{
+		.name = "regs",
+		.flags = IORESOURCE_MEM,
+		.start = AR7_REGS_USB,
+		.end = AR7_REGS_USB + 0xff,
+	},
+	{
+		.name = "irq",
+		.flags = IORESOURCE_IRQ,
+		.start = 32,
+		.end = 32,
+	},
+	{
+		.name = "mem",
+		.flags = IORESOURCE_MEM,
+		.start = 0x03400000,
+		.end = 0x034001fff,
+	},
+};
+
+static struct physmap_flash_data physmap_flash_data = {
+	.width = 2,
+};
+
+/* lets assume this is suitable for both high and low cpmacs links */
+static struct fixed_phy_status fixed_phy_status __initdata = {
+	.link = 1,
+	.speed = 100,
+	.duplex = 1,
+};
+
+static struct plat_cpmac_data cpmac_low_data = {
+	.reset_bit = 17,
+	.power_bit = 20,
+	.phy_mask = 0x80000000,
+};
+
+static struct plat_cpmac_data cpmac_high_data = {
+	.reset_bit = 21,
+	.power_bit = 22,
+	.phy_mask = 0x7fffffff,
+};
+
+static struct plat_vlynq_data vlynq_low_data = {
+	.ops.on = vlynq_on,
+	.ops.off = vlynq_off,
+	.reset_bit = 20,
+	.gpio_bit = 18,
+};
+
+static struct plat_vlynq_data vlynq_high_data = {
+	.ops.on = vlynq_on,
+	.ops.off = vlynq_off,
+	.reset_bit = 16,
+	.gpio_bit = 19,
+};
+
+static struct platform_device physmap_flash = {
+	.id = 0,
+	.name = "physmap-flash",
+	.dev.platform_data = &physmap_flash_data,
+	.resource = &physmap_flash_resource,
+	.num_resources = 1,
+};
+
+static u64 cpmac_dma_mask = DMA_32BIT_MASK;
+static struct platform_device cpmac_low = {
+	.id = 0,
+	.name = "cpmac",
+	.dev = {
+		.dma_mask = &cpmac_dma_mask,
+		.coherent_dma_mask = DMA_32BIT_MASK,
+		.platform_data = &cpmac_low_data,
+	},
+	.resource = cpmac_low_res,
+	.num_resources = ARRAY_SIZE(cpmac_low_res),
+};
+
+static struct platform_device cpmac_high = {
+	.id = 1,
+	.name = "cpmac",
+	.dev = {
+		.dma_mask = &cpmac_dma_mask,
+		.coherent_dma_mask = DMA_32BIT_MASK,
+		.platform_data = &cpmac_high_data,
+	},
+	.resource = cpmac_high_res,
+	.num_resources = ARRAY_SIZE(cpmac_high_res),
+};
+
+static struct platform_device vlynq_low = {
+	.id = 0,
+	.name = "vlynq",
+	.dev.platform_data = &vlynq_low_data,
+	.resource = vlynq_low_res,
+	.num_resources = ARRAY_SIZE(vlynq_low_res),
+};
+
+static struct platform_device vlynq_high = {
+	.id = 1,
+	.name = "vlynq",
+	.dev.platform_data = &vlynq_high_data,
+	.resource = vlynq_high_res,
+	.num_resources = ARRAY_SIZE(vlynq_high_res),
+};
+
+
+/* This is proper way to define uart ports, but they are then detected
+ * as xscale and, obviously, don't work...
+ */
+#if !defined(CONFIG_SERIAL_8250)
+
+static struct plat_serial8250_port uart0_data = {
+	.mapbase = AR7_REGS_UART0,
+	.irq = AR7_IRQ_UART0,
+	.regshift = 2,
+	.iotype = UPIO_MEM,
+	.flags = UPF_BOOT_AUTOCONF | UPF_IOREMAP,
+};
+
+static struct plat_serial8250_port uart1_data = {
+	.mapbase = UR8_REGS_UART1,
+	.irq = AR7_IRQ_UART1,
+	.regshift = 2,
+	.iotype = UPIO_MEM,
+	.flags = UPF_BOOT_AUTOCONF | UPF_IOREMAP,
+};
+
+static struct plat_serial8250_port uart_data[] = {
+	uart0_data,
+	uart1_data,
+	{ .flags = 0 }
+};
+
+static struct plat_serial8250_port uart_data_single[] = {
+	uart0_data,
+	{ .flags = 0 }
+};
+
+static struct platform_device uart = {
+	.id = 0,
+	.name = "serial8250",
+	.dev.platform_data = uart_data_single
+};
+#endif
+
+static struct gpio_led default_leds[] = {
+	{ .name = "status", .gpio = 8, .active_low = 1, },
+};
+
+static struct gpio_led dsl502t_leds[] = {
+	{ .name = "status", .gpio = 9, .active_low = 1, },
+	{ .name = "ethernet", .gpio = 7, .active_low = 1, },
+	{ .name = "usb", .gpio = 12, .active_low = 1, },
+};
+
+static struct gpio_led dg834g_leds[] = {
+	{ .name = "ppp", .gpio = 6, .active_low = 1, },
+	{ .name = "status", .gpio = 7, .active_low = 1, },
+	{ .name = "adsl", .gpio = 8, .active_low = 1, },
+	{ .name = "wifi", .gpio = 12, .active_low = 1, },
+	{ .name = "power", .gpio = 14, .active_low = 1, .default_trigger = "default-on", },
+};
+
+static struct gpio_led fb_sl_leds[] = {
+	{ .name = "1", .gpio = 7, },
+	{ .name = "2", .gpio = 13, .active_low = 1, },
+	{ .name = "3", .gpio = 10, .active_low = 1, },
+	{ .name = "4", .gpio = 12, .active_low = 1, },
+	{ .name = "5", .gpio = 9, .active_low = 1, },
+};
+
+static struct gpio_led fb_fon_leds[] = {
+	{ .name = "1", .gpio = 8, },
+	{ .name = "2", .gpio = 3, .active_low = 1, },
+	{ .name = "3", .gpio = 5, },
+	{ .name = "4", .gpio = 4, .active_low = 1, },
+	{ .name = "5", .gpio = 11, .active_low = 1, },
+};
+
+static struct gpio_led_platform_data ar7_led_data;
+
+static struct platform_device ar7_gpio_leds = {
+	.name = "leds-gpio",
+	.id = -1,
+	.dev = {
+		.platform_data = &ar7_led_data,
+	}
+};
+
+static struct platform_device ar7_udc = {
+	.id = -1,
+	.name = "ar7_udc",
+	.resource = usb_res,
+	.num_resources = ARRAY_SIZE(usb_res),
+};
+
+static inline unsigned char char2hex(char h)
+{
+	switch (h) {
+	case '0': case '1': case '2': case '3': case '4':
+	case '5': case '6': case '7': case '8': case '9':
+		return h - '0';
+	case 'A': case 'B': case 'C': case 'D': case 'E': case 'F':
+		return h - 'A' + 10;
+	case 'a': case 'b': case 'c': case 'd': case 'e': case 'f':
+		return h - 'a' + 10;
+	default:
+		return 0;
+	}
+}
+
+static void cpmac_get_mac(int instance, unsigned char *dev_addr)
+{
+	int i;
+	char name[5], default_mac[] = "00:00:00:12:34:56", *mac;
+
+	mac = NULL;
+	sprintf(name, "mac%c", 'a' + instance);
+	mac = prom_getenv(name);
+	if (!mac) {
+		sprintf(name, "mac%c", 'a');
+		mac = prom_getenv(name);
+	}
+	if (!mac)
+		mac = default_mac;
+	for (i = 0; i < 6; i++)
+		dev_addr[i] = (char2hex(mac[i * 3]) << 4) +
+			char2hex(mac[i * 3 + 1]);
+}
+
+static void __init detect_leds(void)
+{
+	char *prId, *usb_prod;
+
+	/* Default LEDs	*/
+	ar7_led_data.num_leds = ARRAY_SIZE(default_leds);
+	ar7_led_data.leds = default_leds;
+
+	/* FIXME: the whole thing is unreliable */
+	prId = prom_getenv("ProductID");
+	usb_prod = prom_getenv("usb_prod");
+	
+	/* If we can't get the product id from PROM, use the default LEDs */
+	if (!prId)
+		return;
+
+	if (strstr(prId, "Fritz_Box_FON")) {
+		ar7_led_data.num_leds = ARRAY_SIZE(fb_fon_leds);
+		ar7_led_data.leds = fb_fon_leds;
+	} else if (strstr(prId, "Fritz_Box_")) {
+		ar7_led_data.num_leds = ARRAY_SIZE(fb_sl_leds);
+		ar7_led_data.leds = fb_sl_leds;
+	} else if ((!strcmp(prId, "AR7RD") || !strcmp(prId, "AR7DB")) && usb_prod != NULL && strstr(usb_prod, "DSL-502T")) {
+		ar7_led_data.num_leds = ARRAY_SIZE(dsl502t_leds);
+		ar7_led_data.leds = dsl502t_leds;
+	} else if (strstr(prId, "DG834")) {
+		ar7_led_data.num_leds = ARRAY_SIZE(dg834g_leds);
+		ar7_led_data.leds = dg834g_leds;
+	}
+}
+
+static int __init ar7_register_devices(void)
+{
+	int res;
+
+#ifdef CONFIG_SERIAL_8250
+
+	static struct uart_port uart_port[2];
+
+	memset(uart_port, 0, sizeof(struct uart_port) * 2);
+
+	uart_port[0].type = PORT_AR7;
+	uart_port[0].line = 0;
+	uart_port[0].irq = AR7_IRQ_UART0;
+	uart_port[0].uartclk = ar7_bus_freq() / 2;
+	uart_port[0].iotype = UPIO_MEM;
+	uart_port[0].mapbase = AR7_REGS_UART0;
+	uart_port[0].membase = ioremap(uart_port[0].mapbase, 256);
+	uart_port[0].regshift = 2;
+	res = early_serial_setup(&uart_port[0]);
+	if (res)
+		return res;
+
+
+	/* Only TNETD73xx have a second serial port */
+	if (ar7_has_second_uart()) {
+		uart_port[1].type = PORT_AR7;
+		uart_port[1].line = 1;
+		uart_port[1].irq = AR7_IRQ_UART1;
+		uart_port[1].uartclk = ar7_bus_freq() / 2;
+		uart_port[1].iotype = UPIO_MEM;
+		uart_port[1].mapbase = UR8_REGS_UART1;
+		uart_port[1].membase = ioremap(uart_port[1].mapbase, 256);
+		uart_port[1].regshift = 2;
+		res = early_serial_setup(&uart_port[1]);
+		if (res)
+			return res;
+	}
+
+#else /* !CONFIG_SERIAL_8250 */
+
+	uart_data[0].uartclk = ar7_bus_freq() / 2;
+	uart_data[1].uartclk = uart_data[0].uartclk;
+
+	/* Only TNETD73xx have a second serial port */
+	if (ar7_has_second_uart())
+		uart.dev.platform_data = uart_data;
+
+	res = platform_device_register(&uart);
+	if (res)
+		return res;
+
+#endif /* CONFIG_SERIAL_8250 */
+
+	res = platform_device_register(&physmap_flash);
+	if (res)
+		return res;
+
+	ar7_device_disable(vlynq_low_data.reset_bit);
+	res = platform_device_register(&vlynq_low);
+	if (res)
+		return res;
+
+	if (ar7_has_high_vlynq()) {
+		ar7_device_disable(vlynq_high_data.reset_bit);
+		res = platform_device_register(&vlynq_high);
+		if (res)
+			return res;
+	}
+
+	if (ar7_has_high_cpmac()) {
+		res = fixed_phy_add(PHY_POLL, cpmac_high.id, &fixed_phy_status);
+		if (res && res != -ENODEV)
+			return res;
+
+		cpmac_get_mac(1, cpmac_high_data.dev_addr);
+		res = platform_device_register(&cpmac_high);
+		if (res)
+			return res;
+	} else {
+		cpmac_low_data.phy_mask = 0xffffffff;
+	}
+
+	res = fixed_phy_add(PHY_POLL, cpmac_low.id, &fixed_phy_status);
+	if (res && res != -ENODEV)
+		return res;
+
+	cpmac_get_mac(0, cpmac_low_data.dev_addr);
+	res = platform_device_register(&cpmac_low);
+	if (res)
+		return res;
+
+	detect_leds();
+	res = platform_device_register(&ar7_gpio_leds);
+	if (res)
+		return res;
+
+	res = platform_device_register(&ar7_udc);
+
+	return res;
+}
+
+
+arch_initcall(ar7_register_devices);
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/prom.c linux-2.6.30.5/arch/mips/ar7/prom.c
--- linux-2.6.30.5.orig/arch/mips/ar7/prom.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/prom.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,321 @@
+/*
+ * Carsten Langgaard, carstenl@mips.com
+ * Copyright (C) 1999,2000 MIPS Technologies, Inc.  All rights reserved.
+ *
+ *  This program is free software; you can distribute it and/or modify it
+ *  under the terms of the GNU General Public License (Version 2) as
+ *  published by the Free Software Foundation.
+ *
+ *  This program is distributed in the hope it will be useful, but WITHOUT
+ *  ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
+ *  FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
+ *  for more details.
+ *
+ *  You should have received a copy of the GNU General Public License along
+ *  with this program; if not, write to the Free Software Foundation, Inc.,
+ *  59 Temple Place - Suite 330, Boston MA 02111-1307, USA.
+ *
+ * Putting things on the screen/serial line using YAMONs facilities.
+ */
+#include <linux/init.h>
+#include <linux/kernel.h>
+#include <linux/serial_reg.h>
+#include <linux/spinlock.h>
+#include <linux/module.h>
+#include <linux/string.h>
+#include <linux/io.h>
+#include <asm/bootinfo.h>
+
+#include <asm/ar7/ar7.h>
+#include <asm/ar7/prom.h>
+
+#define MAX_ENTRY 80
+
+struct env_var {
+	char *name;
+	char *value;
+};
+
+static struct env_var adam2_env[MAX_ENTRY] = { { 0, }, };
+
+char *prom_getenv(const char *name)
+{
+	int i;
+	for (i = 0; (i < MAX_ENTRY) && adam2_env[i].name; i++)
+		if (!strcmp(name, adam2_env[i].name))
+			return adam2_env[i].value;
+
+	return NULL;
+}
+EXPORT_SYMBOL(prom_getenv);
+
+char * __init prom_getcmdline(void)
+{
+	return &(arcs_cmdline[0]);
+}
+
+static void  __init ar7_init_cmdline(int argc, char *argv[])
+{
+	char *cp;
+	int actr;
+
+	actr = 1; /* Always ignore argv[0] */
+
+	cp = &(arcs_cmdline[0]);
+	while (actr < argc) {
+		strcpy(cp, argv[actr]);
+		cp += strlen(argv[actr]);
+		*cp++ = ' ';
+		actr++;
+	}
+	if (cp != &(arcs_cmdline[0])) {
+		/* get rid of trailing space */
+		--cp;
+		*cp = '\0';
+	}
+}
+
+struct psbl_rec {
+	u32 psbl_size;
+	u32 env_base;
+	u32 env_size;
+	u32 ffs_base;
+	u32 ffs_size;
+};
+
+static __initdata char psp_env_version[] = "TIENV0.8";
+
+struct psp_env_chunk {
+	u8 num;
+	u8 ctrl;
+	u16 csum;
+	u8 len;
+	char data[11];
+} __attribute__ ((packed));
+
+struct psp_var_map_entry {
+	u8 num;
+	char *value;
+};
+
+static struct psp_var_map_entry psp_var_map[] = {
+	{ 1, "cpufrequency" },
+	{ 2, "memsize" },
+	{ 3, "flashsize" },
+	{ 4, "modetty0" },
+	{ 5, "modetty1" },
+	{ 8, "maca" },
+	{ 9, "macb" },
+	{ 28, "sysfrequency" },
+	{ 38, "mipsfrequency" },
+};
+
+/*
+
+Well-known variable (num is looked up in table above for matching variable name)
+Example: cpufrequency=211968000
++----+----+----+----+----+----+----+----+----+----+----+----+----+----+----+---
+| 01 |CTRL|CHECKSUM | 01 | _2 | _1 | _1 | _9 | _6 | _8 | _0 | _0 | _0 | \0 | FF
++----+----+----+----+----+----+----+----+----+----+----+----+----+----+----+---
+
+Name=Value pair in a single chunk
+Example: NAME=VALUE
++----+----+----+----+----+----+----+----+----+----+----+----+----+----+----+---
+| 00 |CTRL|CHECKSUM | 01 | _N | _A | _M | _E | _0 | _V | _A | _L | _U | _E | \0
++----+----+----+----+----+----+----+----+----+----+----+----+----+----+----+---
+
+Name=Value pair in 2 chunks (len is the number of chunks)
+Example: bootloaderVersion=1.3.7.15
++----+----+----+----+----+----+----+----+----+----+----+----+----+----+----+---
+| 00 |CTRL|CHECKSUM | 02 | _b | _o | _o | _t | _l | _o | _a | _d | _e | _r | _V
++----+----+----+----+----+----+----+----+----+----+----+----+----+----+----+---
+| _e | _r | _s | _i | _o | _n | \0 | _1 | _. | _3 | _. | _7 | _. | _1 | _5 | \0
++----+----+----+----+----+----+----+----+----+----+----+----+----+----+----+---
+
+Data is padded with 0xFF
+
+*/
+
+#define PSP_ENV_SIZE  4096
+
+static char psp_env_data[PSP_ENV_SIZE] = { 0, };
+
+static char * __init lookup_psp_var_map(u8 num)
+{
+	int i;
+
+	for (i = 0; i < sizeof(psp_var_map); i++)
+		if (psp_var_map[i].num == num)
+			return psp_var_map[i].value;
+
+	return NULL;
+}
+
+static void __init add_adam2_var(char *name, char *value)
+{
+	int i;
+	for (i = 0; i < MAX_ENTRY; i++) {
+		if (!adam2_env[i].name) {
+			adam2_env[i].name = name;
+			adam2_env[i].value = value;
+			return;
+		} else if (!strcmp(adam2_env[i].name, name)) {
+			adam2_env[i].value = value;
+			return;
+		}
+	}
+}
+
+static int __init parse_psp_env(void *psp_env_base)
+{
+	int i, n;
+	char *name, *value;
+	struct psp_env_chunk *chunks = (struct psp_env_chunk *)psp_env_data;
+
+	memcpy_fromio(chunks, psp_env_base, PSP_ENV_SIZE);
+
+	i = 1;
+	n = PSP_ENV_SIZE / sizeof(struct psp_env_chunk);
+	while (i < n) {
+		if ((chunks[i].num == 0xff) || ((i + chunks[i].len) > n))
+			break;
+		value = chunks[i].data;
+		if (chunks[i].num) {
+			name = lookup_psp_var_map(chunks[i].num);
+		} else {
+			name = value;
+			value += strlen(name) + 1;
+		}
+		if (name)
+			add_adam2_var(name, value);
+		i += chunks[i].len;
+	}
+	return 0;
+}
+
+static void __init ar7_init_env(struct env_var *env)
+{
+	int i;
+	struct psbl_rec *psbl = (struct psbl_rec *)(KSEG1ADDR(0x14000300));
+	void *psp_env = (void *)KSEG1ADDR(psbl->env_base);
+
+	if (strcmp(psp_env, psp_env_version) == 0) {
+		parse_psp_env(psp_env);
+	} else {
+		for (i = 0; i < MAX_ENTRY; i++, env++)
+			if (env->name)
+				add_adam2_var(env->name, env->value);
+	}
+}
+
+static void __init console_config(void)
+{
+#ifdef CONFIG_SERIAL_8250_CONSOLE
+	char console_string[40];
+	int baud = 0;
+	char parity = '\0', bits = '\0', flow = '\0';
+	char *s, *p;
+
+	if (strstr(prom_getcmdline(), "console="))
+		return;
+
+#ifdef CONFIG_KGDB
+	if (!strstr(prom_getcmdline(), "nokgdb")) {
+		strcat(prom_getcmdline(), " console=kgdb");
+		kgdb_enabled = 1;
+		return;
+	}
+#endif
+
+	if ((s = prom_getenv("modetty0"))) {
+		baud = simple_strtoul(s, &p, 10);
+		s = p;
+		if (*s == ',') s++;
+		if (*s) parity = *s++;
+		if (*s == ',') s++;
+		if (*s) bits = *s++;
+		if (*s == ',') s++;
+		if (*s == 'h') flow = 'r';
+	}
+
+	if (baud == 0)
+		baud = 38400;
+	if (parity != 'n' && parity != 'o' && parity != 'e')
+		parity = 'n';
+	if (bits != '7' && bits != '8')
+		bits = '8';
+
+	if (flow == 'r')
+		sprintf(console_string, " console=ttyS0,%d%c%c%c", baud,
+			parity, bits, flow);
+        else
+		sprintf(console_string, " console=ttyS0,%d%c%c", baud, parity,
+			bits);
+	strcat(prom_getcmdline(), console_string);
+#endif
+}
+
+void __init prom_init(void)
+{
+	ar7_init_cmdline(fw_arg0, (char **)fw_arg1);
+	ar7_init_env((struct env_var *)fw_arg2);
+	console_config();
+}
+
+#define PORT(offset) (KSEG1ADDR(AR7_REGS_UART0 + (offset * 4)))
+static inline unsigned int serial_in(int offset)
+{
+	return readb((void *)PORT(offset));
+}
+
+static inline void serial_out(int offset, int value)
+{
+	writeb(value, (void *)PORT(offset));
+}
+
+char prom_getchar(void)
+{
+	while (!(serial_in(UART_LSR) & UART_LSR_DR));
+	return serial_in(UART_RX);
+}
+
+int prom_putchar(char c)
+{
+	while ((serial_in(UART_LSR) & UART_LSR_TEMT) == 0);
+	serial_out(UART_TX, c);
+	return 1;
+}
+
+/* from adm5120/prom.c */
+void prom_printf(const char *fmt, ...)
+{
+	va_list args;
+	int l;
+	char *p, *buf_end;
+	char buf[1024];
+
+	va_start(args, fmt);
+	l = vsprintf(buf, fmt, args); /* hopefully i < sizeof(buf) */
+	va_end(args);
+
+	buf_end = buf + l;
+
+	for (p = buf; p < buf_end; p++) {
+		/* Crude cr/nl handling is better than none */
+		if (*p == '\n')
+			prom_putchar('\r');
+		prom_putchar(*p);
+	}
+}
+
+#ifdef CONFIG_KGDB
+int putDebugChar(char c)
+{
+	return prom_putchar(c);
+}
+
+char getDebugChar(void)
+{
+       return prom_getchar();
+}
+#endif
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/setup.c linux-2.6.30.5/arch/mips/ar7/setup.c
--- linux-2.6.30.5.orig/arch/mips/ar7/setup.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/setup.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,105 @@
+/*
+ * Carsten Langgaard, carstenl@mips.com
+ * Copyright (C) 2000 MIPS Technologies, Inc.  All rights reserved.
+ *
+ *  This program is free software; you can distribute it and/or modify it
+ *  under the terms of the GNU General Public License (Version 2) as
+ *  published by the Free Software Foundation.
+ *
+ *  This program is distributed in the hope it will be useful, but WITHOUT
+ *  ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
+ *  FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
+ *  for more details.
+ *
+ *  You should have received a copy of the GNU General Public License along
+ *  with this program; if not, write to the Free Software Foundation, Inc.,
+ *  59 Temple Place - Suite 330, Boston MA 02111-1307, USA.
+ */
+#include <linux/version.h>
+#include <linux/init.h>
+#include <linux/ioport.h>
+#include <linux/pm.h>
+
+#include <asm/reboot.h>
+#include <asm/time.h>
+#include <asm/ar7/ar7.h>
+#include <asm/ar7/prom.h>
+
+static void ar7_machine_restart(char *command);
+static void ar7_machine_halt(void);
+static void ar7_machine_power_off(void);
+
+static void ar7_machine_restart(char *command)
+{
+	u32 *softres_reg = (u32 *)ioremap(AR7_REGS_RESET +
+					  AR7_RESET_SOFTWARE, 1);
+	writel(1, softres_reg);
+}
+
+static void ar7_machine_halt(void)
+{
+	while (1);
+}
+
+static void ar7_machine_power_off(void)
+{
+	u32 *power_reg = (u32 *)ioremap(AR7_REGS_POWER, 1);
+	u32 power_state = readl(power_reg) | (3 << 30);
+	writel(power_state, power_reg);
+	ar7_machine_halt();
+}
+
+const char *get_system_type(void)
+{
+	u16 chip_id = ar7_chip_id();
+	switch (chip_id) {
+	case AR7_CHIP_7300:
+		return "TI AR7 (TNETD7300)";
+	case AR7_CHIP_7100:
+		return "TI AR7 (TNETD7100)";
+	case AR7_CHIP_7200:
+		return "TI AR7 (TNETD7200)";
+	default:
+		return "TI AR7 (Unknown)";
+	}
+}
+
+static int __init ar7_init_console(void)
+{
+	return 0;
+}
+
+/*
+ * Initializes basic routines and structures pointers, memory size (as
+ * given by the bios and saves the command line.
+ */
+
+extern void ar7_init_clocks(void);
+
+void __init plat_mem_setup(void)
+{
+	unsigned long io_base;
+
+	_machine_restart = ar7_machine_restart;
+	_machine_halt = ar7_machine_halt;
+	pm_power_off = ar7_machine_power_off;
+	panic_timeout = 3;
+
+	io_base = (unsigned long)ioremap(AR7_REGS_BASE, 0x10000);
+	if (!io_base) panic("Can't remap IO base!\n");
+	set_io_port_base(io_base);
+
+	prom_meminit();
+	ar7_init_clocks();
+
+	ioport_resource.start = 0;
+	ioport_resource.end   = ~0;
+	iomem_resource.start  = 0;
+	iomem_resource.end    = ~0;
+
+	printk(KERN_INFO "%s, ID: 0x%04x, Revision: 0x%02x\n",
+					get_system_type(),
+		ar7_chip_id(), ar7_chip_rev());
+}
+
+console_initcall(ar7_init_console);
diff -Nur linux-2.6.30.5.orig/arch/mips/ar7/time.c linux-2.6.30.5/arch/mips/ar7/time.c
--- linux-2.6.30.5.orig/arch/mips/ar7/time.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/ar7/time.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,28 @@
+/*
+ * Carsten Langgaard, carstenl@mips.com
+ * Copyright (C) 1999,2000 MIPS Technologies, Inc.  All rights reserved.
+ *
+ *  This program is free software; you can distribute it and/or modify it
+ *  under the terms of the GNU General Public License (Version 2) as
+ *  published by the Free Software Foundation.
+ *
+ *  This program is distributed in the hope it will be useful, but WITHOUT
+ *  ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
+ *  FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
+ *  for more details.
+ *
+ *  You should have received a copy of the GNU General Public License along
+ *  with this program; if not, write to the Free Software Foundation, Inc.,
+ *  59 Temple Place - Suite 330, Boston MA 02111-1307, USA.
+ *
+ * Setting up the clock on the MIPS boards.
+ */
+
+#include <linux/version.h>
+#include <asm/time.h>
+#include <asm/ar7/ar7.h>
+
+void __init plat_time_init(void)
+{
+	mips_hpt_frequency = ar7_cpu_freq() / 2;
+}
diff -Nur linux-2.6.30.5.orig/arch/mips/include/asm/ar7/ar7.h linux-2.6.30.5/arch/mips/include/asm/ar7/ar7.h
--- linux-2.6.30.5.orig/arch/mips/include/asm/ar7/ar7.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/include/asm/ar7/ar7.h	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,170 @@
+/*
+ * Copyright (C) 2006,2007 Felix Fietkau <nbd@openwrt.org>
+ * Copyright (C) 2006,2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#ifndef __AR7_H__
+#define __AR7_H__
+
+#include <linux/delay.h>
+#include <asm/addrspace.h>
+#include <linux/io.h>
+
+#define AR7_REGS_BASE	0x08610000
+
+#define AR7_REGS_MAC0	(AR7_REGS_BASE + 0x0000)
+#define AR7_REGS_GPIO	(AR7_REGS_BASE + 0x0900)
+/* 0x08610A00 - 0x08610BFF (512 bytes, 128 bytes / clock) */
+#define AR7_REGS_POWER	(AR7_REGS_BASE + 0x0a00)
+#define AR7_REGS_UART0	(AR7_REGS_BASE + 0x0e00)
+#define AR7_REGS_USB	(AR7_REGS_BASE + 0x1200)
+#define AR7_REGS_RESET	(AR7_REGS_BASE + 0x1600)
+#define AR7_REGS_VLYNQ0	(AR7_REGS_BASE + 0x1800)
+#define AR7_REGS_DCL	(AR7_REGS_BASE + 0x1a00)
+#define AR7_REGS_VLYNQ1	(AR7_REGS_BASE + 0x1c00)
+#define AR7_REGS_MDIO	(AR7_REGS_BASE + 0x1e00)
+#define AR7_REGS_IRQ	(AR7_REGS_BASE + 0x2400)
+#define AR7_REGS_MAC1	(AR7_REGS_BASE + 0x2800)
+
+#define AR7_REGS_WDT	(AR7_REGS_BASE + 0x1f00)
+#define UR8_REGS_WDT	(AR7_REGS_BASE + 0x0b00)
+#define UR8_REGS_UART1	(AR7_REGS_BASE + 0x0f00)
+
+#define AR7_RESET_PEREPHERIAL	0x0
+#define AR7_RESET_SOFTWARE	0x4
+#define AR7_RESET_STATUS	0x8
+
+#define AR7_RESET_BIT_CPMAC_LO	17
+#define AR7_RESET_BIT_CPMAC_HI	21
+#define AR7_RESET_BIT_MDIO	22
+#define AR7_RESET_BIT_EPHY	26
+
+/* GPIO control registers */
+#define AR7_GPIO_INPUT	0x0
+#define AR7_GPIO_OUTPUT	0x4
+#define AR7_GPIO_DIR	0x8
+#define AR7_GPIO_ENABLE	0xc
+
+#define AR7_CHIP_7100	0x18
+#define AR7_CHIP_7200	0x2b
+#define AR7_CHIP_7300	0x05
+
+/* Interrupts */
+#define AR7_IRQ_UART0	15
+#define AR7_IRQ_UART1	16
+
+/* Clocks */
+#define AR7_AFE_CLOCK	35328000
+#define AR7_REF_CLOCK	25000000
+#define AR7_XTAL_CLOCK	24000000
+
+struct plat_cpmac_data {
+	int reset_bit;
+	int power_bit;
+	u32 phy_mask;
+	char dev_addr[6];
+};
+
+struct plat_dsl_data {
+	int reset_bit_dsl;
+	int reset_bit_sar;
+};
+
+extern int ar7_cpu_clock, ar7_bus_clock, ar7_dsp_clock;
+
+static inline u16 ar7_chip_id(void)
+{
+	return readl((void *)KSEG1ADDR(AR7_REGS_GPIO + 0x14)) & 0xffff;
+}
+
+static inline u8 ar7_chip_rev(void)
+{
+	return (readl((void *)KSEG1ADDR(AR7_REGS_GPIO + 0x14)) >> 16) & 0xff;
+}
+
+static inline int ar7_cpu_freq(void)
+{
+	return ar7_cpu_clock;
+}
+
+static inline int ar7_bus_freq(void)
+{
+	return ar7_bus_clock;
+}
+
+static inline int ar7_vbus_freq(void)
+{
+	return ar7_bus_clock / 2;
+}
+#define ar7_cpmac_freq ar7_vbus_freq
+
+static inline int ar7_dsp_freq(void)
+{
+	return ar7_dsp_clock;
+}
+
+static inline int ar7_has_high_cpmac(void)
+{
+	u16 chip_id = ar7_chip_id();
+	switch (chip_id) {
+	case AR7_CHIP_7100:
+	case AR7_CHIP_7200:
+		return 0;
+	default:
+		return 1;
+	}
+}
+#define ar7_has_high_vlynq ar7_has_high_cpmac
+#define ar7_has_second_uart ar7_has_high_cpmac
+
+static inline void ar7_device_enable(u32 bit)
+{
+	void *reset_reg =
+		(void *)KSEG1ADDR(AR7_REGS_RESET + AR7_RESET_PEREPHERIAL);
+	writel(readl(reset_reg) | (1 << bit), reset_reg);
+	mdelay(20);
+}
+
+static inline void ar7_device_disable(u32 bit)
+{
+	void *reset_reg =
+		(void *)KSEG1ADDR(AR7_REGS_RESET + AR7_RESET_PEREPHERIAL);
+	writel(readl(reset_reg) & ~(1 << bit), reset_reg);
+	mdelay(20);
+}
+
+static inline void ar7_device_reset(u32 bit)
+{
+	ar7_device_disable(bit);
+	ar7_device_enable(bit);
+}
+
+static inline void ar7_device_on(u32 bit)
+{
+	void *power_reg = (void *)KSEG1ADDR(AR7_REGS_POWER);
+	writel(readl(power_reg) | (1 << bit), power_reg);
+	mdelay(20);
+}
+
+static inline void ar7_device_off(u32 bit)
+{
+	void *power_reg = (void *)KSEG1ADDR(AR7_REGS_POWER);
+	writel(readl(power_reg) & ~(1 << bit), power_reg);
+	mdelay(20);
+}
+
+#endif /* __AR7_H__ */
diff -Nur linux-2.6.30.5.orig/arch/mips/include/asm/ar7/gpio.h linux-2.6.30.5/arch/mips/include/asm/ar7/gpio.h
--- linux-2.6.30.5.orig/arch/mips/include/asm/ar7/gpio.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/include/asm/ar7/gpio.h	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,109 @@
+/*
+ * Copyright (C) 2007 Florian Fainelli <florian@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#ifndef __AR7_GPIO_H__
+#define __AR7_GPIO_H__
+#include <asm/ar7/ar7.h>
+
+#define AR7_GPIO_MAX 32
+
+extern int gpio_request(unsigned gpio, const char *label);
+extern void gpio_free(unsigned gpio);
+
+/* Common GPIO layer */
+static inline int gpio_get_value(unsigned gpio)
+{
+	void __iomem *gpio_in =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_INPUT);
+
+	return readl(gpio_in) & (1 << gpio);
+}
+
+static inline void gpio_set_value(unsigned gpio, int value)
+{
+	void __iomem *gpio_out =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_OUTPUT);
+	unsigned tmp;
+
+	tmp = readl(gpio_out) & ~(1 << gpio);
+	if (value)
+		tmp |= 1 << gpio;
+	writel(tmp, gpio_out);
+}
+
+static inline int gpio_direction_input(unsigned gpio)
+{
+	void __iomem *gpio_dir =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_DIR);
+
+	if (gpio >= AR7_GPIO_MAX)
+		return -EINVAL;
+
+	writel(readl(gpio_dir) | (1 << gpio), gpio_dir);
+
+	return 0;
+}
+
+static inline int gpio_direction_output(unsigned gpio, int value)
+{
+	void __iomem *gpio_dir =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_DIR);
+
+	if (gpio >= AR7_GPIO_MAX)
+		return -EINVAL;
+
+	gpio_set_value(gpio, value);
+	writel(readl(gpio_dir) & ~(1 << gpio), gpio_dir);
+
+	return 0;
+}
+
+static inline int gpio_to_irq(unsigned gpio)
+{
+	return -EINVAL;
+}
+
+static inline int irq_to_gpio(unsigned irq)
+{
+	return -EINVAL;
+}
+
+/* Board specific GPIO functions */
+static inline int ar7_gpio_enable(unsigned gpio)
+{
+	void __iomem *gpio_en =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_ENABLE);
+
+	writel(readl(gpio_en) | (1 << gpio), gpio_en);
+
+	return 0;
+}
+
+static inline int ar7_gpio_disable(unsigned gpio)
+{
+	void __iomem *gpio_en =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_ENABLE);
+
+	writel(readl(gpio_en) & ~(1 << gpio), gpio_en);
+
+	return 0;
+}
+
+#include <asm-generic/gpio.h>
+
+#endif
diff -Nur linux-2.6.30.5.orig/arch/mips/include/asm/ar7/irq.h linux-2.6.30.5/arch/mips/include/asm/ar7/irq.h
--- linux-2.6.30.5.orig/arch/mips/include/asm/ar7/irq.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/include/asm/ar7/irq.h	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,16 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Shamelessly copied from asm-mips/mach-emma2rh/
+ * Copyright (C) 2003 by Ralf Baechle
+ */
+#ifndef __ASM_AR7_IRQ_H
+#define __ASM_AR7_IRQ_H
+
+#define NR_IRQS	256
+
+#include_next <irq.h>
+
+#endif /* __ASM_AR7_IRQ_H */
diff -Nur linux-2.6.30.5.orig/arch/mips/include/asm/ar7/prom.h linux-2.6.30.5/arch/mips/include/asm/ar7/prom.h
--- linux-2.6.30.5.orig/arch/mips/include/asm/ar7/prom.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/include/asm/ar7/prom.h	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,26 @@
+/*
+ * Copyright (C) 2006, 2007 Florian Fainelli <florian@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#ifndef __PROM_H__
+#define __PROM_H__
+
+extern char *prom_getenv(const char *name);
+extern void prom_printf(const char *fmt, ...) __attribute__((format(printf, 1, 2)));
+extern void prom_meminit(void);
+
+#endif /* __PROM_H__ */
diff -Nur linux-2.6.30.5.orig/arch/mips/include/asm/ar7/spaces.h linux-2.6.30.5/arch/mips/include/asm/ar7/spaces.h
--- linux-2.6.30.5.orig/arch/mips/include/asm/ar7/spaces.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/include/asm/ar7/spaces.h	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,32 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 1994 - 1999, 2000, 03, 04 Ralf Baechle
+ * Copyright (C) 2000, 2002  Maciej W. Rozycki
+ * Copyright (C) 1990, 1999, 2000 Silicon Graphics, Inc.
+ */
+#ifndef _ASM_AR7_SPACES_H
+#define _ASM_AR7_SPACES_H
+
+#define CAC_BASE		0x80000000
+#define IO_BASE			0xa0000000
+#define UNCAC_BASE		0xa0000000
+#define MAP_BASE		0xc0000000
+
+/*
+ * This handles the memory map.
+ * We handle pages at KSEG0 for kernels with 32 bit address space.
+ */
+#define PAGE_OFFSET		0x94000000UL
+#define PHYS_OFFSET		0x14000000UL
+
+/*
+ * Memory above this physical address will be considered highmem.
+ */
+#ifndef HIGHMEM_START
+#define HIGHMEM_START		0x40000000UL
+#endif
+
+#endif /* __ASM_AR7_SPACES_H */
diff -Nur linux-2.6.30.5.orig/arch/mips/include/asm/ar7/war.h linux-2.6.30.5/arch/mips/include/asm/ar7/war.h
--- linux-2.6.30.5.orig/arch/mips/include/asm/ar7/war.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/arch/mips/include/asm/ar7/war.h	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,25 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 2002, 2004, 2007 by Ralf Baechle <ralf@linux-mips.org>
+ */
+#ifndef __ASM_MIPS_MACH_BCM947XX_WAR_H
+#define __ASM_MIPS_MACH_BCM947XX_WAR_H
+
+#define R4600_V1_INDEX_ICACHEOP_WAR	0
+#define R4600_V1_HIT_CACHEOP_WAR	0
+#define R4600_V2_HIT_CACHEOP_WAR	0
+#define R5432_CP0_INTERRUPT_WAR		0
+#define BCM1250_M3_WAR			0
+#define SIBYTE_1956_WAR			0
+#define MIPS4K_ICACHE_REFILL_WAR	0
+#define MIPS_CACHE_SYNC_WAR		0
+#define TX49XX_ICACHE_INDEX_INV_WAR	0
+#define RM9000_CDEX_SMP_WAR		0
+#define ICACHE_REFILLS_WORKAROUND_WAR	0
+#define R10000_LLSC_WAR			0
+#define MIPS34K_MISSED_ITLB_WAR		0
+
+#endif /* __ASM_MIPS_MACH_BCM947XX_WAR_H */
diff -Nur linux-2.6.30.5.orig/arch/mips/include/asm/page.h linux-2.6.30.5/arch/mips/include/asm/page.h
--- linux-2.6.30.5.orig/arch/mips/include/asm/page.h	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/arch/mips/include/asm/page.h	2009-08-26 20:05:14.000000000 +0200
@@ -185,8 +185,10 @@
 #define VM_DATA_DEFAULT_FLAGS	(VM_READ | VM_WRITE | VM_EXEC | \
 				 VM_MAYREAD | VM_MAYWRITE | VM_MAYEXEC)
 
-#define UNCAC_ADDR(addr)	((addr) - PAGE_OFFSET + UNCAC_BASE)
-#define CAC_ADDR(addr)		((addr) - UNCAC_BASE + PAGE_OFFSET)
+#define UNCAC_ADDR(addr)	((addr) - PAGE_OFFSET + UNCAC_BASE +	\
+				 PHYS_OFFSET)
+#define CAC_ADDR(addr)		((addr) - UNCAC_BASE + PAGE_OFFSET -	\
+				 PHYS_OFFSET)
 
 #include <asm-generic/memory_model.h>
 #include <asm-generic/page.h>
diff -Nur linux-2.6.30.5.orig/arch/mips/Kconfig linux-2.6.30.5/arch/mips/Kconfig
--- linux-2.6.30.5.orig/arch/mips/Kconfig	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/arch/mips/Kconfig	2009-08-27 21:44:10.000000000 +0200
@@ -19,6 +19,23 @@
 	prompt "System type"
 	default SGI_IP22
 
+config AR7
+	bool "Texas Instruments AR7"
+	select BOOT_ELF32
+	select DMA_NONCOHERENT
+	select CEVT_R4K
+	select CSRC_R4K
+	select IRQ_CPU
+	select SWAP_IO_SPACE
+	select SYS_HAS_CPU_MIPS32_R1
+	select SYS_HAS_EARLY_PRINTK
+	select SYS_SUPPORTS_32BIT_KERNEL
+	select SYS_SUPPORTS_KGDB
+	select SYS_SUPPORTS_LITTLE_ENDIAN
+	select SYS_SUPPORTS_BIG_ENDIAN
+	select GENERIC_GPIO
+	select GENERIC_HARDIRQS_NO__DO_IRQ
+
 config MACH_ALCHEMY
 	bool "Alchemy processor based machines"
 
diff -Nur linux-2.6.30.5.orig/arch/mips/kernel/traps.c linux-2.6.30.5/arch/mips/kernel/traps.c
--- linux-2.6.30.5.orig/arch/mips/kernel/traps.c	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/arch/mips/kernel/traps.c	2009-08-26 20:05:14.000000000 +0200
@@ -1256,9 +1256,22 @@
 
 	exception_handlers[n] = handler;
 	if (n == 0 && cpu_has_divec) {
-		*(u32 *)(ebase + 0x200) = 0x08000000 |
-					  (0x03ffffff & (handler >> 2));
-		local_flush_icache_range(ebase + 0x200, ebase + 0x204);
+		if ((handler ^ (ebase + 4)) & 0xfc000000) {
+			/* lui k0, 0x0000 */
+			*(u32 *)(ebase + 0x200) = 0x3c1a0000 | (handler >> 16);
+			/* ori k0, 0x0000 */
+			*(u32 *)(ebase + 0x204) =
+					0x375a0000 | (handler & 0xffff);
+			/* jr k0 */
+			*(u32 *)(ebase + 0x208) = 0x03400008;
+			/* nop */
+			*(u32 *)(ebase + 0x20C) = 0x00000000;
+			flush_icache_range(ebase + 0x200, ebase + 0x210);
+		} else {
+			*(u32 *)(ebase + 0x200) =
+				0x08000000 | (0x03ffffff & (handler >> 2));
+			flush_icache_range(ebase + 0x200, ebase + 0x204);
+		}
 	}
 	return (void *)old_handler;
 }
diff -Nur linux-2.6.30.5.orig/arch/mips/Makefile linux-2.6.30.5/arch/mips/Makefile
--- linux-2.6.30.5.orig/arch/mips/Makefile	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/arch/mips/Makefile	2009-08-26 20:05:14.000000000 +0200
@@ -174,6 +174,13 @@
 #
 
 #
+# Texas Instruments AR7
+#
+core-$(CONFIG_AR7)		+= arch/mips/ar7/
+cflags-$(CONFIG_AR7)		+= -Iinclude/asm-mips/ar7
+load-$(CONFIG_AR7)		+= 0xffffffff94100000
+
+#
 # Acer PICA 61, Mips Magnum 4000 and Olivetti M700.
 #
 core-$(CONFIG_MACH_JAZZ)	+= arch/mips/jazz/
diff -Nur linux-2.6.30.5.orig/drivers/char/ar7_gpio.c linux-2.6.30.5/drivers/char/ar7_gpio.c
--- linux-2.6.30.5.orig/drivers/char/ar7_gpio.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/drivers/char/ar7_gpio.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,158 @@
+/*
+ * Copyright (C) 2007 Nicolas Thill <nico@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#include <linux/device.h>
+#include <linux/fs.h>
+#include <linux/module.h>
+#include <linux/errno.h>
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/uaccess.h>
+#include <linux/io.h>
+#include <linux/types.h>
+#include <linux/cdev.h>
+#include <gpio.h>
+
+#define DRVNAME "ar7_gpio"
+#define LONGNAME "TI AR7 GPIOs Driver"
+
+MODULE_AUTHOR("Nicolas Thill <nico@openwrt.org>");
+MODULE_DESCRIPTION(LONGNAME);
+MODULE_LICENSE("GPL");
+
+static int ar7_gpio_major;
+
+static ssize_t ar7_gpio_write(struct file *file, const char __user *buf,
+	size_t len, loff_t *ppos)
+{
+	int pin = iminor(file->f_dentry->d_inode);
+	size_t i;
+
+	for (i = 0; i < len; ++i) {
+		char c;
+		if (get_user(c, buf + i))
+			return -EFAULT;
+		switch (c) {
+		case '0':
+			gpio_set_value(pin, 0);
+			break;
+		case '1':
+			gpio_set_value(pin, 1);
+			break;
+		case 'd':
+		case 'D':
+			ar7_gpio_disable(pin);
+			break;
+		case 'e':
+		case 'E':
+			ar7_gpio_enable(pin);
+			break;
+		case 'i':
+		case 'I':
+		case '<':
+			gpio_direction_input(pin);
+			break;
+		case 'o':
+		case 'O':
+		case '>':
+			gpio_direction_output(pin, 0);
+			break;
+		default:
+			return -EINVAL;
+		}
+	}
+
+	return len;
+}
+
+static ssize_t ar7_gpio_read(struct file *file, char __user *buf,
+	size_t len, loff_t *ppos)
+{
+	int pin = iminor(file->f_dentry->d_inode);
+	int value;
+
+	value = gpio_get_value(pin);
+	if (put_user(value ? '1' : '0', buf))
+		return -EFAULT;
+
+	return 1;
+}
+
+static int ar7_gpio_open(struct inode *inode, struct file *file)
+{
+	int m = iminor(inode);
+
+	if (m >= AR7_GPIO_MAX)
+		return -EINVAL;
+
+	return nonseekable_open(inode, file);
+}
+
+static int ar7_gpio_release(struct inode *inode, struct file *file)
+{
+	return 0;
+}
+
+static const struct file_operations ar7_gpio_fops = {
+	.owner   = THIS_MODULE,
+	.write   = ar7_gpio_write,
+	.read    = ar7_gpio_read,
+	.open    = ar7_gpio_open,
+	.release = ar7_gpio_release,
+	.llseek  = no_llseek,
+};
+
+static struct platform_device *ar7_gpio_device;
+
+static int __init ar7_gpio_init(void)
+{
+	int rc;
+
+	ar7_gpio_device = platform_device_alloc(DRVNAME, -1);
+	if (!ar7_gpio_device)
+		return -ENOMEM;
+
+	rc = platform_device_add(ar7_gpio_device);
+	if (rc < 0)
+		goto out_put;
+
+	rc = register_chrdev(ar7_gpio_major, DRVNAME, &ar7_gpio_fops);
+	if (rc < 0)
+		goto out_put;
+
+	ar7_gpio_major = rc;
+
+	rc = 0;
+
+	goto out;
+
+out_put:
+	platform_device_put(ar7_gpio_device);
+out:
+	return rc;
+}
+
+static void __exit ar7_gpio_exit(void)
+{
+	unregister_chrdev(ar7_gpio_major, DRVNAME);
+	platform_device_unregister(ar7_gpio_device);
+}
+
+module_init(ar7_gpio_init);
+module_exit(ar7_gpio_exit);
diff -Nur linux-2.6.30.5.orig/drivers/char/Kconfig linux-2.6.30.5/drivers/char/Kconfig
--- linux-2.6.30.5.orig/drivers/char/Kconfig	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/char/Kconfig	2009-08-26 20:05:23.000000000 +0200
@@ -974,6 +974,15 @@
 	  To compile this driver as a module, choose M here: the
 	  module will be called mwave.
 
+config AR7_GPIO
+	tristate "TI AR7 GPIO Support"
+	depends on AR7
+	help
+	  Give userspace access to the GPIO pins on the Texas Instruments AR7 
+	  processors.
+
+	  If compiled as a module, it will be called ar7_gpio.
+
 config SCx200_GPIO
 	tristate "NatSemi SCx200 GPIO Support"
 	depends on SCx200
diff -Nur linux-2.6.30.5.orig/drivers/char/Makefile linux-2.6.30.5/drivers/char/Makefile
--- linux-2.6.30.5.orig/drivers/char/Makefile	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/char/Makefile	2009-08-26 20:05:23.000000000 +0200
@@ -90,6 +90,7 @@
 obj-$(CONFIG_PPDEV)		+= ppdev.o
 obj-$(CONFIG_NWBUTTON)		+= nwbutton.o
 obj-$(CONFIG_NWFLASH)		+= nwflash.o
+obj-$(CONFIG_AR7_GPIO)		+= ar7_gpio.o
 obj-$(CONFIG_SCx200_GPIO)	+= scx200_gpio.o
 obj-$(CONFIG_PC8736x_GPIO)	+= pc8736x_gpio.o
 obj-$(CONFIG_NSC_GPIO)		+= nsc_gpio.o
diff -Nur linux-2.6.30.5.orig/drivers/char/watchdog/ar7_wdt.c linux-2.6.30.5/drivers/char/watchdog/ar7_wdt.c
--- linux-2.6.30.5.orig/drivers/char/watchdog/ar7_wdt.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/drivers/char/watchdog/ar7_wdt.c	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,349 @@
+/*
+ * drivers/watchdog/ar7_wdt.c
+ *
+ * Copyright (C) 2007 Nicolas Thill <nico@openwrt.org>
+ * Copyright (c) 2005 Enrik Berkhan <Enrik.Berkhan@akk.org>
+ *
+ * Some code taken from:
+ * National Semiconductor SCx200 Watchdog support
+ * Copyright (c) 2001,2002 Christer Weinigel <wingel@nano-system.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/errno.h>
+#include <linux/init.h>
+#include <linux/miscdevice.h>
+#include <linux/watchdog.h>
+#include <linux/notifier.h>
+#include <linux/reboot.h>
+#include <linux/fs.h>
+#include <linux/ioport.h>
+#include <linux/io.h>
+#include <linux/uaccess.h>
+
+#include <asm/addrspace.h>
+#include <asm/ar7/ar7.h>
+
+#define DRVNAME "ar7_wdt"
+#define LONGNAME "TI AR7 Watchdog Timer"
+
+MODULE_AUTHOR("Nicolas Thill <nico@openwrt.org>");
+MODULE_DESCRIPTION(LONGNAME);
+MODULE_LICENSE("GPL");
+MODULE_ALIAS_MISCDEV(WATCHDOG_MINOR);
+
+static int margin = 60;
+module_param(margin, int, 0);
+MODULE_PARM_DESC(margin, "Watchdog margin in seconds");
+
+static int nowayout = WATCHDOG_NOWAYOUT;
+module_param(nowayout, int, 0);
+MODULE_PARM_DESC(nowayout, "Disable watchdog shutdown on close");
+
+#define READ_REG(x) readl((void __iomem *)&(x))
+#define WRITE_REG(x, v) writel((v), (void __iomem *)&(x))
+
+struct ar7_wdt {
+	u32 kick_lock;
+	u32 kick;
+	u32 change_lock;
+	u32 change;
+	u32 disable_lock;
+	u32 disable;
+	u32 prescale_lock;
+	u32 prescale;
+};
+
+static struct semaphore open_semaphore;
+static unsigned expect_close;
+
+/* XXX currently fixed, allows max margin ~68.72 secs */
+#define prescale_value 0xffff
+
+/* Offset of the WDT registers */
+static unsigned long ar7_regs_wdt;
+/* Pointer to the remapped WDT IO space */
+static struct ar7_wdt *ar7_wdt;
+static void ar7_wdt_get_regs(void)
+{
+	u16 chip_id = ar7_chip_id();
+	switch (chip_id) {
+	case AR7_CHIP_7100:
+	case AR7_CHIP_7200:
+		ar7_regs_wdt = AR7_REGS_WDT;
+		break;
+	default:
+		ar7_regs_wdt = UR8_REGS_WDT;
+		break;
+	}
+}
+
+
+static void ar7_wdt_kick(u32 value)
+{
+	WRITE_REG(ar7_wdt->kick_lock, 0x5555);
+	if ((READ_REG(ar7_wdt->kick_lock) & 3) == 1) {
+		WRITE_REG(ar7_wdt->kick_lock, 0xaaaa);
+		if ((READ_REG(ar7_wdt->kick_lock) & 3) == 3) {
+			WRITE_REG(ar7_wdt->kick, value);
+			return;
+		}
+	}
+	printk(KERN_ERR DRVNAME ": failed to unlock WDT kick reg\n");
+}
+
+static void ar7_wdt_prescale(u32 value)
+{
+	WRITE_REG(ar7_wdt->prescale_lock, 0x5a5a);
+	if ((READ_REG(ar7_wdt->prescale_lock) & 3) == 1) {
+		WRITE_REG(ar7_wdt->prescale_lock, 0xa5a5);
+		if ((READ_REG(ar7_wdt->prescale_lock) & 3) == 3) {
+			WRITE_REG(ar7_wdt->prescale, value);
+			return;
+		}
+	}
+	printk(KERN_ERR DRVNAME ": failed to unlock WDT prescale reg\n");
+}
+
+static void ar7_wdt_change(u32 value)
+{
+	WRITE_REG(ar7_wdt->change_lock, 0x6666);
+	if ((READ_REG(ar7_wdt->change_lock) & 3) == 1) {
+		WRITE_REG(ar7_wdt->change_lock, 0xbbbb);
+		if ((READ_REG(ar7_wdt->change_lock) & 3) == 3) {
+			WRITE_REG(ar7_wdt->change, value);
+			return;
+		}
+	}
+	printk(KERN_ERR DRVNAME ": failed to unlock WDT change reg\n");
+}
+
+static void ar7_wdt_disable(u32 value)
+{
+	WRITE_REG(ar7_wdt->disable_lock, 0x7777);
+	if ((READ_REG(ar7_wdt->disable_lock) & 3) == 1) {
+		WRITE_REG(ar7_wdt->disable_lock, 0xcccc);
+		if ((READ_REG(ar7_wdt->disable_lock) & 3) == 2) {
+			WRITE_REG(ar7_wdt->disable_lock, 0xdddd);
+			if ((READ_REG(ar7_wdt->disable_lock) & 3) == 3) {
+				WRITE_REG(ar7_wdt->disable, value);
+				return;
+			}
+		}
+	}
+	printk(KERN_ERR DRVNAME ": failed to unlock WDT disable reg\n");
+}
+
+static void ar7_wdt_update_margin(int new_margin)
+{
+	u32 change;
+
+	change = new_margin * (ar7_vbus_freq() / prescale_value);
+	if (change < 1) change = 1;
+	if (change > 0xffff) change = 0xffff;
+	ar7_wdt_change(change);
+	margin = change * prescale_value / ar7_vbus_freq();
+	printk(KERN_INFO DRVNAME
+	       ": timer margin %d seconds (prescale %d, change %d, freq %d)\n",
+	       margin, prescale_value, change, ar7_vbus_freq());
+}
+
+static void ar7_wdt_enable_wdt(void)
+{
+	printk(KERN_DEBUG DRVNAME ": enabling watchdog timer\n");
+	ar7_wdt_disable(1);
+	ar7_wdt_kick(1);
+}
+
+static void ar7_wdt_disable_wdt(void)
+{
+	printk(KERN_DEBUG DRVNAME ": disabling watchdog timer\n");
+	ar7_wdt_disable(0);
+}
+
+static int ar7_wdt_open(struct inode *inode, struct file *file)
+{
+	/* only allow one at a time */
+	if (down_trylock(&open_semaphore))
+		return -EBUSY;
+	ar7_wdt_enable_wdt();
+	expect_close = 0;
+
+	return nonseekable_open(inode, file);
+}
+
+static int ar7_wdt_release(struct inode *inode, struct file *file)
+{
+	if (!expect_close)
+		printk(KERN_WARNING DRVNAME
+		": watchdog device closed unexpectedly,"
+		"will not disable the watchdog timer\n");
+	else if (!nowayout)
+		ar7_wdt_disable_wdt();
+
+	up(&open_semaphore);
+
+	return 0;
+}
+
+static int ar7_wdt_notify_sys(struct notifier_block *this,
+			      unsigned long code, void *unused)
+{
+	if (code == SYS_HALT || code == SYS_POWER_OFF)
+		if (!nowayout)
+			ar7_wdt_disable_wdt();
+
+	return NOTIFY_DONE;
+}
+
+static struct notifier_block ar7_wdt_notifier = {
+	.notifier_call = ar7_wdt_notify_sys
+};
+
+static ssize_t ar7_wdt_write(struct file *file, const char *data,
+			     size_t len, loff_t *ppos)
+{
+	/* check for a magic close character */
+	if (len) {
+		size_t i;
+
+		ar7_wdt_kick(1);
+
+		expect_close = 0;
+		for (i = 0; i < len; ++i) {
+			char c;
+			if (get_user(c, data+i))
+				return -EFAULT;
+			if (c == 'V')
+				expect_close = 1;
+		}
+
+	}
+	return len;
+}
+
+static int ar7_wdt_ioctl(struct inode *inode, struct file *file,
+			 unsigned int cmd, unsigned long arg)
+{
+	static struct watchdog_info ident = {
+		.identity = LONGNAME,
+		.firmware_version = 1,
+		.options = (WDIOF_SETTIMEOUT | WDIOF_MAGICCLOSE | WDIOF_KEEPALIVEPING),
+	};
+	int new_margin;
+
+	switch (cmd) {
+	default:
+		return -ENOTTY;
+	case WDIOC_GETSUPPORT:
+		if (copy_to_user((struct watchdog_info *)arg, &ident,
+				sizeof(ident)))
+			return -EFAULT;
+		return 0;
+	case WDIOC_GETSTATUS:
+	case WDIOC_GETBOOTSTATUS:
+		if (put_user(0, (int *)arg))
+			return -EFAULT;
+		return 0;
+	case WDIOC_KEEPALIVE:
+		ar7_wdt_kick(1);
+		return 0;
+	case WDIOC_SETTIMEOUT:
+		if (get_user(new_margin, (int *)arg))
+			return -EFAULT;
+		if (new_margin < 1)
+			return -EINVAL;
+
+		ar7_wdt_update_margin(new_margin);
+		ar7_wdt_kick(1);
+
+	case WDIOC_GETTIMEOUT:
+		if (put_user(margin, (int *)arg))
+			return -EFAULT;
+		return 0;
+	}
+}
+
+static struct file_operations ar7_wdt_fops = {
+	.owner		= THIS_MODULE,
+	.write		= ar7_wdt_write,
+	.ioctl		= ar7_wdt_ioctl,
+	.open		= ar7_wdt_open,
+	.release	= ar7_wdt_release,
+};
+
+static struct miscdevice ar7_wdt_miscdev = {
+	.minor		= WATCHDOG_MINOR,
+	.name		= "watchdog",
+	.fops		= &ar7_wdt_fops,
+};
+
+static int __init ar7_wdt_init(void)
+{
+	int rc;
+
+	ar7_wdt_get_regs();
+
+	if (!request_mem_region(ar7_regs_wdt, sizeof(struct ar7_wdt),
+							LONGNAME)) {
+		printk(KERN_WARNING DRVNAME ": watchdog I/O region busy\n");
+		return -EBUSY;
+	}
+
+	ar7_wdt = (struct ar7_wdt *)
+			ioremap(ar7_regs_wdt, sizeof(struct ar7_wdt));
+
+	ar7_wdt_disable_wdt();
+	ar7_wdt_prescale(prescale_value);
+	ar7_wdt_update_margin(margin);
+
+	sema_init(&open_semaphore, 1);
+
+	rc = register_reboot_notifier(&ar7_wdt_notifier);
+	if (rc) {
+		printk(KERN_ERR DRVNAME
+			": unable to register reboot notifier\n");
+		goto out_alloc;
+	}
+
+	rc = misc_register(&ar7_wdt_miscdev);
+	if (rc) {
+		printk(KERN_ERR DRVNAME ": unable to register misc device\n");
+		goto out_register;
+	}
+	goto out;
+
+out_register:
+	unregister_reboot_notifier(&ar7_wdt_notifier);
+out_alloc:
+	iounmap(ar7_wdt);
+	release_mem_region(ar7_regs_wdt, sizeof(struct ar7_wdt));
+out:
+	return rc;
+}
+
+static void __exit ar7_wdt_cleanup(void)
+{
+	misc_deregister(&ar7_wdt_miscdev);
+	unregister_reboot_notifier(&ar7_wdt_notifier);
+	iounmap(ar7_wdt);
+	release_mem_region(ar7_regs_wdt, sizeof(struct ar7_wdt));
+}
+
+module_init(ar7_wdt_init);
+module_exit(ar7_wdt_cleanup);
diff -Nur linux-2.6.30.5.orig/drivers/Kconfig linux-2.6.30.5/drivers/Kconfig
--- linux-2.6.30.5.orig/drivers/Kconfig	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/Kconfig	2009-08-26 20:05:30.000000000 +0200
@@ -104,6 +104,8 @@
 
 source "drivers/uio/Kconfig"
 
+source "drivers/vlynq/Kconfig"
+
 source "drivers/xen/Kconfig"
 
 source "drivers/staging/Kconfig"
diff -Nur linux-2.6.30.5.orig/drivers/Makefile linux-2.6.30.5/drivers/Makefile
--- linux-2.6.30.5.orig/drivers/Makefile	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/Makefile	2009-08-26 20:05:30.000000000 +0200
@@ -103,6 +103,7 @@
 obj-$(CONFIG_HID)		+= hid/
 obj-$(CONFIG_PPC_PS3)		+= ps3/
 obj-$(CONFIG_OF)		+= of/
+obj-$(CONFIG_VLYNQ)		+= vlynq/
 obj-$(CONFIG_SSB)		+= ssb/
 obj-$(CONFIG_VIRTIO)		+= virtio/
 obj-$(CONFIG_STAGING)		+= staging/
diff -Nur linux-2.6.30.5.orig/drivers/mtd/maps/physmap.c linux-2.6.30.5/drivers/mtd/maps/physmap.c
--- linux-2.6.30.5.orig/drivers/mtd/maps/physmap.c	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/mtd/maps/physmap.c	2009-08-26 20:05:19.000000000 +0200
@@ -80,7 +80,7 @@
 					"map_rom",
 					NULL };
 #ifdef CONFIG_MTD_PARTITIONS
-static const char *part_probe_types[] = { "cmdlinepart", "RedBoot", NULL };
+static const char *part_probe_types[] = { "cmdlinepart", "RedBoot", "ar7part", NULL };
 #endif
 
 static int physmap_flash_probe(struct platform_device *dev)
diff -Nur linux-2.6.30.5.orig/drivers/net/cpmac.c linux-2.6.30.5/drivers/net/cpmac.c
--- linux-2.6.30.5.orig/drivers/net/cpmac.c	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/net/cpmac.c	2009-08-26 22:00:29.000000000 +0200
@@ -615,13 +615,13 @@
 
 		dev_kfree_skb_irq(desc->skb);
 		desc->skb = NULL;
-		if (netif_subqueue_stopped(dev, queue))
+		if (__netif_subqueue_stopped(dev, queue))
 			netif_wake_subqueue(dev, queue);
 	} else {
 		if (netif_msg_tx_err(priv) && net_ratelimit())
 			printk(KERN_WARNING
 			       "%s: end_xmit: spurious interrupt\n", dev->name);
-		if (netif_subqueue_stopped(dev, queue))
+		if (__netif_subqueue_stopped(dev, queue))
 			netif_wake_subqueue(dev, queue);
 	}
 }
@@ -731,7 +731,6 @@
 
 static void cpmac_hw_error(struct work_struct *work)
 {
-	int i;
 	struct cpmac_priv *priv =
 		container_of(work, struct cpmac_priv, reset_work);
 
@@ -818,7 +817,6 @@
 
 static void cpmac_tx_timeout(struct net_device *dev)
 {
-	int i;
 	struct cpmac_priv *priv = netdev_priv(dev);
 
 	spin_lock(&priv->lock);
@@ -1097,15 +1095,18 @@
 
 static int __devinit cpmac_probe(struct platform_device *pdev)
 {
-	int rc, phy_id, i;
-	char *mdio_bus_id = "0";
+	int rc, phy_id;
+	char mdio_bus_id[BUS_ID_SIZE];
 	struct resource *mem;
 	struct cpmac_priv *priv;
 	struct net_device *dev;
 	struct plat_cpmac_data *pdata;
 
 	pdata = pdev->dev.platform_data;
+	strncpy(mdio_bus_id, "0", BUS_ID_SIZE);
+	phy_id = pdev->id;
 
+	/*
 	for (phy_id = 0; phy_id < PHY_MAX_ADDR; phy_id++) {
 		if (!(pdata->phy_mask & (1 << phy_id)))
 			continue;
@@ -1116,15 +1117,17 @@
 
 	if (phy_id == PHY_MAX_ADDR) {
 		if (external_switch || dumb_switch) {
-			mdio_bus_id = 0; /* fixed phys bus */
+			strncpy(mdio_bus_id, "0", BUS_ID_SIZE);
 			phy_id = pdev->id;
 		} else {
 			dev_err(&pdev->dev, "no PHY present\n");
 			return -ENODEV;
 		}
 	}
+	*/
 
 	dev = alloc_etherdev_mq(sizeof(*priv), CPMAC_QUEUES);
+	//~ dev = alloc_etherdev(sizeof(*priv));
 
 	if (!dev) {
 		printk(KERN_ERR "cpmac: Unable to allocate net_device\n");
@@ -1161,8 +1164,11 @@
 	priv->msg_enable = netif_msg_init(debug_level, 0xff);
 	memcpy(dev->dev_addr, pdata->dev_addr, sizeof(dev->dev_addr));
 
-	priv->phy = phy_connect(dev, dev_name(&cpmac_mii->phy_map[phy_id]->dev),
+ 	snprintf(priv->phy_name, BUS_ID_SIZE, PHY_ID_FMT, mdio_bus_id, phy_id);
+	//priv->phy = phy_connect(dev, dev_name(&cpmac_mii->phy_map[phy_id]->dev),
+ 	priv->phy = phy_connect(dev, priv->phy_name,
 				&cpmac_adjust_link, 0, PHY_INTERFACE_MODE_MII);
+
 	if (IS_ERR(priv->phy)) {
 		if (netif_msg_drv(priv))
 			printk(KERN_ERR "%s: Could not attach to PHY\n",
@@ -1249,7 +1255,7 @@
 	}
 
 	cpmac_mii->phy_mask = ~(mask | 0x80000000);
-	snprintf(cpmac_mii->id, MII_BUS_ID_SIZE, "0");
+	snprintf(cpmac_mii->id, MII_BUS_ID_SIZE, "1");
 
 	res = mdiobus_register(cpmac_mii);
 	if (res)
diff -Nur linux-2.6.30.5.orig/drivers/net/Kconfig linux-2.6.30.5/drivers/net/Kconfig
--- linux-2.6.30.5.orig/drivers/net/Kconfig	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/net/Kconfig	2009-08-26 20:06:44.000000000 +0200
@@ -1760,7 +1760,7 @@
 
 config CPMAC
 	tristate "TI AR7 CPMAC Ethernet support (EXPERIMENTAL)"
-	depends on NET_ETHERNET && EXPERIMENTAL && AR7 && BROKEN
+	depends on NET_ETHERNET && EXPERIMENTAL && AR7
 	select PHYLIB
 	help
 	  TI AR7 CPMAC Ethernet support
diff -Nur linux-2.6.30.5.orig/drivers/serial/8250.c linux-2.6.30.5/drivers/serial/8250.c
--- linux-2.6.30.5.orig/drivers/serial/8250.c	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/serial/8250.c	2009-08-26 20:06:59.000000000 +0200
@@ -287,6 +287,13 @@
 		.fcr		= UART_FCR_ENABLE_FIFO | UART_FCR_R_TRIG_10,
 		.flags		= UART_CAP_FIFO,
 	},
+	[PORT_AR7] = {
+		.name		= "TI-AR7",
+		.fifo_size	= 16,
+		.tx_loadsz	= 16,
+		.fcr		= UART_FCR_ENABLE_FIFO | UART_FCR_R_TRIG_00,
+		.flags		= UART_CAP_FIFO | UART_CAP_AFE,
+	},
 };
 
 #if defined (CONFIG_SERIAL_8250_AU1X00)
@@ -2702,7 +2709,11 @@
 {
 	struct uart_8250_port *up = (struct uart_8250_port *)port;
 
+#ifdef CONFIG_AR7
+	wait_for_xmitr(up, BOTH_EMPTY);
+#else
 	wait_for_xmitr(up, UART_LSR_THRE);
+#endif
 	serial_out(up, UART_TX, ch);
 }
 
diff -Nur linux-2.6.30.5.orig/drivers/vlynq/Kconfig linux-2.6.30.5/drivers/vlynq/Kconfig
--- linux-2.6.30.5.orig/drivers/vlynq/Kconfig	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/drivers/vlynq/Kconfig	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,13 @@
+menu "TI VLYNQ"
+
+config VLYNQ
+	bool "TI VLYNQ bus support"
+	depends on AR7 && EXPERIMENTAL
+	help
+	  Support for the TI VLYNQ bus
+
+	  The module will be called vlynq
+
+	  If unsure, say N
+
+endmenu
diff -Nur linux-2.6.30.5.orig/drivers/vlynq/Makefile linux-2.6.30.5/drivers/vlynq/Makefile
--- linux-2.6.30.5.orig/drivers/vlynq/Makefile	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/drivers/vlynq/Makefile	2009-08-26 20:05:03.000000000 +0200
@@ -0,0 +1,5 @@
+#
+# Makefile for kernel vlynq drivers
+#
+
+obj-$(CONFIG_VLYNQ) += vlynq.o
diff -Nur linux-2.6.30.5.orig/drivers/vlynq/vlynq.c linux-2.6.30.5/drivers/vlynq/vlynq.c
--- linux-2.6.30.5.orig/drivers/vlynq/vlynq.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/drivers/vlynq/vlynq.c	2009-08-26 20:06:33.000000000 +0200
@@ -0,0 +1,813 @@
+/*
+ * Copyright (C) 2006, 2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ *
+ * Parts of the VLYNQ specification can be found here:
+ * http://www.ti.com/litv/pdf/sprue36a
+ */
+
+#include <linux/init.h>
+#include <linux/types.h>
+#include <linux/kernel.h>
+#include <linux/string.h>
+#include <linux/device.h>
+#include <linux/module.h>
+#include <linux/errno.h>
+#include <linux/platform_device.h>
+#include <linux/interrupt.h>
+#include <linux/delay.h>
+#include <linux/io.h>
+
+#include <linux/vlynq.h>
+
+#define VLYNQ_CTRL_PM_ENABLE		0x80000000
+#define VLYNQ_CTRL_CLOCK_INT		0x00008000
+#define VLYNQ_CTRL_CLOCK_DIV(x)		(((x) & 7) << 16)
+#define VLYNQ_CTRL_INT_LOCAL		0x00004000
+#define VLYNQ_CTRL_INT_ENABLE		0x00002000
+#define VLYNQ_CTRL_INT_VECTOR(x)	(((x) & 0x1f) << 8)
+#define VLYNQ_CTRL_INT2CFG		0x00000080
+#define VLYNQ_CTRL_RESET		0x00000001
+
+#define VLYNQ_CTRL_CLOCK_MASK          (0x7 << 16)
+
+#define VLYNQ_INT_OFFSET		0x00000014
+#define VLYNQ_REMOTE_OFFSET		0x00000080
+
+#define VLYNQ_STATUS_LINK		0x00000001
+#define VLYNQ_STATUS_LERROR		0x00000080
+#define VLYNQ_STATUS_RERROR		0x00000100
+
+#define VINT_ENABLE			0x00000100
+#define VINT_TYPE_EDGE			0x00000080
+#define VINT_LEVEL_LOW			0x00000040
+#define VINT_VECTOR(x)			((x) & 0x1f)
+#define VINT_OFFSET(irq)		(8 * ((irq) % 4))
+
+#define VLYNQ_AUTONEGO_V2		0x00010000
+
+struct vlynq_regs {
+	u32 revision;
+	u32 control;
+	u32 status;
+	u32 int_prio;
+	u32 int_status;
+	u32 int_pending;
+	u32 int_ptr;
+	u32 tx_offset;
+	struct vlynq_mapping rx_mapping[4];
+	u32 chip;
+	u32 autonego;
+	u32 unused[6];
+	u32 int_device[8];
+};
+
+#ifdef CONFIG_VLYNQ_DEBUG
+static void vlynq_dump_regs(struct vlynq_device *dev)
+{
+	int i;
+
+	printk(KERN_DEBUG "VLYNQ local=%p remote=%p\n",
+			dev->local, dev->remote);
+	for (i = 0; i < 32; i++) {
+		printk(KERN_DEBUG "VLYNQ: local %d: %08x\n",
+			i + 1, ((u32 *)dev->local)[i]);
+		printk(KERN_DEBUG "VLYNQ: remote %d: %08x\n",
+			i + 1, ((u32 *)dev->remote)[i]);
+	}
+}
+
+static void vlynq_dump_mem(u32 *base, int count)
+{
+	int i;
+
+	for (i = 0; i < (count + 3) / 4; i++) {
+		if (i % 4 == 0)
+			printk(KERN_DEBUG "\nMEM[0x%04x]:", i * 4);
+		printk(KERN_DEBUG " 0x%08x", *(base + i));
+	}
+	printk(KERN_DEBUG "\n");
+}
+#endif
+
+/* Check the VLYNQ link status with a given device */
+static int vlynq_linked(struct vlynq_device *dev)
+{
+	int i;
+
+	for (i = 0; i < 100; i++)
+		if (readl(&dev->local->status) & VLYNQ_STATUS_LINK)
+			return 1;
+		else
+			cpu_relax();
+
+	return 0;
+}
+
+static void vlynq_reset(struct vlynq_device *dev)
+{
+	writel(readl(&dev->local->control) | VLYNQ_CTRL_RESET,
+			&dev->local->control);
+
+	/* Wait for the devices to finish resetting */
+	msleep(5);
+
+	/* Remove reset bit */
+	writel(readl(&dev->local->control) & ~VLYNQ_CTRL_RESET,
+			&dev->local->control);
+
+	/* Give some time for the devices to settle */
+	msleep(5);
+}
+
+static void vlynq_irq_unmask(unsigned int irq)
+{
+	u32 val;
+	struct vlynq_device *dev = get_irq_chip_data(irq);
+	int virq;
+
+	BUG_ON(!dev);
+	virq = irq - dev->irq_start;
+	val = readl(&dev->remote->int_device[virq >> 2]);
+	val |= (VINT_ENABLE | virq) << VINT_OFFSET(virq);
+	writel(val, &dev->remote->int_device[virq >> 2]);
+}
+
+static void vlynq_irq_mask(unsigned int irq)
+{
+	u32 val;
+	struct vlynq_device *dev = get_irq_chip_data(irq);
+	int virq;
+
+	BUG_ON(!dev);
+	virq = irq - dev->irq_start;
+	val = readl(&dev->remote->int_device[virq >> 2]);
+	val &= ~(VINT_ENABLE << VINT_OFFSET(virq));
+	writel(val, &dev->remote->int_device[virq >> 2]);
+}
+
+static int vlynq_irq_type(unsigned int irq, unsigned int flow_type)
+{
+	u32 val;
+	struct vlynq_device *dev = get_irq_chip_data(irq);
+	int virq;
+
+	BUG_ON(!dev);
+	virq = irq - dev->irq_start;
+	val = readl(&dev->remote->int_device[virq >> 2]);
+	switch (flow_type & IRQ_TYPE_SENSE_MASK) {
+	case IRQ_TYPE_EDGE_RISING:
+	case IRQ_TYPE_EDGE_FALLING:
+	case IRQ_TYPE_EDGE_BOTH:
+		val |= VINT_TYPE_EDGE << VINT_OFFSET(virq);
+		val &= ~(VINT_LEVEL_LOW << VINT_OFFSET(virq));
+		break;
+	case IRQ_TYPE_LEVEL_HIGH:
+		val &= ~(VINT_TYPE_EDGE << VINT_OFFSET(virq));
+		val &= ~(VINT_LEVEL_LOW << VINT_OFFSET(virq));
+		break;
+	case IRQ_TYPE_LEVEL_LOW:
+		val &= ~(VINT_TYPE_EDGE << VINT_OFFSET(virq));
+		val |= VINT_LEVEL_LOW << VINT_OFFSET(virq);
+		break;
+	default:
+		return -EINVAL;
+	}
+	writel(val, &dev->remote->int_device[virq >> 2]);
+	return 0;
+}
+
+static void vlynq_local_ack(unsigned int irq)
+{
+	struct vlynq_device *dev = get_irq_chip_data(irq);
+
+	u32 status = readl(&dev->local->status);
+
+	pr_debug("%s: local status: 0x%08x\n",
+		       dev_name(&dev->dev), status);
+	writel(status, &dev->local->status);
+}
+
+static void vlynq_remote_ack(unsigned int irq)
+{
+	struct vlynq_device *dev = get_irq_chip_data(irq);
+
+	u32 status = readl(&dev->remote->status);
+
+	pr_debug("%s: remote status: 0x%08x\n",
+		       dev_name(&dev->dev), status);
+	writel(status, &dev->remote->status);
+}
+
+static irqreturn_t vlynq_irq(int irq, void *dev_id)
+{
+	struct vlynq_device *dev = dev_id;
+	u32 status;
+	int virq = 0;
+
+	status = readl(&dev->local->int_status);
+	writel(status, &dev->local->int_status);
+
+	if (unlikely(!status))
+		spurious_interrupt();
+
+	while (status) {
+		if (status & 1)
+			do_IRQ(dev->irq_start + virq);
+		status >>= 1;
+		virq++;
+	}
+
+	return IRQ_HANDLED;
+}
+
+static struct irq_chip vlynq_irq_chip = {
+	.name = "vlynq",
+	.unmask = vlynq_irq_unmask,
+	.mask = vlynq_irq_mask,
+	.set_type = vlynq_irq_type,
+};
+
+static struct irq_chip vlynq_local_chip = {
+	.name = "vlynq local error",
+	.unmask = vlynq_irq_unmask,
+	.mask = vlynq_irq_mask,
+	.ack = vlynq_local_ack,
+};
+
+static struct irq_chip vlynq_remote_chip = {
+	.name = "vlynq local error",
+	.unmask = vlynq_irq_unmask,
+	.mask = vlynq_irq_mask,
+	.ack = vlynq_remote_ack,
+};
+
+static int vlynq_setup_irq(struct vlynq_device *dev)
+{
+	u32 val;
+	int i, virq;
+
+	if (dev->local_irq == dev->remote_irq) {
+		printk(KERN_ERR
+		       "%s: local vlynq irq should be different from remote\n",
+		       dev_name(&dev->dev));
+		return -EINVAL;
+	}
+
+	/* Clear local and remote error bits */
+	writel(readl(&dev->local->status), &dev->local->status);
+	writel(readl(&dev->remote->status), &dev->remote->status);
+
+	/* Now setup interrupts */
+	val = VLYNQ_CTRL_INT_VECTOR(dev->local_irq);
+	val |= VLYNQ_CTRL_INT_ENABLE | VLYNQ_CTRL_INT_LOCAL |
+		VLYNQ_CTRL_INT2CFG;
+	val |= readl(&dev->local->control);
+	writel(VLYNQ_INT_OFFSET, &dev->local->int_ptr);
+	writel(val, &dev->local->control);
+
+	val = VLYNQ_CTRL_INT_VECTOR(dev->remote_irq);
+	val |= VLYNQ_CTRL_INT_ENABLE;
+	val |= readl(&dev->remote->control);
+	writel(VLYNQ_INT_OFFSET, &dev->remote->int_ptr);
+	writel(val, &dev->remote->int_ptr);
+	writel(val, &dev->remote->control);
+
+	for (i = dev->irq_start; i <= dev->irq_end; i++) {
+		virq = i - dev->irq_start;
+		if (virq == dev->local_irq) {
+			set_irq_chip_and_handler(i, &vlynq_local_chip,
+						 handle_level_irq);
+			set_irq_chip_data(i, dev);
+		} else if (virq == dev->remote_irq) {
+			set_irq_chip_and_handler(i, &vlynq_remote_chip,
+						 handle_level_irq);
+			set_irq_chip_data(i, dev);
+		} else {
+			set_irq_chip_and_handler(i, &vlynq_irq_chip,
+						 handle_simple_irq);
+			set_irq_chip_data(i, dev);
+			writel(0, &dev->remote->int_device[virq >> 2]);
+		}
+	}
+
+	if (request_irq(dev->irq, vlynq_irq, IRQF_SHARED, "vlynq", dev)) {
+		printk(KERN_ERR "%s: request_irq failed\n",
+					dev_name(&dev->dev));
+		return -EAGAIN;
+	}
+
+	return 0;
+}
+
+static void vlynq_device_release(struct device *dev)
+{
+	struct vlynq_device *vdev = to_vlynq_device(dev);
+	kfree(vdev);
+}
+
+static int vlynq_device_match(struct device *dev,
+			      struct device_driver *drv)
+{
+	struct vlynq_device *vdev = to_vlynq_device(dev);
+	struct vlynq_driver *vdrv = to_vlynq_driver(drv);
+	struct vlynq_device_id *ids = vdrv->id_table;
+
+	while (ids->id) {
+		if (ids->id == vdev->dev_id) {
+			vdev->divisor = ids->divisor;
+			vlynq_set_drvdata(vdev, ids);
+			printk(KERN_INFO "Driver found for VLYNQ "
+				"device: %08x\n", vdev->dev_id);
+			return 1;
+		}
+		printk(KERN_DEBUG "Not using the %08x VLYNQ device's driver"
+			" for VLYNQ device: %08x\n", ids->id, vdev->dev_id);
+		ids++;
+	}
+	return 0;
+}
+
+static int vlynq_device_probe(struct device *dev)
+{
+	struct vlynq_device *vdev = to_vlynq_device(dev);
+	struct vlynq_driver *drv = to_vlynq_driver(dev->driver);
+	struct vlynq_device_id *id = vlynq_get_drvdata(vdev);
+	int result = -ENODEV;
+
+	if (drv->probe)
+		result = drv->probe(vdev, id);
+	if (result)
+		put_device(dev);
+	return result;
+}
+
+static int vlynq_device_remove(struct device *dev)
+{
+	struct vlynq_driver *drv = to_vlynq_driver(dev->driver);
+
+	if (drv->remove)
+		drv->remove(to_vlynq_device(dev));
+
+	return 0;
+}
+
+int __vlynq_register_driver(struct vlynq_driver *driver, struct module *owner)
+{
+	driver->driver.name = driver->name;
+	driver->driver.bus = &vlynq_bus_type;
+	return driver_register(&driver->driver);
+}
+EXPORT_SYMBOL(__vlynq_register_driver);
+
+void vlynq_unregister_driver(struct vlynq_driver *driver)
+{
+	driver_unregister(&driver->driver);
+}
+EXPORT_SYMBOL(vlynq_unregister_driver);
+
+/*
+ * A VLYNQ remote device can clock the VLYNQ bus master
+ * using a dedicated clock line. In that case, both the
+ * remove device and the bus master should have the same
+ * serial clock dividers configured. Iterate through the
+ * 8 possible dividers until we actually link with the
+ * device.
+ */
+static int __vlynq_try_remote(struct vlynq_device *dev)
+{
+	int i;
+
+	vlynq_reset(dev);
+	for (i = dev->dev_id ? vlynq_rdiv2 : vlynq_rdiv8; dev->dev_id ?
+			i <= vlynq_rdiv8 : i >= vlynq_rdiv2;
+		dev->dev_id ? i++ : i--) {
+
+		if (!vlynq_linked(dev))
+			break;
+
+		writel((readl(&dev->remote->control) &
+				~VLYNQ_CTRL_CLOCK_MASK) |
+				VLYNQ_CTRL_CLOCK_INT |
+				VLYNQ_CTRL_CLOCK_DIV(i - vlynq_rdiv1),
+				&dev->remote->control);
+		writel((readl(&dev->local->control)
+				& ~(VLYNQ_CTRL_CLOCK_INT |
+				VLYNQ_CTRL_CLOCK_MASK)) |
+				VLYNQ_CTRL_CLOCK_DIV(i - vlynq_rdiv1),
+				&dev->local->control);
+
+		if (vlynq_linked(dev)) {
+			printk(KERN_DEBUG
+				"%s: using remote clock divisor %d\n",
+				dev_name(&dev->dev), i - vlynq_rdiv1 + 1);
+			dev->divisor = i;
+			return 0;
+		} else {
+			vlynq_reset(dev);
+		}
+	}
+
+	return -ENODEV;
+}
+
+/*
+ * A VLYNQ remote device can be clocked by the VLYNQ bus
+ * master using a dedicated clock line. In that case, only
+ * the bus master configures the serial clock divider.
+ * Iterate through the 8 possible dividers until we
+ * actually get a link with the device.
+ */
+static int __vlynq_try_local(struct vlynq_device *dev)
+{
+	int i;
+
+	vlynq_reset(dev);
+
+	for (i = dev->dev_id ? vlynq_ldiv2 : vlynq_ldiv8; dev->dev_id ?
+			i <= vlynq_ldiv8 : i >= vlynq_ldiv2;
+		dev->dev_id ? i++ : i--) {
+
+		writel((readl(&dev->local->control) &
+				~VLYNQ_CTRL_CLOCK_MASK) |
+				VLYNQ_CTRL_CLOCK_INT |
+				VLYNQ_CTRL_CLOCK_DIV(i - vlynq_ldiv1),
+				&dev->local->control);
+
+		if (vlynq_linked(dev)) {
+			printk(KERN_DEBUG
+				"%s: using local clock divisor %d\n",
+				dev_name(&dev->dev), i - vlynq_ldiv1 + 1);
+			dev->divisor = i;
+			return 0;
+		} else {
+			vlynq_reset(dev);
+		}
+	}
+
+	return -ENODEV;
+}
+
+/*
+ * When using external clocking method, serial clock
+ * is supplied by an external oscillator, therefore we
+ * should mask the local clock bit in the clock control
+ * register for both the bus master and the remote device.
+ */
+static int __vlynq_try_external(struct vlynq_device *dev)
+{
+	vlynq_reset(dev);
+	if (!vlynq_linked(dev))
+		return -ENODEV;
+
+	writel((readl(&dev->remote->control) &
+			~VLYNQ_CTRL_CLOCK_INT),
+			&dev->remote->control);
+
+	writel((readl(&dev->local->control) &
+			~VLYNQ_CTRL_CLOCK_INT),
+			&dev->local->control);
+
+	if (vlynq_linked(dev)) {
+		printk(KERN_DEBUG "%s: using external clock\n",
+			dev_name(&dev->dev));
+			dev->divisor = vlynq_div_external;
+		return 0;
+	}
+
+	return -ENODEV;
+}
+
+static int __vlynq_enable_device(struct vlynq_device *dev)
+{
+	int result;
+	struct plat_vlynq_ops *ops = dev->dev.platform_data;
+
+	result = ops->on(dev);
+	if (result)
+		return result;
+
+	switch (dev->divisor) {
+	case vlynq_div_external:
+	case vlynq_div_auto:
+		/* When the device is brought from reset it should have clock
+		 * generation negotiated by hardware.
+		 * Check which device is generating clocks and perform setup
+		 * accordingly */
+		if (vlynq_linked(dev) && readl(&dev->remote->control) &
+		   VLYNQ_CTRL_CLOCK_INT) {
+			if (!__vlynq_try_remote(dev) ||
+				!__vlynq_try_local(dev)  ||
+				!__vlynq_try_external(dev))
+				return 0;
+		} else {
+			if (!__vlynq_try_external(dev) ||
+				!__vlynq_try_local(dev)    ||
+				!__vlynq_try_remote(dev))
+				return 0;
+		}
+		break;
+	case vlynq_ldiv1:
+	case vlynq_ldiv2:
+	case vlynq_ldiv3:
+	case vlynq_ldiv4:
+	case vlynq_ldiv5:
+	case vlynq_ldiv6:
+	case vlynq_ldiv7:
+	case vlynq_ldiv8:
+		writel(VLYNQ_CTRL_CLOCK_INT |
+			VLYNQ_CTRL_CLOCK_DIV(dev->divisor -
+			vlynq_ldiv1), &dev->local->control);
+		writel(0, &dev->remote->control);
+		if (vlynq_linked(dev)) {
+			printk(KERN_DEBUG
+				"%s: using local clock divisor %d\n",
+				dev_name(&dev->dev),
+				dev->divisor - vlynq_ldiv1 + 1);
+			return 0;
+		}
+		break;
+	case vlynq_rdiv1:
+	case vlynq_rdiv2:
+	case vlynq_rdiv3:
+	case vlynq_rdiv4:
+	case vlynq_rdiv5:
+	case vlynq_rdiv6:
+	case vlynq_rdiv7:
+	case vlynq_rdiv8:
+		writel(0, &dev->local->control);
+		writel(VLYNQ_CTRL_CLOCK_INT |
+			VLYNQ_CTRL_CLOCK_DIV(dev->divisor -
+			vlynq_rdiv1), &dev->remote->control);
+		if (vlynq_linked(dev)) {
+			printk(KERN_DEBUG
+				"%s: using remote clock divisor %d\n",
+				dev_name(&dev->dev),
+				dev->divisor - vlynq_rdiv1 + 1);
+			return 0;
+		}
+		break;
+	}
+
+	ops->off(dev);
+	return -ENODEV;
+}
+
+int vlynq_enable_device(struct vlynq_device *dev)
+{
+	struct plat_vlynq_ops *ops = dev->dev.platform_data;
+	int result = -ENODEV;
+
+	result = __vlynq_enable_device(dev);
+	if (result)
+		return result;
+
+	result = vlynq_setup_irq(dev);
+	if (result)
+		ops->off(dev);
+
+	dev->enabled = !result;
+	return result;
+}
+EXPORT_SYMBOL(vlynq_enable_device);
+
+
+void vlynq_disable_device(struct vlynq_device *dev)
+{
+	struct plat_vlynq_ops *ops = dev->dev.platform_data;
+
+	dev->enabled = 0;
+	free_irq(dev->irq, dev);
+	ops->off(dev);
+}
+EXPORT_SYMBOL(vlynq_disable_device);
+
+int vlynq_set_local_mapping(struct vlynq_device *dev, u32 tx_offset,
+			    struct vlynq_mapping *mapping)
+{
+	int i;
+
+	if (!dev->enabled)
+		return -ENXIO;
+
+	writel(tx_offset, &dev->local->tx_offset);
+	for (i = 0; i < 4; i++) {
+		writel(mapping[i].offset, &dev->local->rx_mapping[i].offset);
+		writel(mapping[i].size, &dev->local->rx_mapping[i].size);
+	}
+	return 0;
+}
+EXPORT_SYMBOL(vlynq_set_local_mapping);
+
+int vlynq_set_remote_mapping(struct vlynq_device *dev, u32 tx_offset,
+			     struct vlynq_mapping *mapping)
+{
+	int i;
+
+	if (!dev->enabled)
+		return -ENXIO;
+
+	writel(tx_offset, &dev->remote->tx_offset);
+	for (i = 0; i < 4; i++) {
+		writel(mapping[i].offset, &dev->remote->rx_mapping[i].offset);
+		writel(mapping[i].size, &dev->remote->rx_mapping[i].size);
+	}
+	return 0;
+}
+EXPORT_SYMBOL(vlynq_set_remote_mapping);
+
+int vlynq_set_local_irq(struct vlynq_device *dev, int virq)
+{
+	int irq = dev->irq_start + virq;
+	if (dev->enabled)
+		return -EBUSY;
+
+	if ((irq < dev->irq_start) || (irq > dev->irq_end))
+		return -EINVAL;
+
+	if (virq == dev->remote_irq)
+		return -EINVAL;
+
+	dev->local_irq = virq;
+
+	return 0;
+}
+EXPORT_SYMBOL(vlynq_set_local_irq);
+
+int vlynq_set_remote_irq(struct vlynq_device *dev, int virq)
+{
+	int irq = dev->irq_start + virq;
+	if (dev->enabled)
+		return -EBUSY;
+
+	if ((irq < dev->irq_start) || (irq > dev->irq_end))
+		return -EINVAL;
+
+	if (virq == dev->local_irq)
+		return -EINVAL;
+
+	dev->remote_irq = virq;
+
+	return 0;
+}
+EXPORT_SYMBOL(vlynq_set_remote_irq);
+
+static int vlynq_probe(struct platform_device *pdev)
+{
+	struct vlynq_device *dev;
+	struct resource *regs_res, *mem_res, *irq_res;
+	int len, result;
+
+	regs_res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "regs");
+	if (!regs_res)
+		return -ENODEV;
+
+	mem_res = platform_get_resource_byname(pdev, IORESOURCE_MEM, "mem");
+	if (!mem_res)
+		return -ENODEV;
+
+	irq_res = platform_get_resource_byname(pdev, IORESOURCE_IRQ, "devirq");
+	if (!irq_res)
+		return -ENODEV;
+
+	dev = kzalloc(sizeof(*dev), GFP_KERNEL);
+	if (!dev) {
+		printk(KERN_ERR
+		       "vlynq: failed to allocate device structure\n");
+		return -ENOMEM;
+	}
+
+	dev->id = pdev->id;
+	dev->dev.bus = &vlynq_bus_type;
+	dev->dev.parent = &pdev->dev;
+	dev_set_name(&dev->dev, "vlynq%d", dev->id);
+	dev->dev.platform_data = pdev->dev.platform_data;
+	dev->dev.release = vlynq_device_release;
+
+	dev->regs_start = regs_res->start;
+	dev->regs_end = regs_res->end;
+	dev->mem_start = mem_res->start;
+	dev->mem_end = mem_res->end;
+
+	len = regs_res->end - regs_res->start;
+	if (!request_mem_region(regs_res->start, len, dev_name(&dev->dev))) {
+		printk(KERN_ERR "%s: Can't request vlynq registers\n",
+		       dev_name(&dev->dev));
+		result = -ENXIO;
+		goto fail_request;
+	}
+
+	dev->local = ioremap(regs_res->start, len);
+	if (!dev->local) {
+		printk(KERN_ERR "%s: Can't remap vlynq registers\n",
+		       dev_name(&dev->dev));
+		result = -ENXIO;
+		goto fail_remap;
+	}
+
+	dev->remote = (struct vlynq_regs *)((void *)dev->local +
+					    VLYNQ_REMOTE_OFFSET);
+
+	dev->irq = platform_get_irq_byname(pdev, "irq");
+	dev->irq_start = irq_res->start;
+	dev->irq_end = irq_res->end;
+	dev->local_irq = dev->irq_end - dev->irq_start;
+	dev->remote_irq = dev->local_irq - 1;
+
+	if (device_register(&dev->dev))
+		goto fail_register;
+	platform_set_drvdata(pdev, dev);
+
+	printk(KERN_INFO "%s: regs 0x%p, irq %d, mem 0x%p\n",
+	       dev_name(&dev->dev), (void *)dev->regs_start, dev->irq,
+	       (void *)dev->mem_start);
+
+	dev->dev_id = 0;
+	dev->divisor = vlynq_div_auto;
+	result = __vlynq_enable_device(dev);
+	if (result == 0) {
+		dev->dev_id = readl(&dev->remote->chip);
+		((struct plat_vlynq_ops *)(dev->dev.platform_data))->off(dev);
+	}
+	if (dev->dev_id)
+		printk(KERN_INFO "Found a VLYNQ device: %08x\n", dev->dev_id);
+
+	return 0;
+
+fail_register:
+	iounmap(dev->local);
+fail_remap:
+fail_request:
+	release_mem_region(regs_res->start, len);
+	kfree(dev);
+	return result;
+}
+
+static int vlynq_remove(struct platform_device *pdev)
+{
+	struct vlynq_device *dev = platform_get_drvdata(pdev);
+
+	device_unregister(&dev->dev);
+	iounmap(dev->local);
+	release_mem_region(dev->regs_start, dev->regs_end - dev->regs_start);
+
+	kfree(dev);
+
+	return 0;
+}
+
+static struct platform_driver vlynq_platform_driver = {
+	.driver.name = "vlynq",
+	.probe = vlynq_probe,
+	.remove = __devexit_p(vlynq_remove),
+};
+
+struct bus_type vlynq_bus_type = {
+	.name = "vlynq",
+	.match = vlynq_device_match,
+	.probe = vlynq_device_probe,
+	.remove = vlynq_device_remove,
+};
+EXPORT_SYMBOL(vlynq_bus_type);
+
+static int __devinit vlynq_init(void)
+{
+	int res = 0;
+
+	res = bus_register(&vlynq_bus_type);
+	if (res)
+		goto fail_bus;
+
+	res = platform_driver_register(&vlynq_platform_driver);
+	if (res)
+		goto fail_platform;
+
+	return 0;
+
+fail_platform:
+	bus_unregister(&vlynq_bus_type);
+fail_bus:
+	return res;
+}
+
+static void __devexit vlynq_exit(void)
+{
+	platform_driver_unregister(&vlynq_platform_driver);
+	bus_unregister(&vlynq_bus_type);
+}
+
+module_init(vlynq_init);
+module_exit(vlynq_exit);
diff -Nur linux-2.6.30.5.orig/drivers/watchdog/ar7_wdt.c linux-2.6.30.5/drivers/watchdog/ar7_wdt.c
--- linux-2.6.30.5.orig/drivers/watchdog/ar7_wdt.c	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/drivers/watchdog/ar7_wdt.c	2009-08-26 20:06:40.000000000 +0200
@@ -298,14 +298,28 @@
 	.fops		= &ar7_wdt_fops,
 };
 
+#define AR7_WDT_HARDWARE_ENABLE 0x10
+
 static int __init ar7_wdt_init(void)
 {
 	int rc;
+	u32 *bootcr;
+	u32 bootcr_value;
 
 	spin_lock_init(&wdt_lock);
 
 	ar7_wdt_get_regs();
 
+	/* arch/mips/ar7/clocks.c is the only other thing that reads this */
+	bootcr = (u32 *)ioremap_nocache(AR7_REGS_DCL, 4);
+	bootcr_value = *bootcr;
+	iounmap(bootcr);
+
+	if (!(bootcr_value & AR7_WDT_HARDWARE_ENABLE)) { 
+		printk(KERN_INFO DRVNAME ": watchdog disabled in hardware (bootcr=%#x)\n", bootcr_value);
+		return -ENODEV; 
+        } 
+
 	if (!request_mem_region(ar7_regs_wdt, sizeof(struct ar7_wdt),
 							LONGNAME)) {
 		printk(KERN_WARNING DRVNAME ": watchdog I/O region busy\n");
diff -Nur linux-2.6.30.5.orig/include/asm-mips/ar7/ar7.h linux-2.6.30.5/include/asm-mips/ar7/ar7.h
--- linux-2.6.30.5.orig/include/asm-mips/ar7/ar7.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/include/asm-mips/ar7/ar7.h	2009-08-26 20:05:02.000000000 +0200
@@ -0,0 +1,170 @@
+/*
+ * Copyright (C) 2006,2007 Felix Fietkau <nbd@openwrt.org>
+ * Copyright (C) 2006,2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#ifndef __AR7_H__
+#define __AR7_H__
+
+#include <linux/delay.h>
+#include <asm/addrspace.h>
+#include <linux/io.h>
+
+#define AR7_REGS_BASE	0x08610000
+
+#define AR7_REGS_MAC0	(AR7_REGS_BASE + 0x0000)
+#define AR7_REGS_GPIO	(AR7_REGS_BASE + 0x0900)
+/* 0x08610A00 - 0x08610BFF (512 bytes, 128 bytes / clock) */
+#define AR7_REGS_POWER	(AR7_REGS_BASE + 0x0a00)
+#define AR7_REGS_UART0	(AR7_REGS_BASE + 0x0e00)
+#define AR7_REGS_USB	(AR7_REGS_BASE + 0x1200)
+#define AR7_REGS_RESET	(AR7_REGS_BASE + 0x1600)
+#define AR7_REGS_VLYNQ0	(AR7_REGS_BASE + 0x1800)
+#define AR7_REGS_DCL	(AR7_REGS_BASE + 0x1a00)
+#define AR7_REGS_VLYNQ1	(AR7_REGS_BASE + 0x1c00)
+#define AR7_REGS_MDIO	(AR7_REGS_BASE + 0x1e00)
+#define AR7_REGS_IRQ	(AR7_REGS_BASE + 0x2400)
+#define AR7_REGS_MAC1	(AR7_REGS_BASE + 0x2800)
+
+#define AR7_REGS_WDT	(AR7_REGS_BASE + 0x1f00)
+#define UR8_REGS_WDT	(AR7_REGS_BASE + 0x0b00)
+#define UR8_REGS_UART1	(AR7_REGS_BASE + 0x0f00)
+
+#define AR7_RESET_PEREPHERIAL	0x0
+#define AR7_RESET_SOFTWARE	0x4
+#define AR7_RESET_STATUS	0x8
+
+#define AR7_RESET_BIT_CPMAC_LO	17
+#define AR7_RESET_BIT_CPMAC_HI	21
+#define AR7_RESET_BIT_MDIO	22
+#define AR7_RESET_BIT_EPHY	26
+
+/* GPIO control registers */
+#define AR7_GPIO_INPUT	0x0
+#define AR7_GPIO_OUTPUT	0x4
+#define AR7_GPIO_DIR	0x8
+#define AR7_GPIO_ENABLE	0xc
+
+#define AR7_CHIP_7100	0x18
+#define AR7_CHIP_7200	0x2b
+#define AR7_CHIP_7300	0x05
+
+/* Interrupts */
+#define AR7_IRQ_UART0	15
+#define AR7_IRQ_UART1	16
+
+/* Clocks */
+#define AR7_AFE_CLOCK	35328000
+#define AR7_REF_CLOCK	25000000
+#define AR7_XTAL_CLOCK	24000000
+
+struct plat_cpmac_data {
+	int reset_bit;
+	int power_bit;
+	u32 phy_mask;
+	char dev_addr[6];
+};
+
+struct plat_dsl_data {
+	int reset_bit_dsl;
+	int reset_bit_sar;
+};
+
+extern int ar7_cpu_clock, ar7_bus_clock, ar7_dsp_clock;
+
+static inline u16 ar7_chip_id(void)
+{
+	return readl((void *)KSEG1ADDR(AR7_REGS_GPIO + 0x14)) & 0xffff;
+}
+
+static inline u8 ar7_chip_rev(void)
+{
+	return (readl((void *)KSEG1ADDR(AR7_REGS_GPIO + 0x14)) >> 16) & 0xff;
+}
+
+static inline int ar7_cpu_freq(void)
+{
+	return ar7_cpu_clock;
+}
+
+static inline int ar7_bus_freq(void)
+{
+	return ar7_bus_clock;
+}
+
+static inline int ar7_vbus_freq(void)
+{
+	return ar7_bus_clock / 2;
+}
+#define ar7_cpmac_freq ar7_vbus_freq
+
+static inline int ar7_dsp_freq(void)
+{
+	return ar7_dsp_clock;
+}
+
+static inline int ar7_has_high_cpmac(void)
+{
+	u16 chip_id = ar7_chip_id();
+	switch (chip_id) {
+	case AR7_CHIP_7100:
+	case AR7_CHIP_7200:
+		return 0;
+	default:
+		return 1;
+	}
+}
+#define ar7_has_high_vlynq ar7_has_high_cpmac
+#define ar7_has_second_uart ar7_has_high_cpmac
+
+static inline void ar7_device_enable(u32 bit)
+{
+	void *reset_reg =
+		(void *)KSEG1ADDR(AR7_REGS_RESET + AR7_RESET_PEREPHERIAL);
+	writel(readl(reset_reg) | (1 << bit), reset_reg);
+	mdelay(20);
+}
+
+static inline void ar7_device_disable(u32 bit)
+{
+	void *reset_reg =
+		(void *)KSEG1ADDR(AR7_REGS_RESET + AR7_RESET_PEREPHERIAL);
+	writel(readl(reset_reg) & ~(1 << bit), reset_reg);
+	mdelay(20);
+}
+
+static inline void ar7_device_reset(u32 bit)
+{
+	ar7_device_disable(bit);
+	ar7_device_enable(bit);
+}
+
+static inline void ar7_device_on(u32 bit)
+{
+	void *power_reg = (void *)KSEG1ADDR(AR7_REGS_POWER);
+	writel(readl(power_reg) | (1 << bit), power_reg);
+	mdelay(20);
+}
+
+static inline void ar7_device_off(u32 bit)
+{
+	void *power_reg = (void *)KSEG1ADDR(AR7_REGS_POWER);
+	writel(readl(power_reg) & ~(1 << bit), power_reg);
+	mdelay(20);
+}
+
+#endif /* __AR7_H__ */
diff -Nur linux-2.6.30.5.orig/include/asm-mips/ar7/gpio.h linux-2.6.30.5/include/asm-mips/ar7/gpio.h
--- linux-2.6.30.5.orig/include/asm-mips/ar7/gpio.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/include/asm-mips/ar7/gpio.h	2009-08-26 20:05:02.000000000 +0200
@@ -0,0 +1,109 @@
+/*
+ * Copyright (C) 2007 Florian Fainelli <florian@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#ifndef __AR7_GPIO_H__
+#define __AR7_GPIO_H__
+#include <asm/ar7/ar7.h>
+
+#define AR7_GPIO_MAX 32
+
+extern int gpio_request(unsigned gpio, const char *label);
+extern void gpio_free(unsigned gpio);
+
+/* Common GPIO layer */
+static inline int gpio_get_value(unsigned gpio)
+{
+	void __iomem *gpio_in =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_INPUT);
+
+	return readl(gpio_in) & (1 << gpio);
+}
+
+static inline void gpio_set_value(unsigned gpio, int value)
+{
+	void __iomem *gpio_out =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_OUTPUT);
+	unsigned tmp;
+
+	tmp = readl(gpio_out) & ~(1 << gpio);
+	if (value)
+		tmp |= 1 << gpio;
+	writel(tmp, gpio_out);
+}
+
+static inline int gpio_direction_input(unsigned gpio)
+{
+	void __iomem *gpio_dir =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_DIR);
+
+	if (gpio >= AR7_GPIO_MAX)
+		return -EINVAL;
+
+	writel(readl(gpio_dir) | (1 << gpio), gpio_dir);
+
+	return 0;
+}
+
+static inline int gpio_direction_output(unsigned gpio, int value)
+{
+	void __iomem *gpio_dir =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_DIR);
+
+	if (gpio >= AR7_GPIO_MAX)
+		return -EINVAL;
+
+	gpio_set_value(gpio, value);
+	writel(readl(gpio_dir) & ~(1 << gpio), gpio_dir);
+
+	return 0;
+}
+
+static inline int gpio_to_irq(unsigned gpio)
+{
+	return -EINVAL;
+}
+
+static inline int irq_to_gpio(unsigned irq)
+{
+	return -EINVAL;
+}
+
+/* Board specific GPIO functions */
+static inline int ar7_gpio_enable(unsigned gpio)
+{
+	void __iomem *gpio_en =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_ENABLE);
+
+	writel(readl(gpio_en) | (1 << gpio), gpio_en);
+
+	return 0;
+}
+
+static inline int ar7_gpio_disable(unsigned gpio)
+{
+	void __iomem *gpio_en =
+		(void __iomem *)KSEG1ADDR(AR7_REGS_GPIO + AR7_GPIO_ENABLE);
+
+	writel(readl(gpio_en) & ~(1 << gpio), gpio_en);
+
+	return 0;
+}
+
+#include <asm-generic/gpio.h>
+
+#endif
diff -Nur linux-2.6.30.5.orig/include/asm-mips/ar7/irq.h linux-2.6.30.5/include/asm-mips/ar7/irq.h
--- linux-2.6.30.5.orig/include/asm-mips/ar7/irq.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/include/asm-mips/ar7/irq.h	2009-08-26 20:05:02.000000000 +0200
@@ -0,0 +1,16 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Shamelessly copied from asm-mips/mach-emma2rh/
+ * Copyright (C) 2003 by Ralf Baechle
+ */
+#ifndef __ASM_AR7_IRQ_H
+#define __ASM_AR7_IRQ_H
+
+#define NR_IRQS	256
+
+#include_next <irq.h>
+
+#endif /* __ASM_AR7_IRQ_H */
diff -Nur linux-2.6.30.5.orig/include/asm-mips/ar7/prom.h linux-2.6.30.5/include/asm-mips/ar7/prom.h
--- linux-2.6.30.5.orig/include/asm-mips/ar7/prom.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/include/asm-mips/ar7/prom.h	2009-08-26 20:05:02.000000000 +0200
@@ -0,0 +1,26 @@
+/*
+ * Copyright (C) 2006, 2007 Florian Fainelli <florian@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#ifndef __PROM_H__
+#define __PROM_H__
+
+extern char *prom_getenv(const char *name);
+extern void prom_printf(const char *fmt, ...) __attribute__((format(printf, 1, 2)));
+extern void prom_meminit(void);
+
+#endif /* __PROM_H__ */
diff -Nur linux-2.6.30.5.orig/include/asm-mips/ar7/spaces.h linux-2.6.30.5/include/asm-mips/ar7/spaces.h
--- linux-2.6.30.5.orig/include/asm-mips/ar7/spaces.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/include/asm-mips/ar7/spaces.h	2009-08-26 20:05:02.000000000 +0200
@@ -0,0 +1,32 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 1994 - 1999, 2000, 03, 04 Ralf Baechle
+ * Copyright (C) 2000, 2002  Maciej W. Rozycki
+ * Copyright (C) 1990, 1999, 2000 Silicon Graphics, Inc.
+ */
+#ifndef _ASM_AR7_SPACES_H
+#define _ASM_AR7_SPACES_H
+
+#define CAC_BASE		0x80000000
+#define IO_BASE			0xa0000000
+#define UNCAC_BASE		0xa0000000
+#define MAP_BASE		0xc0000000
+
+/*
+ * This handles the memory map.
+ * We handle pages at KSEG0 for kernels with 32 bit address space.
+ */
+#define PAGE_OFFSET		0x94000000UL
+#define PHYS_OFFSET		0x14000000UL
+
+/*
+ * Memory above this physical address will be considered highmem.
+ */
+#ifndef HIGHMEM_START
+#define HIGHMEM_START		0x40000000UL
+#endif
+
+#endif /* __ASM_AR7_SPACES_H */
diff -Nur linux-2.6.30.5.orig/include/asm-mips/ar7/war.h linux-2.6.30.5/include/asm-mips/ar7/war.h
--- linux-2.6.30.5.orig/include/asm-mips/ar7/war.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/include/asm-mips/ar7/war.h	2009-08-26 20:05:02.000000000 +0200
@@ -0,0 +1,25 @@
+/*
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ *
+ * Copyright (C) 2002, 2004, 2007 by Ralf Baechle <ralf@linux-mips.org>
+ */
+#ifndef __ASM_MIPS_MACH_BCM947XX_WAR_H
+#define __ASM_MIPS_MACH_BCM947XX_WAR_H
+
+#define R4600_V1_INDEX_ICACHEOP_WAR	0
+#define R4600_V1_HIT_CACHEOP_WAR	0
+#define R4600_V2_HIT_CACHEOP_WAR	0
+#define R5432_CP0_INTERRUPT_WAR		0
+#define BCM1250_M3_WAR			0
+#define SIBYTE_1956_WAR			0
+#define MIPS4K_ICACHE_REFILL_WAR	0
+#define MIPS_CACHE_SYNC_WAR		0
+#define TX49XX_ICACHE_INDEX_INV_WAR	0
+#define RM9000_CDEX_SMP_WAR		0
+#define ICACHE_REFILLS_WORKAROUND_WAR	0
+#define R10000_LLSC_WAR			0
+#define MIPS34K_MISSED_ITLB_WAR		0
+
+#endif /* __ASM_MIPS_MACH_BCM947XX_WAR_H */
diff -Nur linux-2.6.30.5.orig/include/linux/serial_core.h linux-2.6.30.5/include/linux/serial_core.h
--- linux-2.6.30.5.orig/include/linux/serial_core.h	2009-08-16 23:19:38.000000000 +0200
+++ linux-2.6.30.5/include/linux/serial_core.h	2009-08-26 20:06:59.000000000 +0200
@@ -41,6 +41,7 @@
 #define PORT_XSCALE	15
 #define PORT_RM9000	16	/* PMC-Sierra RM9xxx internal UART */
 #define PORT_OCTEON	17	/* Cavium OCTEON internal UART */
+#define PORT_AR7	18	/* TI AR7 internal UART */
 #define PORT_MAX_8250	17	/* max port ID */
 
 /*
diff -Nur linux-2.6.30.5.orig/include/linux/vlynq.h linux-2.6.30.5/include/linux/vlynq.h
--- linux-2.6.30.5.orig/include/linux/vlynq.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.30.5/include/linux/vlynq.h	2009-08-26 20:05:02.000000000 +0200
@@ -0,0 +1,161 @@
+/*
+ * Copyright (C) 2006, 2007 Eugene Konev <ejka@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
+ */
+
+#ifndef __VLYNQ_H__
+#define __VLYNQ_H__
+
+#include <linux/device.h>
+#include <linux/module.h>
+#include <linux/types.h>
+
+#define VLYNQ_NUM_IRQS 32
+
+struct vlynq_mapping {
+	u32 size;
+	u32 offset;
+};
+
+enum vlynq_divisor {
+	vlynq_div_auto = 0,
+	vlynq_ldiv1,
+	vlynq_ldiv2,
+	vlynq_ldiv3,
+	vlynq_ldiv4,
+	vlynq_ldiv5,
+	vlynq_ldiv6,
+	vlynq_ldiv7,
+	vlynq_ldiv8,
+	vlynq_rdiv1,
+	vlynq_rdiv2,
+	vlynq_rdiv3,
+	vlynq_rdiv4,
+	vlynq_rdiv5,
+	vlynq_rdiv6,
+	vlynq_rdiv7,
+	vlynq_rdiv8,
+	vlynq_div_external
+};
+
+struct vlynq_device_id {
+	u32 id;
+	enum vlynq_divisor divisor;
+	unsigned long driver_data;
+};
+
+struct vlynq_regs;
+struct vlynq_device {
+	u32 id, dev_id;
+	int local_irq;
+	int remote_irq;
+	enum vlynq_divisor divisor;
+	u32 regs_start, regs_end;
+	u32 mem_start, mem_end;
+	u32 irq_start, irq_end;
+	int irq;
+	int enabled;
+	struct vlynq_regs *local;
+	struct vlynq_regs *remote;
+	struct device dev;
+};
+
+struct vlynq_driver {
+	char *name;
+	struct vlynq_device_id *id_table;
+	int (*probe)(struct vlynq_device *dev, struct vlynq_device_id *id);
+	void (*remove)(struct vlynq_device *dev);
+	struct device_driver driver;
+};
+
+struct plat_vlynq_ops {
+	int (*on)(struct vlynq_device *dev);
+	void (*off)(struct vlynq_device *dev);
+};
+
+static inline struct vlynq_driver *to_vlynq_driver(struct device_driver *drv)
+{
+	return container_of(drv, struct vlynq_driver, driver);
+}
+
+static inline struct vlynq_device *to_vlynq_device(struct device *device)
+{
+	return container_of(device, struct vlynq_device, dev);
+}
+
+extern struct bus_type vlynq_bus_type;
+
+extern int __vlynq_register_driver(struct vlynq_driver *driver,
+				   struct module *owner);
+
+static inline int vlynq_register_driver(struct vlynq_driver *driver)
+{
+	return __vlynq_register_driver(driver, THIS_MODULE);
+}
+
+static inline void *vlynq_get_drvdata(struct vlynq_device *dev)
+{
+	return dev_get_drvdata(&dev->dev);
+}
+
+static inline void vlynq_set_drvdata(struct vlynq_device *dev, void *data)
+{
+	dev_set_drvdata(&dev->dev, data);
+}
+
+static inline u32 vlynq_mem_start(struct vlynq_device *dev)
+{
+	return dev->mem_start;
+}
+
+static inline u32 vlynq_mem_end(struct vlynq_device *dev)
+{
+	return dev->mem_end;
+}
+
+static inline u32 vlynq_mem_len(struct vlynq_device *dev)
+{
+	return dev->mem_end - dev->mem_start + 1;
+}
+
+static inline int vlynq_virq_to_irq(struct vlynq_device *dev, int virq)
+{
+	int irq = dev->irq_start + virq;
+	if ((irq < dev->irq_start) || (irq > dev->irq_end))
+		return -EINVAL;
+
+	return irq;
+}
+
+static inline int vlynq_irq_to_virq(struct vlynq_device *dev, int irq)
+{
+	if ((irq < dev->irq_start) || (irq > dev->irq_end))
+		return -EINVAL;
+
+	return irq - dev->irq_start;
+}
+
+extern void vlynq_unregister_driver(struct vlynq_driver *driver);
+extern int vlynq_enable_device(struct vlynq_device *dev);
+extern void vlynq_disable_device(struct vlynq_device *dev);
+extern int vlynq_set_local_mapping(struct vlynq_device *dev, u32 tx_offset,
+				   struct vlynq_mapping *mapping);
+extern int vlynq_set_remote_mapping(struct vlynq_device *dev, u32 tx_offset,
+				    struct vlynq_mapping *mapping);
+extern int vlynq_set_local_irq(struct vlynq_device *dev, int virq);
+extern int vlynq_set_remote_irq(struct vlynq_device *dev, int virq);
+
+#endif /* __VLYNQ_H__ */
