--- tcl8.5.8.orig/generic/tclStrToD.c	2009-07-16 22:50:54.000000000 +0200
+++ tcl8.5.8/generic/tclStrToD.c	2010-01-14 20:44:55.000000000 +0100
@@ -73,9 +73,11 @@ typedef unsigned int fpu_control_t __att
  * MIPS floating-point units need special settings in control registers
  * to use gradual underflow as we expect.
  */
+/*
 #if defined(__mips)
 #include <sys/fpu.h>
 #endif
+*/
 /*
  * HP's PA_RISC architecture uses 7ff4000000000000 to represent a quiet NaN.
  * Everyone else uses 7ff8000000000000. (Why, HP, why?)
@@ -2166,6 +2168,7 @@ TclInitDoubleConversion(void)
     } bitwhack;
 #endif
 
+/*
 #if defined(__mips)
     union fpc_csr mipsCR;
 
@@ -2173,6 +2176,7 @@ TclInitDoubleConversion(void)
     mipsCR.fc_struct.flush = 0;
     set_fpc_csr(mipsCR.fc_word);
 #endif
+*/
 
     /*
      * Initialize table of powers of 10 expressed as wide integers.
