menu "Miscellaneous devices support"

source target/linux/config/Config.in.leds

config ADK_KERNEL_WATCHDOG
	boolean
	default n

config ADK_KPACKAGE_KMOD_SOFT_WATCHDOG
	prompt "kmod-softdog...................... Software watchdog"
	tristate
	default n
	select ADK_KERNEL_WATCHDOG
	help
	  A software monitoring watchdog. This will fail to reboot your system
	  from some situations that the hardware watchdog will recover
	  from. Equally it's a lot cheaper to install.

config ADK_KPACKAGE_KMOD_WD1100
	prompt "kmod-wd1100....................... Soekris net4801 watchdog"
	tristate
	select ADK_KERNEL_WATCHDOG
	default n
	help
	  Driver for the NatSemi SC1x00 series Watchdog
	  found on Soekris net4801 boards

config ADK_KPACKAGE_KMOD_PARPORT
	prompt "kmod-parport...................... generic parallel port support"
	tristate
	default n
	help
	  Kernel module for generic parallel port support

config ADK_KPACKAGE_KMOD_PLIP
	prompt "kmod-plip....................... PLIP (internet over parallel port)"
	tristate
	default n
	depends on ADK_KPACKAGE_KMOD_PARPORT
	help
	  PLIP: IPv4 over parallel port, using a Turbo Laplink
	  (crossed null-printer) cable. Drivers exist for DOS
	  (from Crynwr), Linux 2.x (protocol changed and is no
	  longer compatible with Linux 1.x), FreeBSD and MirBSD.
	  This will enlarge your kernel by about 8 KiB.

config ADK_KPACKAGE_KMOD_PRINTER
	prompt "kmod-lp......................... line printer support"
	tristate
	default n
	depends on ADK_KPACKAGE_KMOD_PARPORT
	help
	  Kernel module for line printer support

config ADK_KPACKAGE_KMOD_PPDEV
	prompt "kmod-ppdev...................... userland parallel port driver"
	tristate
	default n
	depends on ADK_KPACKAGE_KMOD_PARPORT
	help
	  Kernel module for userland parallel port access

config ADK_KPACKAGE_KMOD_FW_LOADER
	prompt "kmod-fw-loader.................. userspace firmware loading support"
	tristate
	default n
	help
	  This may be necessary when using drivers which require
	  loading of external firmware files.

config ADK_KPACKAGE_KMOD_EEPROM_93CX6
	prompt "kmod-eeprom-93cx6................ 93cx6 eeprom support"
	tristate
	default n
	help

endmenu
