menu "Network devices support"
depends on !ADK_LINUX_CRIS_FOXBOARD

config ADK_KERNEL_NETDEVICES
	boolean
	default n

config ADK_KERNEL_NET_ETHERNET
	boolean
	default n

config ADK_KERNEL_MII
	boolean
	default n

config ADK_KERNEL_NET_PCI
	boolean
	default n

config ADK_KERNEL_NETDEV_1000
	boolean
	default n

menu "Ethernet card support"

config ADK_KPACKAGE_KMOD_NE2K_PCI
	prompt "kmod-net-ne2k-pci............. NE2000 PCI driver"
	select ADK_KERNEL_NETDEVICES
	select ADK_KERNEL_NET_ETHERNET
	select ADK_KERNEL_NET_PCI
	select ADK_KERNEL_MII
	tristate
	default n
	help
	  NE2000 pci driver

config ADK_KPACKAGE_KMOD_E100
	prompt "kmod-net-e100................. Intel(R) PRO/100+ driver"
	select ADK_KERNEL_NETDEVICES
	select ADK_KERNEL_NET_PCI
	select ADK_KERNEL_MII
	tristate
	default n
	help
	  Intel(R) PRO/100+ cards kernel support

config ADK_KPACKAGE_KMOD_E1000
	prompt "kmod-net-e1000................ Intel(R) PRO/1000 Gigabit Ethernet driver"
	select ADK_KERNEL_NETDEVICES
	select ADK_KERNEL_NET_ETHERNET
	select ADK_KERNEL_NETDEV_1000
	tristate
	default n
	help
	  This driver supports Intel(R) PRO/1000 gigabit ethernet family of
	  adapters.  For more information on how to identify your adapter, go 
	  to the Adapter & Driver ID Guide at:

	  <http://support.intel.com/support/network/adapter/pro100/21397.htm>

endmenu

config ADK_KERNEL_WIRELESS
	boolean
	default n

config ADK_KERNEL_WIRELESS_EXT
	boolean
	default n

config ADK_KERNEL_MAC80211_LEDS
	bool
	select ADK_KPACKAGE_KMOD_LEDS_CLASS
	select ADK_KERNEL_NEW_LEDS
	default n

config ADK_KERNEL_WLAN_80211
	boolean
	default n

config ADK_KERNEL_RT2X00
	boolean
	select ADK_KPACKAGE_KMOD_RT2X00
	select ADK_KPACKAGE_KMOD_FW_LOADER
	select ADK_KPACKAGE_KMOD_EEPROM_93CX6
	default n

config ADK_MOD_KERNEL_CFG80211
	tristate
	default n

config ADK_MOD_KERNEL_MAC80211
	tristate
	select ADK_MOD_KERNEL_CFG80211
	select ADK_KPACKAGE_KMOD_CRYPTO_AES
	select ADK_KPACKAGE_KMOD_CRYPTO_ECB
	select ADK_KPACKAGE_KMOD_CRYPTO_ARC4
	select ADK_KERNEL_CRC32
	select ADK_KERNEL_WIRELESS
	select ADK_KERNEL_WIRELESS_EXT
	select ADK_KERNEL_WLAN_80211
	select ADK_KERNEL_MAC80211_LEDS
	default n

menu "Wireless card support"

config ADK_KPACKAGE_KMOD_MAC80211
	prompt "kmod-mac80211................... mac80211 softmac"
	tristate
	select ADK_MOD_KERNEL_CFG80211
	select ADK_KPACKAGE_KMOD_CRYPTO_AES
	select ADK_KPACKAGE_KMOD_CRYPTO_ECB
	select ADK_KPACKAGE_KMOD_CRYPTO_ARC4
	select ADK_KERNEL_WIRELESS
	select ADK_KERNEL_WIRELESS_EXT
	select ADK_KERNEL_WLAN_80211
	select ADK_KERNEL_CRC32
	default n

config ADK_KPACKAGE_KMOD_ATH5K
	prompt "kmod-mac80211-ath5k............ Atheros 5xxx wireless cards"
	tristate
	select ADK_KERNEL_MAC80211_LEDS
	depends on ADK_KPACKAGE_KMOD_MAC80211
	default n
	help
	  Driver for Atheros 5xxx/24xx cards.

config ADK_KERNEL_ATH5K_DEBUG
	prompt "enable debugging info via debugfs"
	depends on ADK_KPACKAGE_KMOD_ATH5K
	default n
	select ADK_KERNEL_DEBUG_FS
	boolean
	help
   	  Atheros 5xxx debugging messages.
	  Say Y, if and you will get debug options for ath5k.
	  To use this, you need to mount debugfs:
	   mkdir /debug/
	   mount -t debugfs debug /debug/  
	  You will get access to files under:
	   /debug/ath5k/phy0/
          To enable debug, pass the debug level to the debug module
	  parameter. For example:
	   insmod ath5k.ko debug=0x00000400

config ADK_KPACKAGE_KMOD_RT2X00
	tristate
	default n

config ADK_KPACKAGE_KMOD_RT2400PCI
	prompt "kmod-mac80211-rt2400........... Ralink rt2400"
	tristate
	default n
	select ADK_KERNEL_RT2X00
	select ADK_KERNEL_MAC80211_LEDS
	depends on ADK_KPACKAGE_KMOD_MAC80211
	help
	  This adds support for rt2400 wireless chipset family.
	  Supported chips: RT2460.

config ADK_KPACKAGE_KMOD_RT2500PCI
	prompt "kmod-mac80211-rt2500........... Ralink rt2500"
	tristate
	default n
	select ADK_KERNEL_RT2X00
	select ADK_KERNEL_MAC80211_LEDS
	depends on ADK_KPACKAGE_KMOD_MAC80211
	help
	  This adds support for rt2500 wireless chipset family.
	  Supported chips: RT2560.

config ADK_KPACKAGE_KMOD_RT61PCI
	prompt "kmod-mac80211-rt2501........... Ralink rt2501/rt61"
	tristate
	default n
	select ADK_KERNEL_RT2X00
	select ADK_KERNEL_MAC80211_LEDS
	select ADK_KPACKAGE_KMOD_CRC_ITU_T
	select ADK_PACKAGE_WIRELESS_FIRMWARE_RT61
	depends on ADK_KPACKAGE_KMOD_MAC80211
	help
	  This adds support for rt2501 wireless chipset family.
	  Supported chips: RT2561, RT2561S & RT2661.

config ADK_KERNEL_RT2X00_DEBUG
	prompt "enable debugging info"
	depends on ADK_KPACKAGE_KMOD_RT61PCI || \
		ADK_KPACKAGE_KMOD_RT2500PCI || ADK_KPACKAGE_KMOD_RT2400PCI	
	default n
	boolean
	help

source package/mac80211/Config.in

endmenu
endmenu
