From 34dcc540e28cc2253fd3bdaacdd77faf1d42d759 Mon Sep 17 00:00:00 2001
From: Phil Sutter <phil@nwl.cc>
Date: Tue, 13 May 2014 00:17:06 +0200
Subject: [PATCH] spi: add various flags to spi_transfer and spi_message
 structs

---
 include/linux/spi/spi.h | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/include/linux/spi/spi.h b/include/linux/spi/spi.h
index 4203c66..4ee1a02 100644
--- a/include/linux/spi/spi.h
+++ b/include/linux/spi/spi.h
@@ -581,6 +581,8 @@ struct spi_transfer {
 	dma_addr_t	rx_dma;
 
 	unsigned	cs_change:1;
+	unsigned	verify:1;
+	unsigned	fast_write:1;
 	unsigned	tx_nbits:3;
 	unsigned	rx_nbits:3;
 #define	SPI_NBITS_SINGLE	0x01 /* 1bit transfer */
@@ -627,6 +629,7 @@ struct spi_message {
 	struct spi_device	*spi;
 
 	unsigned		is_dma_mapped:1;
+	unsigned		fast_read:1;
 
 	/* REVISIT:  we might want a flag affecting the behavior of the
 	 * last transfer ... allowing things like "read 16 bit length L"
-- 
1.8.5.3

