# This file is part of the OpenADK project. OpenADK is copyrighted
# material, please see the LICENCE file in the top-level directory.

config ADK_KERNEL_BRIDGE_NF_EBTABLES
	tristate 'Ethernet Bridge tables support'
	select ADK_KERNEL_BRIDGE_NETFILTER
	default n
	help
	  ebtables is a general, extensible frame/packet identification
	  framework. Say 'Y' or 'M' here if you want to do Ethernet
	  filtering/NAT/brouting on the Ethernet bridge.

config ADK_KERNEL_BRIDGE_EBT_BROUTE
	tristate "broute table support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  The ebtables broute table is used to define rules that decide between
	  bridging and routing frames, giving Linux the functionality of a
	  brouter. See the man page for ebtables(8) and examples on the ebtables
	  website.

	  To compile it as a module, choose M here.  If unsure, say N.

config ADK_KERNEL_BRIDGE_EBT_T_FILTER
	tristate "filter table support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  The ebtables filter table is used to define frame filtering rules at
	  local input, forwarding and local output. See the man page for
	  ebtables(8).

	  To compile it as a module, choose M here.  If unsure, say N.

config ADK_KERNEL_BRIDGE_EBT_T_NAT
	tristate "nat table support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  The ebtables nat table is used to define rules that alter the MAC
	  source address (MAC SNAT) or the MAC destination address (MAC DNAT).
	  See the man page for ebtables(8).

#
# matches
#
config ADK_KERNEL_BRIDGE_EBT_802_3
	tristate "802.3 filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds matching support for 802.3 Ethernet frames.

config ADK_KERNEL_BRIDGE_EBT_AMONG
	tristate "among filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the among match, which allows matching the MAC source
	  and/or destination address on a list of addresses. Optionally,
	  MAC/IP address pairs can be matched, f.e. for anti-spoofing rules.

config ADK_KERNEL_BRIDGE_EBT_ARP
	tristate "ARP filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the ARP match, which allows ARP and RARP header field
	  filtering.

config ADK_KERNEL_BRIDGE_EBT_IP
	tristate "IP filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the IP match, which allows basic IP header field
	  filtering.

config ADK_KERNEL_BRIDGE_EBT_IP6
	tristate "IP6 filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES && ADK_KERNEL_IPV6
	default n
	help
	  This option adds the IP6 match, which allows basic IPV6 header field
	  filtering.

config ADK_KERNEL_BRIDGE_EBT_LIMIT
	tristate "limit match support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the limit match, which allows you to control
	  the rate at which a rule can be matched. This match is the
	  equivalent of the iptables limit match.

config ADK_KERNEL_BRIDGE_EBT_MARK
	tristate "mark filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the mark match, which allows matching frames based on
	  the 'nfmark' value in the frame. This can be set by the mark target.
	  This value is the same as the one used in the iptables mark match and
	  target.

config ADK_KERNEL_BRIDGE_EBT_PKTTYPE
	tristate "packet type filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the packet type match, which allows matching on the
	  type of packet based on its Ethernet "class" (as determined by
	  the generic networking code): broadcast, multicast,
	  for this host alone or for another host.

config ADK_KERNEL_BRIDGE_EBT_STP
	tristate "STP filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the Spanning Tree Protocol match, which
	  allows STP header field filtering.

config ADK_KERNEL_BRIDGE_EBT_VLAN
	tristate "802.1Q VLAN filter support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the 802.1Q vlan match, which allows the filtering of
	  802.1Q vlan fields.

#
# targets
#
config ADK_KERNEL_BRIDGE_EBT_ARPREPLY
	tristate "arp reply target support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the arp reply target, which allows
	  automatically sending arp replies to arp requests.

config ADK_KERNEL_BRIDGE_EBT_DNAT
	tristate "dnat target support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the MAC DNAT target, which allows altering the MAC
	  destination address of frames.

config ADK_KERNEL_BRIDGE_EBT_MARK_T
	tristate "mark target support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the mark target, which allows marking frames by
	  setting the 'nfmark' value in the frame.
	  This value is the same as the one used in the iptables mark match and
	  target.

config ADK_KERNEL_BRIDGE_EBT_REDIRECT
	tristate "redirect target support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the MAC redirect target, which allows altering the MAC
	  destination address of a frame to that of the device it arrived on.

config ADK_KERNEL_BRIDGE_EBT_SNAT
	tristate "snat target support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the MAC SNAT target, which allows altering the MAC
	  source address of frames.

#
# watchers
#
config ADK_KERNEL_BRIDGE_EBT_LOG
	tristate "log support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option adds the log watcher, that you can use in any rule
	  in any ebtables table. It records info about the frame header
	  to the syslog.

config ADK_KERNEL_BRIDGE_EBT_ULOG
	tristate "ulog support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option enables the old bridge-specific "ebt_ulog" implementation
	  which has been obsoleted by the new "nfnetlink_log" code (see
	  CONFIG_NETFILTER_NETLINK_LOG).

	  This option adds the ulog watcher, that you can use in any rule
	  in any ebtables table. The packet is passed to a userspace
	  logging daemon using netlink multicast sockets. This differs
	  from the log watcher in the sense that the complete packet is
	  sent to userspace instead of a descriptive text and that
	  netlink multicast sockets are used instead of the syslog.

config ADK_KERNEL_BRIDGE_EBT_NFLOG
	tristate "nflog support"
	depends on ADK_KERNEL_BRIDGE_NF_EBTABLES
	default n
	help
	  This option enables the nflog watcher, which allows to LOG
	  messages through the netfilter logging API, which can use
	  either the old LOG target, the old ULOG target or nfnetlink_log
	  as backend.

	  This option adds the nflog watcher, that you can use in any rule
	  in any ebtables table.

