config ADK_TARGET_SYSTEM_RASPBERRY_PI2
	bool "Raspberry PI 2"
	select ADK_arm
	select ADK_raspberry_pi2
	select ADK_TARGET_LITTLE_ENDIAN
	select ADK_CPU_CORTEX_A7
	select ADK_TARGET_CPU_WITH_NEON
	select ADK_TARGET_BOARD_BCM28XX
	select ADK_TARGET_WITH_VGA
	select ADK_TARGET_WITH_SERIAL
	select ADK_TARGET_WITH_CPU_FREQ
	select ADK_TARGET_WITH_USB
	select ADK_TARGET_WITH_INPUT
	select ADK_TARGET_WITH_SD
	select ADK_TARGET_WITH_I2C
	select ADK_TARGET_WITH_SPI
	select ADK_TARGET_WITH_SMP
	select ADK_PACKAGE_BCM28XX_BOOTLOADER
	select ADK_TARGET_WITH_ROOT_RW
	select ADK_TARGET_KERNEL_ZIMAGE
	help
	  Raspberry PI 2

