--- ppp-2.4.5.orig/pppd/pppd.8	2009-11-16 23:26:07.000000000 +0100
+++ ppp-2.4.5/pppd/pppd.8	2011-01-16 15:51:05.000000000 +0100
@@ -638,9 +638,29 @@ control, as for the \fIcrtscts\fR option
 Enables the use of PPP multilink; this is an alias for the `multilink'
 option.  This option is currently only available under Linux.
 .TP
-.B mppe\-stateful
-Allow MPPE to use stateful mode.  Stateless mode is still attempted first.
-The default is to disallow stateful mode.  
+.B mppc
+Enables MPPC (Microsoft Point to Point Compression).  This is the default.
+.TP
+.B mppe \fIsubopt1[,subopt2[,subopt3[..]]]
+Modify MPPE (Microsoft Point to Point Encryption) parameters. In order
+for MPPE to successfully come up, you must have authenticated with either
+MS-CHAP or MS-CHAPv2. By default MPPE is optional, it means that pppd will
+not propose MPPE to the peer, but will negotiate MPPE if peer wants that.
+You can change this using \fIrequired\fR suboption.
+This option is presently only supported under Linux, and only if your
+kernel has been configured to include MPPE support.
+.IP
+MPPE suboptions:
+.br
+\fIrequired\fR - require MPPE; disconnect if peer doesn't support it,
+.br
+\fIstateless\fR - try to negotiate stateless mode; default is stateful,
+.br
+\fIno40\fR - disable 40 bit keys,
+.br
+\fIno56\fR - disable 56 bit keys,
+.br
+\fIno128\fR - disable 128 bit keys
 .TP
 .B mpshortseq
 Enables the use of short (12-bit) sequence numbers in multilink
@@ -778,17 +798,11 @@ peer is buggy.
 Disables the use of PPP multilink.  This option is currently only
 available under Linux.
 .TP
-.B nomppe
-Disables MPPE (Microsoft Point to Point Encryption).  This is the default.
-.TP
-.B nomppe\-40
-Disable 40-bit encryption with MPPE.
-.TP
-.B nomppe\-128
-Disable 128-bit encryption with MPPE.
+.B nomppc
+Disables MPPC (Microsoft Point to Point Compression).
 .TP
-.B nomppe\-stateful
-Disable MPPE stateful mode.  This is the default.
+.B nomppe
+Disables MPPE (Microsoft Point to Point Encryption).
 .TP
 .B nompshortseq
 Disables the use of short (12-bit) sequence numbers in the PPP
@@ -980,19 +994,6 @@ peer using PAP.
 Require the peer to authenticate itself using CHAP [Challenge
 Handshake Authentication Protocol] authentication.
 .TP
-.B require\-mppe
-Require the use of MPPE (Microsoft Point to Point Encryption).  This
-option disables all other compression types.  This option enables
-both 40-bit and 128-bit encryption.  In order for MPPE to successfully
-come up, you must have authenticated with either MS\-CHAP or MS\-CHAPv2.
-This option is presently only supported under Linux, and only if your
-kernel has been configured to include MPPE support.
-.TP
-.B require\-mppe\-40
-Require the use of MPPE, with 40-bit encryption.
-.TP
-.B require\-mppe\-128
-Require the use of MPPE, with 128-bit encryption.
 .TP
 .B require\-mschap
 Require the peer to authenticate itself using MS\-CHAP [Microsoft Challenge
