#
# For a description of the syntax of this configuration file,
# see extra/config/Kconfig-language.txt
#

config TARGET_ARCH
	string
	default "i386"

config FORCE_OPTIONS_FOR_ARCH
	bool
	default y
	select ARCH_LITTLE_ENDIAN
	select ARCH_HAS_MMU

choice
	prompt "Target x86 Processor Family"
	default CONFIG_GENERIC_386
	help
	  This is the processor type of your CPU. This information is used for
	  optimizing purposes.  To build a library that will run on all x86 CPU
	  types (albeit not optimally fast), you can specify "386" here.  If
	  you pick anything other than "386", there is no guarantee that uClibc
	  will even run on anything other than the selected processor type.

	  Here are the settings recommended for greatest speed:
	  - "Generic 386" select this if your compiler is already setup to 
	     optimize things properly.
	  - "386" for the AMD/Cyrix/Intel 386DX/DXL/SL/SLC/SX, Cyrix/TI
	     486DLC/DLC2, UMC 486SX-S and NexGen Nx586.  Only "386" kernels
	     will run on a 386 class machine.
	  - "486" for the AMD/Cyrix/IBM/Intel 486DX/DX2/DX4 or
	     SL/SLC/SLC2/SLC3/SX/SX2 and UMC U5D or U5S.
	  - "586" for Intel Pentium and other generic Pentium CPUs
	  - "Pentium-MMX" for the Intel Pentium MMX.
	  - "Pentium-Pro" for the Intel Pentium Pro/Celeron/Pentium II.
	  - "Pentium-III" for the Intel Pentium III
	     and Celerons based on the Coppermine core.
	  - "Pentium-4" for the Intel Pentium 4.
	  - "K6" for the AMD K6, K6-II and K6-III (aka K6-3D).
	  - "Athlon" for the AMD K7 family (Athlon/Duron/Thunderbird).
	  - "Elan" for the AMD Elan.
	  - "Crusoe" for the Transmeta Crusoe series.
	  - "Winchip-C6" for original IDT Winchip.
	  - "Winchip-2/Winchip-2A/Winchip-3" for IDT Winchip CPUs
	  - "CyrixIII/VIA C3" for VIA Cyrix III or VIA C3.
	  - "VIA C3-2 Nehemiah" model 9 and above.

	  If you don't know what to do, choose "386".

config CONFIG_GENERIC_386
	bool "Generic 386"

config CONFIG_386
	bool "386"

config CONFIG_486
	bool "486"

config CONFIG_586
	bool "Pentium/586/K5/5x86/6x86/6x86MX"

config CONFIG_586MMX
	bool "Pentium-MMX"

config CONFIG_686
	bool "Pentium-Pro"

config CONFIG_PENTIUMII
	bool "Celeron/Pentium-II"

config CONFIG_PENTIUMIII
	bool "Pentium-III/Celeron(Coppermine)/Pentium-III Xeon"

config CONFIG_PENTIUM4
	bool "Pentium-4/Celeron(P4-based)/Xeon"

config CONFIG_K6
	bool "K6/K6-II/K6-III"

config CONFIG_K7
	bool "Athlon/Duron/K7"

config CONFIG_ELAN
	bool "Elan"

config CONFIG_CRUSOE
	bool "Crusoe"

config CONFIG_WINCHIPC6
	bool "Winchip-C6"

config CONFIG_WINCHIP2
	bool "Winchip-2/Winchip-2A/Winchip-3"

config CONFIG_CYRIXIII
	bool "CyrixIII/VIA-C3"

config CONFIG_NEHEMIAH
	bool "VIA C3-2 (Nehemiah)"

endchoice
