config ADK_PKG_MPDBOX
	bool "Choose packages for MPDBox system"
	default n
	select ADK_PACKAGE_MPDBOX
	select ADK_PACKAGE_DROPBEAR
	select BUSYBOX_NTPD
	select ADK_PACKAGE_CIFS_UTILS
	select ADK_PACKAGE_NFS_UTILS
	select ADK_PACKAGE_NFS_UTILS_CLIENT
	select ADK_PACKAGE_NTFS_3G
	select ADK_PACKAGE_LIBMPDCLIENT
	select ADK_PACKAGE_MPC
	select ADK_PACKAGE_MPD
	select ADK_PACKAGE_MPD_WITH_ALSA
	select ADK_PACKAGE_MPD_WITH_PULSE
	select ADK_PACKAGE_MPD_WITH_MP3
	select ADK_PACKAGE_MPD_WITH_MP4
	select ADK_PACKAGE_MPD_WITH_OGG
	select ADK_PACKAGE_MPD_WITH_OPUS
	select ADK_PACKAGE_MPD_WITH_FLAC
	select ADK_PACKAGE_MPD_WITH_WAV
	select ADK_PACKAGE_MPD_WITH_MMS
	select ADK_PACKAGE_MPD_WITH_FFMPEG
	select ADK_PACKAGE_MPD_WITH_SHOUT
	select ADK_PACKAGE_MPD_WITH_CURL
	select ADK_PACKAGE_MPD_WITH_SAMPLERATE
	select ADK_PACKAGE_MPD_WITH_HTTPD
	select ADK_PACKAGE_FILE
	select ADK_PACKAGE_HTOP
	select ADK_PACKAGE_DROPBEAR
	select ADK_PACKAGE_DROPBEAR_WITH_UTMP
	select ADK_PACKAGE_FFMPEG
	select ADK_PACKAGE_FFPROBE
	select ADK_PACKAGE_LIBFFMPEG
	select ADK_PACKAGE_LIBFFMPEG_WITH_X264
	select ADK_PACKAGE_LIBFFMPEG_WITH_AAC
	select ADK_PACKAGE_LIBFFMPEG_WITH_MP3
	select ADK_PACKAGE_LIBFFMPEG_WITH_VP8
	select ADK_PACKAGE_LIBFFMPEG_WITH_THEORA
	select ADK_PACKAGE_LIBFFMPEG_WITH_XVID
	select ADK_PACKAGE_LIBFFMPEG_WITH_VORBIS
	select ADK_PACKAGE_LIGHTTPD
	select ADK_PACKAGE_LIGHTTPD_WITH_IPV6
	select ADK_PACKAGE_LIGHTTPD_WITH_SSL
	select ADK_PACKAGE_LIGHTTPD_MOD_FASTCGI
	select ADK_PACKAGE_LIGHTTPD_MOD_DIRLISTING
	select ADK_PACKAGE_LIGHTTPD_MOD_AUTH
	select ADK_PACKAGE_PHP
	select ADK_PACKAGE_PHP_MOD_SESSION
	select ADK_PACKAGE_PHP_MOD_JSON
	select ADK_PACKAGE_PHP_FASTCGI
	select ADK_PACKAGE_SCREEN
	select ADK_PACKAGE_VIM
	select ADK_PACKAGE_E2FSCK
	select ADK_PACKAGE_ALSA_UTILS
	select ADK_PACKAGE_ALSA_UTILS_WITH_ALSAMIXER
	select ADK_KPACKAGE_KMOD_SND_INTEL8X0 if ADK_TARGET_SYSTEM_QEMU_I686
	select ADK_KPACKAGE_KMOD_SND_USB_AUDIO
	select ADK_KPACKAGE_KMOD_USB_STORAGE
	select ADK_KPACKAGE_KMOD_SND_BCM2708_SOC_HIFIBERRY_DAC if ADK_TARGET_SYSTEM_RASPBERRY_PI
	help
	  Create a small mpdbox.

