config ADK_KERNEL_INPUT
	boolean
	default y if ADK_TARGET_SYSTEM_ARANYM_M68K
	default y if ADK_TARGET_SYSTEM_VBOX_I686
	default y if ADK_TARGET_SYSTEM_PCENGINES_ALIX1C
	default y if ADK_TARGET_SYSTEM_IBM_X40
	default y if ADK_TARGET_SYSTEM_LEMOTE_YEELONG
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default y if ADK_TARGET_SYSTEM_RASPBERRY_PI
	default n

config ADK_KERNEL_HID_LOGITECH
	boolean
	default n

config ADK_KERNEL_HID_LOGITECH_DJ
	boolean
	default n

config ADK_KERNEL_KEYBOARD_ATARI
	boolean
	default y if ADK_TARGET_SYSTEM_ARANYM_M68K
	default n

config ADK_KERNEL_MOUSE_ATARI
	boolean
	default y if ADK_TARGET_SYSTEM_ARANYM_M68K
	default n

config ADK_KERNEL_KEYBOARD_GPIO
	boolean
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default n

config ADK_KERNEL_KEYBOARD_MATRIX
	boolean
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default n

config ADK_KERNEL_INPUT_TOUCHSCREEN
	boolean
	default n

config ADK_KERNEL_TOUCHSCREEN_ADS7846
	boolean
	select ADK_KERNEL_INPUT_TOUCHSCREEN
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default n

config ADK_KERNEL_INPUT_EVDEV
	boolean
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default y if ADK_TARGET_SYSTEM_RASPBERRY_PI
	default n

config ADK_KERNEL_INPUT_KEYBOARD
	boolean
	default y if ADK_TARGET_SYSTEM_ARANYM_M68K
	default y if ADK_TARGET_SYSTEM_VBOX_I686
	default y if ADK_TARGET_SYSTEM_PCENGINES_ALIX1C
	default y if ADK_TARGET_SYSTEM_IBM_X40
	default y if ADK_TARGET_SYSTEM_LEMOTE_YEELONG
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default y if ADK_TARGET_SYSTEM_RASPBERRY_PI
	default n

config ADK_KERNEL_KEYBOARD_ATKBD
	boolean
	default y if ADK_TARGET_SYSTEM_VBOX_I686
	default y if ADK_TARGET_SYSTEM_PCENGINES_ALIX1C
	default y if ADK_TARGET_SYSTEM_IBM_X40
	default y if ADK_TARGET_SYSTEM_LEMOTE_YEELONG
	default n

config ADK_KERNEL_INPUT_MOUSE
	boolean
	default y if ADK_TARGET_SYSTEM_ARANYM_M68K
	default y if ADK_TARGET_SYSTEM_VBOX_I686
	default y if ADK_TARGET_SYSTEM_PCENGINES_ALIX1C
	default y if ADK_TARGET_SYSTEM_IBM_X40
	default y if ADK_TARGET_SYSTEM_LEMOTE_YEELONG
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default y if ADK_TARGET_SYSTEM_RASPBERRY_PI
	default n

config ADK_KERNEL_INPUT_MOUSEDEV
	boolean
	default y if ADK_TARGET_SYSTEM_VBOX_I686
	default y if ADK_TARGET_SYSTEM_PCENGINES_ALIX1C
	default y if ADK_TARGET_SYSTEM_IBM_X40
	default y if ADK_TARGET_SYSTEM_LEMOTE_YEELONG
	default y if ADK_TARGET_SYSTEM_SHARP_ZAURUS
	default y if ADK_TARGET_SYSTEM_RASPBERRY_PI
	default n

config ADK_KERNEL_HID_SUPPORT
	boolean
	default n

config ADK_KERNEL_HID
	boolean
	select ADK_KERNEL_HID_SUPPORT
	default n

config ADK_KERNEL_HID_GENERIC
	boolean
	select ADK_KERNEL_HID_SUPPORT
	default n
	
menu "Input devices"
depends on ADK_TARGET_WITH_USB || ADK_TARGET_WITH_INPUT || ADK_TARGET_WITH_TOUCHSCREEN

config ADK_KPACKAGE_KMOD_USB_HID
	prompt "USB keyboard/mouse support"
	tristate
	depends on !ADK_KERNEL_USB_HID
	select ADK_KERNEL_INPUT
	select ADK_KERNEL_HID
	select ADK_KERNEL_HID_GENERIC
	select ADK_KERNEL_INPUT_KEYBOARD
	select ADK_KERNEL_INPUT_MOUSEDEV
	select ADK_KERNEL_INPUT_MOUSE
	depends on ADK_PACKAGE_KMOD_USB_CONTROLLER
	depends on ADK_TARGET_WITH_USB
	default y if ADK_TARGET_SYSTEM_RASPBERRY_PI
	default n

config ADK_KERNEL_LOGITECH_DINOVO
	prompt "Support for Logitech DiNovo keyboard/mouse"
	boolean
	select ADK_KERNEL_HID_LOGITECH
	select ADK_KERNEL_HID_LOGITECH_DJ
	default n
	help
	  Support for Logitech DiNovo keyboard/mouse combination.

config ADK_KPACKAGE_KMOD_KEYBOARD_ATKBD
	prompt "Keyboard support (AT)"
	tristate
	select ADK_KERNEL_INPUT
	select ADK_KERNEL_INPUT_KEYBOARD
	depends on !ADK_KERNEL_KEYBOARD_ATKBD
	depends on !ADK_TARGET_SYSTEM_RASPBERRY_PI
	default n

config ADK_KPACKAGE_KMOD_INPUT_MOUSEDEV
	prompt "Mouse support"
	tristate
	select ADK_KERNEL_INPUT
	depends on !ADK_KERNEL_INPUT_MOUSEDEV
	default n

config ADK_KPACKAGE_KMOD_INPUT_EVDEV
	prompt "Event device support"
	tristate
	select ADK_KERNEL_INPUT
	depends on !ADK_KERNEL_INPUT_EVDEV
	default n

endmenu
