# This file is part of the OpenADK project. OpenADK is copyrighted
# material, please see the LICENCE file in the top-level directory.

choice
prompt "Optional hardware configuration"
depends on ADK_TARGET_OS_LINUX && ADK_TARGET_SYSTEM_RASPBERRY_PI3 \
	|| ADK_TARGET_SYSTEM_RASPBERRY_PI3_64

config ADK_TARGET_HARDWARE_RPI3_SERIAL
	bool "enable serial"
	select ADK_KERNEL_SERIAL_AMBA_PL011

config ADK_TARGET_HARDWARE_RPI3_BT
	bool "enable bluetooth"
	select ADK_KERNEL_BT_HCIUART_BCM m

config ADK_TARGET_HARDWARE_RPI3_NONE
	bool "disable serial and bluetooth"

endchoice

choice
prompt "Audio Board"
depends on ADK_TARGET_OS_LINUX && ADK_TARGET_BOARD_BCM28XX

config ADK_TARGET_HARDWARE_NONE
	bool "No audio addon board"

config ADK_TARGET_HARDWARE_HIFIBERRY_AMP
	bool "Hifiberry AMP"
	select ADK_KERNEL_SND_BCM2708_SOC_HIFIBERRY_AMP m

config ADK_TARGET_HARDWARE_HIFIBERRY_DAC
	bool "Hifiberry DAC"
	select ADK_KERNEL_SND_BCM2708_SOC_HIFIBERRY_DAC m

config ADK_TARGET_HARDWARE_HIFIBERRY_DACPLUS
	bool "Hifiberry DACPLUS"
	select ADK_KERNEL_SND_BCM2708_SOC_HIFIBERRY_DACPLUS m

config ADK_TARGET_HARDWARE_HIFIBERRY_DIGI
	bool "Hifiberry DIGI"
	select ADK_KERNEL_SND_BCM2708_SOC_HIFIBERRY_DIGI m

config ADK_TARGET_HARDWARE_RPI_DAC
	bool "RPI-DAC"
	select ADK_KERNEL_SND_BCM2708_SOC_RPI_DAC m

config ADK_TARGET_HARDWARE_IQAUDIO_DAC
	bool "IQAudio-DAC"
	select ADK_KERNEL_SND_BCM2708_SOC_IQAUDIO_DAC m

config ADK_TARGET_HARDWARE_RPI_PROTO
	bool "Rpi-Proto"
	select ADK_KERNEL_SND_BCM2708_SOC_RPI_PROTO m

endchoice
