#
# Local PCMCIA Configuration File
#
#----------------------------------------------------------------------
#
# System resources available for PCMCIA cards
#
# NOTE: these settings have no effect on resources assigned to a
# CardBus bridge device itself; this file only affects resources
# assigned to cards.  Also, interrupt settings here will only affect
# ISA bus interrupts assigned to 16-bit cards.  PCI interrupts
# generally can't be reconfigured.
#
# With the kernel PCMCIA subsystem, these settings also have no effect
# at all on resources used for 32-bit CardBus cards.  Those are set by
# the PCI hotplug subsystem.
#

include port 0x100-0x3af
include port 0x3e0-0x4ff
include port 0x820-0x8ff
include port 0xc00-0xcf7

include memory 0xc0000-0xfffff
include memory 0xa0000000-0xa0ffffff
include memory 0x60000000-0x60ffffff

# These may hurt on FSC.
# include port 0x3c0-0x3d2
# Exclude 0x3d3 as Radeon IGP MCE's if you touch these ports
# include port 0x3d4-0x3df

# High port numbers do not always work...
# include port 0x1000-0x17ff
