# This file is part of the OpenADK project. OpenADK is copyrighted
# material, please see the LICENCE file in the top-level directory.

choice 
prompt "Kernel configuration" if !ADK_TARGET_CHOOSE_ARCH
depends on ADK_TARGET_OS_LINUX
default ADK_TARGET_KERNEL_USE_DEFCONFIG if ADK_TARGET_SYSTEM_BEAGLEBONE_BLACK && ADK_TARGET_KERNEL_VERSION_GIT
default ADK_TARGET_KERNEL_USE_DEFCONFIG if ADK_TARGET_SYSTEM_SOLIDRUN_IMX6 && ADK_TARGET_KERNEL_VERSION_GIT
default ADK_TARGET_KERNEL_USE_DEFCONFIG if ADK_TARGET_SYSTEM_SOLIDRUN_CLEARFOG && ADK_TARGET_KERNEL_VERSION_GIT
default ADK_TARGET_KERNEL_USE_DEFCONFIG if ADK_TARGET_BOARD_BCM28XX && ADK_TARGET_KERNEL_VERSION_GIT

config ADK_TARGET_KERNEL_USE_MINICONFIG
	bool "Use mini.config from OpenADK"

config ADK_TARGET_KERNEL_USE_DEFCONFIG
	bool "Use defconfig from Linux kernel"

config ADK_TARGET_KERNEL_USE_CUSTOMCONFIG
	bool "Use custom Linux kernel configuration file"

endchoice

config ADK_TARGET_KERNEL_DEFCONFIG
	string "Defconfig name"
	depends on ADK_TARGET_KERNEL_USE_DEFCONFIG
	default "bcmrpi_defconfig" if ADK_TARGET_SYSTEM_RASPBERRY_PI
	default "bcm2709_defconfig" if ADK_TARGET_SYSTEM_RASPBERRY_PI2
	default "bcm2709_defconfig" if ADK_TARGET_SYSTEM_RASPBERRY_PI3
	default "twr-k70f120m_defconfig" if ADK_TARGET_SYSTEM_KINETIS_K70
	default "imx_v7_cbi_hb_defconfig" if ADK_TARGET_SYSTEM_SOLIDRUN_IMX6
	default "mvebu_extra_defconfig" if ADK_TARGET_SYSTEM_SOLIDRUN_CLEARFOG
	default "nsim_700_defconfig" if ADK_TARGET_SYSTEM_NSIM_ARCV1
	default "nsim_hs_defconfig" if ADK_TARGET_SYSTEM_NSIM_ARCV2
	default "10m50_defconfig" if ADK_TARGET_SYSTEM_QEMU_NIOS2
	default "orca_defconfig" if ADK_TARGET_SYSTEM_ANDES_AG101P
	default "bb.org_defconfig" if ADK_TARGET_SYSTEM_BEAGLEBONE_BLACK
	default "j2_defconfig" if ADK_TARGET_SYSTEM_NUMATO_MIMASV2
	default ""

config ADK_TARGET_KERNEL_CUSTOMCONFIG_PATH
	string "Kernel configuration file location"
	depends on ADK_TARGET_KERNEL_USE_CUSTOMCONFIG
	default ".kernelconfig"

