config ADK_TARGET_SYSTEM_IBM_X40
	bool "IBM X40 laptop"
	select ADK_x86
	select ADK_ibm_x40
	select ADK_CPU_PENTIUM_M
	select ADK_TARGET_CPU_WITH_MMX
	select ADK_TARGET_CPU_WITH_SSE
	select ADK_TARGET_CPU_WITH_SSE2
	select ADK_TARGET_CPU_WITH_MTRR
	select ADK_TARGET_WITH_VGA
	select ADK_TARGET_WITH_CPU_FREQ
	select ADK_TARGET_WITH_USB_BOOT
	select ADK_TARGET_WITH_CARDBUS
	select ADK_TARGET_WITH_USB
	select ADK_TARGET_WITH_INPUT
	select ADK_TARGET_WITH_PATA
	select ADK_TARGET_WITH_RTC
	select ADK_TARGET_WITH_MINIPCI
	select ADK_TARGET_WITH_HDD
	select ADK_TARGET_WITH_PCI
	select ADK_TARGET_WITH_ACPI
	select ADK_TARGET_WITH_WIFI
	# with docking station 
	select ADK_TARGET_WITH_PP
	select ADK_TARGET_WITH_ROOT_RW
	select ADK_TARGET_KERNEL_BZIMAGE
	select ADK_PACKAGE_GRUB
	help
         System profile for IBM X40 laptop.

